/*
WARNING: Do NOT edit the input and output ports in this file in a text
editor if you plan to continue editing the block that represents it in
the Block Editor! File corruption is VERY likely to occur.
*/

/*
Copyright (C) 1991-2009 Altera Corporation
Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and its AMPP partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, Altera MegaCore Function License 
Agreement, or other applicable license agreement, including, 
without limitation, that your use is for the sole purpose of 
programming logic devices manufactured by Altera and sold by 
Altera or its authorized distributors.  Please refer to the 
applicable agreement for further details.
*/

HEADER
{
	VERSION = 1;
	TIME_UNIT = ns;
	PRINT_OPTIONS = "Print_options_version 6\
range_start 0ps\
range_end 1.0us\
width 1\
names_percentage 25\
comments 1\
grid_lines 1\
time_bars 1\
name_every_page 0\
expand_groups 0\
print_all 1\
print_row_height 100";
	DATA_OFFSET = 0.0;
	DATA_DURATION = 1000.0;
	SIMULATION_TIME = 1000.0;
	GRID_PHASE = 0.0;
	GRID_PERIOD = 10.0;
	GRID_DUTY_CYCLE = 50;
}

SIGNAL("ADDR")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 12;
	LSB_INDEX = 0;
	DIRECTION = INPUT;
	PARENT = "";
}

SIGNAL("ADDR[11]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[10]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[9]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[8]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "ADDR";
}

SIGNAL("CLOCK")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "";
}

SIGNAL("DMA_ADDR")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 12;
	LSB_INDEX = 0;
	DIRECTION = INPUT;
	PARENT = "";
}

SIGNAL("DMA_ADDR[11]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "DMA_ADDR";
}

SIGNAL("DMA_ADDR[10]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "DMA_ADDR";
}

SIGNAL("DMA_ADDR[9]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "DMA_ADDR";
}

SIGNAL("DMA_ADDR[8]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "DMA_ADDR";
}

SIGNAL("DMA_ADDR[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "DMA_ADDR";
}

SIGNAL("DMA_ADDR[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "DMA_ADDR";
}

SIGNAL("DMA_ADDR[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "DMA_ADDR";
}

SIGNAL("DMA_ADDR[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "DMA_ADDR";
}

SIGNAL("DMA_ADDR[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "DMA_ADDR";
}

SIGNAL("DMA_ADDR[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "DMA_ADDR";
}

SIGNAL("DMA_ADDR[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "DMA_ADDR";
}

SIGNAL("DMA_ADDR[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "DMA_ADDR";
}

SIGNAL("DMA_CLOCK")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "";
}

SIGNAL("DMA_ON")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "";
}

SIGNAL("DMA_WRITE")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "";
}

SIGNAL("IN_OUT")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 8;
	LSB_INDEX = 0;
	DIRECTION = BIDIR;
	PARENT = "";
}

SIGNAL("IN_OUT[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "IN_OUT";
}

SIGNAL("IN_OUT[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "IN_OUT";
}

SIGNAL("IN_OUT[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "IN_OUT";
}

SIGNAL("IN_OUT[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "IN_OUT";
}

SIGNAL("IN_OUT[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "IN_OUT";
}

SIGNAL("IN_OUT[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "IN_OUT";
}

SIGNAL("IN_OUT[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "IN_OUT";
}

SIGNAL("IN_OUT[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "IN_OUT";
}

SIGNAL("ROM")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "";
}

SIGNAL("WRITE")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "";
}

SIGNAL("DMA_BIDIR")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 8;
	LSB_INDEX = 0;
	DIRECTION = BIDIR;
	PARENT = "";
}

SIGNAL("DMA_BIDIR[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "DMA_BIDIR";
}

SIGNAL("DMA_BIDIR[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "DMA_BIDIR";
}

SIGNAL("DMA_BIDIR[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "DMA_BIDIR";
}

SIGNAL("DMA_BIDIR[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "DMA_BIDIR";
}

SIGNAL("DMA_BIDIR[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "DMA_BIDIR";
}

SIGNAL("DMA_BIDIR[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "DMA_BIDIR";
}

SIGNAL("DMA_BIDIR[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "DMA_BIDIR";
}

SIGNAL("DMA_BIDIR[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "DMA_BIDIR";
}

SIGNAL("DMA_BIDIR[7]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("DMA_BIDIR[6]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("DMA_BIDIR[5]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("DMA_BIDIR[4]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("DMA_BIDIR[3]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("DMA_BIDIR[2]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("DMA_BIDIR[1]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("DMA_BIDIR[0]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("IN_OUT[7]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("IN_OUT[6]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("IN_OUT[5]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("IN_OUT[4]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("IN_OUT[3]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("IN_OUT[2]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("IN_OUT[1]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("IN_OUT[0]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

GROUP("DMA_BIDIR~result")
{
	MEMBERS = "DMA_BIDIR[7]~result", "DMA_BIDIR[6]~result", "DMA_BIDIR[5]~result", "DMA_BIDIR[4]~result", "DMA_BIDIR[3]~result", "DMA_BIDIR[2]~result", "DMA_BIDIR[1]~result", "DMA_BIDIR[0]~result";
}

GROUP("IN_OUT~result")
{
	MEMBERS = "IN_OUT[7]~result", "IN_OUT[6]~result", "IN_OUT[5]~result", "IN_OUT[4]~result", "IN_OUT[3]~result", "IN_OUT[2]~result", "IN_OUT[1]~result", "IN_OUT[0]~result";
}

TRANSITION_LIST("ADDR[11]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("ADDR[10]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("ADDR[9]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("ADDR[8]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("ADDR[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("ADDR[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("ADDR[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 960.0;
		LEVEL 1 FOR 40.0;
	}
}

TRANSITION_LIST("ADDR[4]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 1;
			LEVEL 0 FOR 480.0;
			LEVEL 1 FOR 480.0;
		}
		LEVEL 0 FOR 40.0;
	}
}

TRANSITION_LIST("ADDR[3]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 2;
			LEVEL 0 FOR 240.0;
			LEVEL 1 FOR 240.0;
		}
		LEVEL 0 FOR 40.0;
	}
}

TRANSITION_LIST("ADDR[2]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 4;
			LEVEL 0 FOR 120.0;
			LEVEL 1 FOR 120.0;
		}
		LEVEL 0 FOR 40.0;
	}
}

TRANSITION_LIST("ADDR[1]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 8;
			LEVEL 0 FOR 60.0;
			LEVEL 1 FOR 60.0;
		}
		LEVEL 0 FOR 40.0;
	}
}

TRANSITION_LIST("ADDR[0]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 16;
			LEVEL 0 FOR 30.0;
			LEVEL 1 FOR 30.0;
		}
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 10.0;
	}
}

TRANSITION_LIST("CLOCK")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 830.0;
	}
}

TRANSITION_LIST("DMA_ADDR[11]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DMA_ADDR[10]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DMA_ADDR[9]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DMA_ADDR[8]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DMA_ADDR[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DMA_ADDR[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DMA_ADDR[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DMA_ADDR[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DMA_ADDR[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DMA_ADDR[2]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 1;
			LEVEL 0 FOR 120.0;
			LEVEL 1 FOR 60.0;
		}
		LEVEL 0 FOR 820.0;
	}
}

TRANSITION_LIST("DMA_ADDR[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 60.0;
		LEVEL 1 FOR 60.0;
		LEVEL 0 FOR 880.0;
	}
}

TRANSITION_LIST("DMA_ADDR[0]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 1;
			LEVEL 0 FOR 30.0;
			LEVEL 1 FOR 30.0;
			NODE
			{
				REPEAT = 2;
				LEVEL 0 FOR 30.0;
				LEVEL 1 FOR 30.0;
			}
		}
		LEVEL 0 FOR 820.0;
	}
}

TRANSITION_LIST("DMA_CLOCK")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 830.0;
	}
}

TRANSITION_LIST("DMA_ON")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 90.0;
		LEVEL 1 FOR 90.0;
		LEVEL 0 FOR 820.0;
	}
}

TRANSITION_LIST("DMA_WRITE")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("IN_OUT[7]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 1;
			LEVEL Z FOR 1000.0;
		}
	}
}

TRANSITION_LIST("IN_OUT[6]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 1;
			LEVEL Z FOR 1000.0;
		}
	}
}

TRANSITION_LIST("IN_OUT[5]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 1;
			LEVEL Z FOR 1000.0;
		}
	}
}

TRANSITION_LIST("IN_OUT[4]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 1;
			LEVEL Z FOR 1000.0;
		}
	}
}

TRANSITION_LIST("IN_OUT[3]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 1;
			LEVEL Z FOR 1000.0;
		}
	}
}

TRANSITION_LIST("IN_OUT[2]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 1;
			LEVEL Z FOR 1000.0;
		}
	}
}

TRANSITION_LIST("IN_OUT[1]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 1;
			LEVEL Z FOR 1000.0;
		}
	}
}

TRANSITION_LIST("IN_OUT[0]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 1;
			LEVEL Z FOR 1000.0;
		}
	}
}

TRANSITION_LIST("ROM")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 50.0;
		LEVEL 1 FOR 950.0;
	}
}

TRANSITION_LIST("WRITE")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DMA_BIDIR[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL Z FOR 1000.0;
	}
}

TRANSITION_LIST("DMA_BIDIR[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL Z FOR 1000.0;
	}
}

TRANSITION_LIST("DMA_BIDIR[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL Z FOR 1000.0;
	}
}

TRANSITION_LIST("DMA_BIDIR[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL Z FOR 1000.0;
	}
}

TRANSITION_LIST("DMA_BIDIR[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL Z FOR 1000.0;
	}
}

TRANSITION_LIST("DMA_BIDIR[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL Z FOR 1000.0;
	}
}

TRANSITION_LIST("DMA_BIDIR[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL Z FOR 1000.0;
	}
}

TRANSITION_LIST("DMA_BIDIR[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL Z FOR 1000.0;
	}
}

TRANSITION_LIST("DMA_BIDIR[7]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 90.0;
		LEVEL Z FOR 910.0;
	}
}

TRANSITION_LIST("DMA_BIDIR[6]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 20.0;
		LEVEL Z FOR 910.0;
	}
}

TRANSITION_LIST("DMA_BIDIR[5]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 20.0;
		LEVEL Z FOR 910.0;
	}
}

TRANSITION_LIST("DMA_BIDIR[4]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 90.0;
		LEVEL Z FOR 910.0;
	}
}

TRANSITION_LIST("DMA_BIDIR[3]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 90.0;
		LEVEL Z FOR 910.0;
	}
}

TRANSITION_LIST("DMA_BIDIR[2]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 90.0;
		LEVEL Z FOR 910.0;
	}
}

TRANSITION_LIST("DMA_BIDIR[1]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 80.0;
		LEVEL Z FOR 910.0;
	}
}

TRANSITION_LIST("DMA_BIDIR[0]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 90.0;
		LEVEL Z FOR 910.0;
	}
}

TRANSITION_LIST("IN_OUT[7]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 930.0;
	}
}

TRANSITION_LIST("IN_OUT[6]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 60.0;
		LEVEL 0 FOR 870.0;
	}
}

TRANSITION_LIST("IN_OUT[5]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 60.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 840.0;
	}
}

TRANSITION_LIST("IN_OUT[4]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 10.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 30.0;
			LEVEL 0 FOR 30.0;
		}
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 840.0;
	}
}

TRANSITION_LIST("IN_OUT[3]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 10.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 30.0;
			LEVEL 0 FOR 30.0;
		}
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 840.0;
	}
}

TRANSITION_LIST("IN_OUT[2]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 10.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 30.0;
			LEVEL 0 FOR 30.0;
		}
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 840.0;
	}
}

TRANSITION_LIST("IN_OUT[1]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 90.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 840.0;
	}
}

TRANSITION_LIST("IN_OUT[0]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 60.0;
		LEVEL 1 FOR 840.0;
	}
}

DISPLAY_LINE
{
	CHANNEL = "ADDR";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 0;
	TREE_LEVEL = 0;
	CHILDREN = 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[11]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 1;
	TREE_LEVEL = 1;
	PARENT = 0;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[10]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 2;
	TREE_LEVEL = 1;
	PARENT = 0;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[9]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 3;
	TREE_LEVEL = 1;
	PARENT = 0;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[8]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 4;
	TREE_LEVEL = 1;
	PARENT = 0;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 5;
	TREE_LEVEL = 1;
	PARENT = 0;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 6;
	TREE_LEVEL = 1;
	PARENT = 0;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 7;
	TREE_LEVEL = 1;
	PARENT = 0;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 8;
	TREE_LEVEL = 1;
	PARENT = 0;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 9;
	TREE_LEVEL = 1;
	PARENT = 0;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 10;
	TREE_LEVEL = 1;
	PARENT = 0;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 11;
	TREE_LEVEL = 1;
	PARENT = 0;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 12;
	TREE_LEVEL = 1;
	PARENT = 0;
}

DISPLAY_LINE
{
	CHANNEL = "CLOCK";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 13;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "IN_OUT";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 14;
	TREE_LEVEL = 0;
	CHILDREN = 15, 16, 17, 18, 19, 20, 21, 22;
}

DISPLAY_LINE
{
	CHANNEL = "IN_OUT[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 15;
	TREE_LEVEL = 1;
	PARENT = 14;
}

DISPLAY_LINE
{
	CHANNEL = "IN_OUT[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 16;
	TREE_LEVEL = 1;
	PARENT = 14;
}

DISPLAY_LINE
{
	CHANNEL = "IN_OUT[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 17;
	TREE_LEVEL = 1;
	PARENT = 14;
}

DISPLAY_LINE
{
	CHANNEL = "IN_OUT[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 18;
	TREE_LEVEL = 1;
	PARENT = 14;
}

DISPLAY_LINE
{
	CHANNEL = "IN_OUT[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 19;
	TREE_LEVEL = 1;
	PARENT = 14;
}

DISPLAY_LINE
{
	CHANNEL = "IN_OUT[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 20;
	TREE_LEVEL = 1;
	PARENT = 14;
}

DISPLAY_LINE
{
	CHANNEL = "IN_OUT[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 21;
	TREE_LEVEL = 1;
	PARENT = 14;
}

DISPLAY_LINE
{
	CHANNEL = "IN_OUT[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 22;
	TREE_LEVEL = 1;
	PARENT = 14;
}

DISPLAY_LINE
{
	CHANNEL = "ROM";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 23;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "WRITE";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 24;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_ADDR";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 25;
	TREE_LEVEL = 0;
	CHILDREN = 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36, 37;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_ADDR[11]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 26;
	TREE_LEVEL = 1;
	PARENT = 25;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_ADDR[10]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 27;
	TREE_LEVEL = 1;
	PARENT = 25;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_ADDR[9]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 28;
	TREE_LEVEL = 1;
	PARENT = 25;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_ADDR[8]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 29;
	TREE_LEVEL = 1;
	PARENT = 25;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_ADDR[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 30;
	TREE_LEVEL = 1;
	PARENT = 25;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_ADDR[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 31;
	TREE_LEVEL = 1;
	PARENT = 25;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_ADDR[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 32;
	TREE_LEVEL = 1;
	PARENT = 25;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_ADDR[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 33;
	TREE_LEVEL = 1;
	PARENT = 25;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_ADDR[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 34;
	TREE_LEVEL = 1;
	PARENT = 25;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_ADDR[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 35;
	TREE_LEVEL = 1;
	PARENT = 25;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_ADDR[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 36;
	TREE_LEVEL = 1;
	PARENT = 25;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_ADDR[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 37;
	TREE_LEVEL = 1;
	PARENT = 25;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_ON";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 38;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_CLOCK";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 39;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_WRITE";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 40;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_BIDIR";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 41;
	TREE_LEVEL = 0;
	CHILDREN = 42, 43, 44, 45, 46, 47, 48, 49;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_BIDIR[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 42;
	TREE_LEVEL = 1;
	PARENT = 41;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_BIDIR[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 43;
	TREE_LEVEL = 1;
	PARENT = 41;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_BIDIR[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 44;
	TREE_LEVEL = 1;
	PARENT = 41;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_BIDIR[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 45;
	TREE_LEVEL = 1;
	PARENT = 41;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_BIDIR[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 46;
	TREE_LEVEL = 1;
	PARENT = 41;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_BIDIR[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 47;
	TREE_LEVEL = 1;
	PARENT = 41;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_BIDIR[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 48;
	TREE_LEVEL = 1;
	PARENT = 41;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_BIDIR[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 49;
	TREE_LEVEL = 1;
	PARENT = 41;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_BIDIR~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 50;
	TREE_LEVEL = 0;
	CHILDREN = 51, 52, 53, 54, 55, 56, 57, 58;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_BIDIR[7]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 51;
	TREE_LEVEL = 1;
	PARENT = 50;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_BIDIR[6]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 52;
	TREE_LEVEL = 1;
	PARENT = 50;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_BIDIR[5]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 53;
	TREE_LEVEL = 1;
	PARENT = 50;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_BIDIR[4]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 54;
	TREE_LEVEL = 1;
	PARENT = 50;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_BIDIR[3]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 55;
	TREE_LEVEL = 1;
	PARENT = 50;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_BIDIR[2]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 56;
	TREE_LEVEL = 1;
	PARENT = 50;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_BIDIR[1]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 57;
	TREE_LEVEL = 1;
	PARENT = 50;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_BIDIR[0]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 58;
	TREE_LEVEL = 1;
	PARENT = 50;
}

DISPLAY_LINE
{
	CHANNEL = "IN_OUT~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 59;
	TREE_LEVEL = 0;
	CHILDREN = 60, 61, 62, 63, 64, 65, 66, 67;
}

DISPLAY_LINE
{
	CHANNEL = "IN_OUT[7]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 60;
	TREE_LEVEL = 1;
	PARENT = 59;
}

DISPLAY_LINE
{
	CHANNEL = "IN_OUT[6]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 61;
	TREE_LEVEL = 1;
	PARENT = 59;
}

DISPLAY_LINE
{
	CHANNEL = "IN_OUT[5]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 62;
	TREE_LEVEL = 1;
	PARENT = 59;
}

DISPLAY_LINE
{
	CHANNEL = "IN_OUT[4]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 63;
	TREE_LEVEL = 1;
	PARENT = 59;
}

DISPLAY_LINE
{
	CHANNEL = "IN_OUT[3]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 64;
	TREE_LEVEL = 1;
	PARENT = 59;
}

DISPLAY_LINE
{
	CHANNEL = "IN_OUT[2]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 65;
	TREE_LEVEL = 1;
	PARENT = 59;
}

DISPLAY_LINE
{
	CHANNEL = "IN_OUT[1]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 66;
	TREE_LEVEL = 1;
	PARENT = 59;
}

DISPLAY_LINE
{
	CHANNEL = "IN_OUT[0]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 67;
	TREE_LEVEL = 1;
	PARENT = 59;
}

TIME_BAR
{
	TIME = 18800;
	MASTER = TRUE;
}
;
