/*
WARNING: Do NOT edit the input and output ports in this file in a text
editor if you plan to continue editing the block that represents it in
the Block Editor! File corruption is VERY likely to occur.
*/
/*
Copyright (C) 1991-2009 Altera Corporation
Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and its AMPP partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, Altera MegaCore Function License 
Agreement, or other applicable license agreement, including, 
without limitation, that your use is for the sole purpose of 
programming logic devices manufactured by Altera and sold by 
Altera or its authorized distributors.  Please refer to the 
applicable agreement for further details.
*/
(header "symbol" (version "1.1"))
(symbol
	(rect 16 16 264 208)
	(text "RAM_ROM_BIDIR" (rect 5 0 102 14)(font "Arial" (font_size 8)))
	(text "inst" (rect 8 176 25 188)(font "Arial" ))
	(port
		(pt 0 32)
		(input)
		(text "ADDR[11..0]" (rect 0 0 69 14)(font "Arial" (font_size 8)))
		(text "ADDR[11..0]" (rect 21 27 90 41)(font "Arial" (font_size 8)))
		(line (pt 0 32)(pt 16 32)(line_width 3))
	)
	(port
		(pt 0 48)
		(input)
		(text "CLOCK" (rect 0 0 41 14)(font "Arial" (font_size 8)))
		(text "CLOCK" (rect 21 43 62 57)(font "Arial" (font_size 8)))
		(line (pt 0 48)(pt 16 48)(line_width 1))
	)
	(port
		(pt 0 64)
		(input)
		(text "ROM" (rect 0 0 27 14)(font "Arial" (font_size 8)))
		(text "ROM" (rect 21 59 48 73)(font "Arial" (font_size 8)))
		(line (pt 0 64)(pt 16 64)(line_width 1))
	)
	(port
		(pt 0 80)
		(input)
		(text "WRITE" (rect 0 0 36 14)(font "Arial" (font_size 8)))
		(text "WRITE" (rect 21 75 57 89)(font "Arial" (font_size 8)))
		(line (pt 0 80)(pt 16 80)(line_width 1))
	)
	(port
		(pt 0 96)
		(input)
		(text "DMA_ON" (rect 0 0 51 14)(font "Arial" (font_size 8)))
		(text "DMA_ON" (rect 21 91 72 105)(font "Arial" (font_size 8)))
		(line (pt 0 96)(pt 16 96)(line_width 1))
	)
	(port
		(pt 0 112)
		(input)
		(text "DMA_ADDR[11..0]" (rect 0 0 103 14)(font "Arial" (font_size 8)))
		(text "DMA_ADDR[11..0]" (rect 21 107 124 121)(font "Arial" (font_size 8)))
		(line (pt 0 112)(pt 16 112)(line_width 3))
	)
	(port
		(pt 0 128)
		(input)
		(text "DMA_CLOCK" (rect 0 0 75 14)(font "Arial" (font_size 8)))
		(text "DMA_CLOCK" (rect 21 123 96 137)(font "Arial" (font_size 8)))
		(line (pt 0 128)(pt 16 128)(line_width 1))
	)
	(port
		(pt 0 144)
		(input)
		(text "DMA_WRITE" (rect 0 0 70 14)(font "Arial" (font_size 8)))
		(text "DMA_WRITE" (rect 21 139 91 153)(font "Arial" (font_size 8)))
		(line (pt 0 144)(pt 16 144)(line_width 1))
	)
	(port
		(pt 248 32)
		(bidir)
		(text "IN_OUT[7..0]" (rect 0 0 70 14)(font "Arial" (font_size 8)))
		(text "IN_OUT[7..0]" (rect 157 27 227 41)(font "Arial" (font_size 8)))
		(line (pt 248 32)(pt 232 32)(line_width 3))
	)
	(port
		(pt 248 48)
		(bidir)
		(text "DMA_BIDIR[7..0]" (rect 0 0 92 14)(font "Arial" (font_size 8)))
		(text "DMA_BIDIR[7..0]" (rect 135 43 227 57)(font "Arial" (font_size 8)))
		(line (pt 248 48)(pt 232 48)(line_width 3))
	)
	(parameter
		"ROM/RAM"
		"1/0"
		""
		(type "PARAMETER_STRING")	)
	(drawing
		(rectangle (rect 16 16 232 176)(line_width 1))
	)
	(annotation_block (parameter)(rect 264 -64 364 16))
)
