/*
WARNING: Do NOT edit the input and output ports in this file in a text
editor if you plan to continue editing the block that represents it in
the Block Editor! File corruption is VERY likely to occur.
*/

/*
Copyright (C) 1991-2009 Altera Corporation
Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and its AMPP partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, Altera MegaCore Function License 
Agreement, or other applicable license agreement, including, 
without limitation, that your use is for the sole purpose of 
programming logic devices manufactured by Altera and sold by 
Altera or its authorized distributors.  Please refer to the 
applicable agreement for further details.
*/

HEADER
{
	VERSION = 1;
	TIME_UNIT = ns;
	PRINT_OPTIONS = "Print_options_version 6\
range_start 0ps\
range_end 1.0us\
width 1\
names_percentage 25\
comments 1\
grid_lines 1\
time_bars 1\
name_every_page 0\
expand_groups 0\
print_all 1\
print_row_height 100";
	DATA_OFFSET = 0.0;
	DATA_DURATION = 1000.0;
	SIMULATION_TIME = 1000.0;
	GRID_PHASE = 0.0;
	GRID_PERIOD = 10.0;
	GRID_DUTY_CYCLE = 50;
}

SIGNAL("AR")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 8;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("AR[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "AR";
}

SIGNAL("AR[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "AR";
}

SIGNAL("AR[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "AR";
}

SIGNAL("AR[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "AR";
}

SIGNAL("AR[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "AR";
}

SIGNAL("AR[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "AR";
}

SIGNAL("AR[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "AR";
}

SIGNAL("AR[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "AR";
}

SIGNAL("AX")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 8;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("AX[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "AX";
}

SIGNAL("AX[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "AX";
}

SIGNAL("AX[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "AX";
}

SIGNAL("AX[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "AX";
}

SIGNAL("AX[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "AX";
}

SIGNAL("AX[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "AX";
}

SIGNAL("AX[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "AX";
}

SIGNAL("AX[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "AX";
}

SIGNAL("BX")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 8;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("BX[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "BX";
}

SIGNAL("BX[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "BX";
}

SIGNAL("BX[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "BX";
}

SIGNAL("BX[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "BX";
}

SIGNAL("BX[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "BX";
}

SIGNAL("BX[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "BX";
}

SIGNAL("BX[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "BX";
}

SIGNAL("BX[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "BX";
}

SIGNAL("CLOCK")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "";
}

SIGNAL("CX")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 8;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("CX[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CX";
}

SIGNAL("CX[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CX";
}

SIGNAL("CX[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CX";
}

SIGNAL("CX[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CX";
}

SIGNAL("CX[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CX";
}

SIGNAL("CX[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CX";
}

SIGNAL("CX[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CX";
}

SIGNAL("CX[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CX";
}

SIGNAL("DR")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 8;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("DR[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DR";
}

SIGNAL("DR[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DR";
}

SIGNAL("DR[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DR";
}

SIGNAL("DR[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DR";
}

SIGNAL("DR[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DR";
}

SIGNAL("DR[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DR";
}

SIGNAL("DR[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DR";
}

SIGNAL("DR[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DR";
}

SIGNAL("DX")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 8;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("DX[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DX";
}

SIGNAL("DX[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DX";
}

SIGNAL("DX[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DX";
}

SIGNAL("DX[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DX";
}

SIGNAL("DX[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DX";
}

SIGNAL("DX[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DX";
}

SIGNAL("DX[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DX";
}

SIGNAL("DX[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DX";
}

SIGNAL("IP")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 12;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("IP[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IP";
}

SIGNAL("IP[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IP";
}

SIGNAL("IP[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IP";
}

SIGNAL("IP[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IP";
}

SIGNAL("IP[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IP";
}

SIGNAL("IP[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IP";
}

SIGNAL("IP[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IP";
}

SIGNAL("IP[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IP";
}

SIGNAL("IR")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 4;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("IR[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IR";
}

SIGNAL("IR[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IR";
}

SIGNAL("IR[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IR";
}

SIGNAL("IR[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IR";
}

SIGNAL("ADDR")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 12;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("ADDR[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR";
}

SIGNAL("CACHE-RAM_DATA_BUS")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 8;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("CACHE-RAM_DATA_BUS[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE-RAM_DATA_BUS";
}

SIGNAL("CACHE-RAM_DATA_BUS[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE-RAM_DATA_BUS";
}

SIGNAL("CACHE-RAM_DATA_BUS[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE-RAM_DATA_BUS";
}

SIGNAL("CACHE-RAM_DATA_BUS[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE-RAM_DATA_BUS";
}

SIGNAL("CACHE-RAM_DATA_BUS[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE-RAM_DATA_BUS";
}

SIGNAL("CACHE-RAM_DATA_BUS[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE-RAM_DATA_BUS";
}

SIGNAL("CACHE-RAM_DATA_BUS[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE-RAM_DATA_BUS";
}

SIGNAL("CACHE-RAM_DATA_BUS[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE-RAM_DATA_BUS";
}

SIGNAL("DATA")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 8;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("DATA[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DATA";
}

SIGNAL("DATA[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DATA";
}

SIGNAL("DATA[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DATA";
}

SIGNAL("DATA[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DATA";
}

SIGNAL("DATA[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DATA";
}

SIGNAL("DATA[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DATA";
}

SIGNAL("DATA[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DATA";
}

SIGNAL("DATA[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DATA";
}

SIGNAL("DELAY_ITERATION")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("FLAGS")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 4;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("FLAGS[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "FLAGS";
}

SIGNAL("FLAGS[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "FLAGS";
}

SIGNAL("FLAGS[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "FLAGS";
}

SIGNAL("FLAGS[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "FLAGS";
}

SIGNAL("IP[8]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IP";
}

SIGNAL("IP[9]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IP";
}

SIGNAL("IP[10]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IP";
}

SIGNAL("IP[11]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IP";
}

SIGNAL("ADDR[8]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[9]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[10]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR";
}

SIGNAL("ADDR[11]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR";
}

SIGNAL("ACLR_COUNTER")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("ACLR_COUNTER_OUT")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("ADDR_CACHE")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 12;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("ADDR_CACHE[11]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR_CACHE";
}

SIGNAL("ADDR_CACHE[10]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR_CACHE";
}

SIGNAL("ADDR_CACHE[9]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR_CACHE";
}

SIGNAL("ADDR_CACHE[8]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR_CACHE";
}

SIGNAL("ADDR_CACHE[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR_CACHE";
}

SIGNAL("ADDR_CACHE[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR_CACHE";
}

SIGNAL("ADDR_CACHE[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR_CACHE";
}

SIGNAL("ADDR_CACHE[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR_CACHE";
}

SIGNAL("ADDR_CACHE[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR_CACHE";
}

SIGNAL("ADDR_CACHE[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR_CACHE";
}

SIGNAL("ADDR_CACHE[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR_CACHE";
}

SIGNAL("ADDR_CACHE[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR_CACHE";
}

SIGNAL("ADDR_MEM_OUT")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 8;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("ADDR_MEM_OUT[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR_MEM_OUT";
}

SIGNAL("ADDR_MEM_OUT[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR_MEM_OUT";
}

SIGNAL("ADDR_MEM_OUT[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR_MEM_OUT";
}

SIGNAL("ADDR_MEM_OUT[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR_MEM_OUT";
}

SIGNAL("ADDR_MEM_OUT[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR_MEM_OUT";
}

SIGNAL("ADDR_MEM_OUT[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR_MEM_OUT";
}

SIGNAL("ADDR_MEM_OUT[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR_MEM_OUT";
}

SIGNAL("ADDR_MEM_OUT[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "ADDR_MEM_OUT";
}

SIGNAL("CACHE_DATA_OUT")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 8;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("CACHE_DATA_OUT[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE_DATA_OUT";
}

SIGNAL("CACHE_DATA_OUT[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE_DATA_OUT";
}

SIGNAL("CACHE_DATA_OUT[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE_DATA_OUT";
}

SIGNAL("CACHE_DATA_OUT[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE_DATA_OUT";
}

SIGNAL("CACHE_DATA_OUT[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE_DATA_OUT";
}

SIGNAL("CACHE_DATA_OUT[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE_DATA_OUT";
}

SIGNAL("CACHE_DATA_OUT[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE_DATA_OUT";
}

SIGNAL("CACHE_DATA_OUT[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE_DATA_OUT";
}

SIGNAL("CACHE_MISS_OUT")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("CACHE_TAG_OUT")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 7;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("CACHE_TAG_OUT[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE_TAG_OUT";
}

SIGNAL("CACHE_TAG_OUT[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE_TAG_OUT";
}

SIGNAL("CACHE_TAG_OUT[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE_TAG_OUT";
}

SIGNAL("CACHE_TAG_OUT[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE_TAG_OUT";
}

SIGNAL("CACHE_TAG_OUT[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE_TAG_OUT";
}

SIGNAL("CACHE_TAG_OUT[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE_TAG_OUT";
}

SIGNAL("CACHE_TAG_OUT[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "CACHE_TAG_OUT";
}

SIGNAL("CLOCK_CACHE")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("CLOCK_COUNT_DEC")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("CLOCK_FIX")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("CLOCK_FLAG")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("CLOCK_MEM_OUT")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("COUNTER")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 8;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("COUNTER[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "COUNTER";
}

SIGNAL("COUNTER[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "COUNTER";
}

SIGNAL("COUNTER[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "COUNTER";
}

SIGNAL("COUNTER[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "COUNTER";
}

SIGNAL("COUNTER[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "COUNTER";
}

SIGNAL("COUNTER[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "COUNTER";
}

SIGNAL("COUNTER[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "COUNTER";
}

SIGNAL("COUNTER[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "COUNTER";
}

SIGNAL("COUNTER_CLOCK")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("COUNTER_DECODE")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 4;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("COUNTER_DECODE[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "COUNTER_DECODE";
}

SIGNAL("COUNTER_DECODE[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "COUNTER_DECODE";
}

SIGNAL("COUNTER_DECODE[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "COUNTER_DECODE";
}

SIGNAL("COUNTER_DECODE[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "COUNTER_DECODE";
}

SIGNAL("DATA_REG_GLOB_OUT")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 8;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("DATA_REG_GLOB_OUT[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DATA_REG_GLOB_OUT";
}

SIGNAL("DATA_REG_GLOB_OUT[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DATA_REG_GLOB_OUT";
}

SIGNAL("DATA_REG_GLOB_OUT[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DATA_REG_GLOB_OUT";
}

SIGNAL("DATA_REG_GLOB_OUT[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DATA_REG_GLOB_OUT";
}

SIGNAL("DATA_REG_GLOB_OUT[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DATA_REG_GLOB_OUT";
}

SIGNAL("DATA_REG_GLOB_OUT[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DATA_REG_GLOB_OUT";
}

SIGNAL("DATA_REG_GLOB_OUT[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DATA_REG_GLOB_OUT";
}

SIGNAL("DATA_REG_GLOB_OUT[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "DATA_REG_GLOB_OUT";
}

SIGNAL("EN_OUT_MEM")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("EN_OUT_REG")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("FIX_FLAG")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("IN_CACHE")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 8;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("IN_CACHE[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IN_CACHE";
}

SIGNAL("IN_CACHE[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IN_CACHE";
}

SIGNAL("IN_CACHE[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IN_CACHE";
}

SIGNAL("IN_CACHE[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IN_CACHE";
}

SIGNAL("IN_CACHE[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IN_CACHE";
}

SIGNAL("IN_CACHE[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IN_CACHE";
}

SIGNAL("IN_CACHE[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IN_CACHE";
}

SIGNAL("IN_CACHE[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "IN_CACHE";
}

SIGNAL("IP_UP_SPEC_OUT")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("MISS_FIX")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("qq")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 2;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("qq[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "qq";
}

SIGNAL("qq[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "qq";
}

SIGNAL("ROM_MEM_OUT")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("SELECT_REG_GLOB_OUT")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 5;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("SELECT_REG_GLOB_OUT[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "SELECT_REG_GLOB_OUT";
}

SIGNAL("SELECT_REG_GLOB_OUT[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "SELECT_REG_GLOB_OUT";
}

SIGNAL("SELECT_REG_GLOB_OUT[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "SELECT_REG_GLOB_OUT";
}

SIGNAL("SELECT_REG_GLOB_OUT[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "SELECT_REG_GLOB_OUT";
}

SIGNAL("SELECT_REG_GLOB_OUT[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "SELECT_REG_GLOB_OUT";
}

SIGNAL("STOP_OUT")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("T0")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 7;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("T0[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T0";
}

SIGNAL("T0[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T0";
}

SIGNAL("T0[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T0";
}

SIGNAL("T0[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T0";
}

SIGNAL("T0[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T0";
}

SIGNAL("T0[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T0";
}

SIGNAL("T0[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T0";
}

SIGNAL("T3")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 7;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("T3[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T3";
}

SIGNAL("T3[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T3";
}

SIGNAL("T3[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T3";
}

SIGNAL("T3[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T3";
}

SIGNAL("T3[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T3";
}

SIGNAL("T3[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T3";
}

SIGNAL("T3[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T3";
}

SIGNAL("TAG_FIX")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 7;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("TAG_FIX[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "TAG_FIX";
}

SIGNAL("TAG_FIX[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "TAG_FIX";
}

SIGNAL("TAG_FIX[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "TAG_FIX";
}

SIGNAL("TAG_FIX[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "TAG_FIX";
}

SIGNAL("TAG_FIX[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "TAG_FIX";
}

SIGNAL("TAG_FIX[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "TAG_FIX";
}

SIGNAL("TAG_FIX[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "TAG_FIX";
}

SIGNAL("WRITE_CACHE")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("WRITE_ON_GLOB_OUT")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("WRITE_ON_MEM_OUT")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("T1")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 7;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("T1[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T1";
}

SIGNAL("T1[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T1";
}

SIGNAL("T1[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T1";
}

SIGNAL("T1[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T1";
}

SIGNAL("T1[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T1";
}

SIGNAL("T1[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T1";
}

SIGNAL("T1[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T1";
}

SIGNAL("T2")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 7;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("T2[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T2";
}

SIGNAL("T2[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T2";
}

SIGNAL("T2[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T2";
}

SIGNAL("T2[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T2";
}

SIGNAL("T2[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T2";
}

SIGNAL("T2[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T2";
}

SIGNAL("T2[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "T2";
}

SIGNAL("WAY")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("C")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 4;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("C[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "C";
}

SIGNAL("C[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "C";
}

SIGNAL("C[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "C";
}

SIGNAL("C_ALCR")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("C_CLOCK")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("C[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "C";
}

SIGNAL("DMA_ADDR")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 3;
	LSB_INDEX = 0;
	DIRECTION = INPUT;
	PARENT = "";
}

SIGNAL("DMA_ADDR[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "DMA_ADDR";
}

SIGNAL("DMA_ADDR[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "DMA_ADDR";
}

SIGNAL("DMA_ADDR[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "DMA_ADDR";
}

SIGNAL("DMA_CLOCK")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "";
}

SIGNAL("DMA_DATA_BIDIR")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 8;
	LSB_INDEX = 0;
	DIRECTION = BIDIR;
	PARENT = "";
}

SIGNAL("DMA_DATA_BIDIR[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "DMA_DATA_BIDIR";
}

SIGNAL("DMA_DATA_BIDIR[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "DMA_DATA_BIDIR";
}

SIGNAL("DMA_DATA_BIDIR[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "DMA_DATA_BIDIR";
}

SIGNAL("DMA_DATA_BIDIR[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "DMA_DATA_BIDIR";
}

SIGNAL("DMA_DATA_BIDIR[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "DMA_DATA_BIDIR";
}

SIGNAL("DMA_DATA_BIDIR[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "DMA_DATA_BIDIR";
}

SIGNAL("DMA_DATA_BIDIR[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "DMA_DATA_BIDIR";
}

SIGNAL("DMA_DATA_BIDIR[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = BIDIR;
	PARENT = "DMA_DATA_BIDIR";
}

SIGNAL("DMA_WRITE")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "";
}

SIGNAL("DMA_DATA_BIDIR[7]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("DMA_DATA_BIDIR[6]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("DMA_DATA_BIDIR[5]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("DMA_DATA_BIDIR[4]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("DMA_DATA_BIDIR[3]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("DMA_DATA_BIDIR[2]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("DMA_DATA_BIDIR[1]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("DMA_DATA_BIDIR[0]~result")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "";
}

GROUP("DMA_DATA_BIDIR~result")
{
	MEMBERS = "DMA_DATA_BIDIR[7]~result", "DMA_DATA_BIDIR[6]~result", "DMA_DATA_BIDIR[5]~result", "DMA_DATA_BIDIR[4]~result", "DMA_DATA_BIDIR[3]~result", "DMA_DATA_BIDIR[2]~result", "DMA_DATA_BIDIR[1]~result", "DMA_DATA_BIDIR[0]~result";
}

TRANSITION_LIST("AR[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 172.5;
		LEVEL 1 FOR 100.0;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 110.0;
		LEVEL 0 FOR 572.5;
	}
}

TRANSITION_LIST("AR[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 112.5;
		LEVEL 1 FOR 160.0;
		LEVEL 0 FOR 155.0;
		LEVEL 1 FOR 572.5;
	}
}

TRANSITION_LIST("AR[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 52.5;
		LEVEL 1 FOR 60.0;
		LEVEL 0 FOR 60.0;
		LEVEL 1 FOR 827.5;
	}
}

TRANSITION_LIST("AR[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("AR[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("AR[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("AR[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 52.5;
		LEVEL 1 FOR 60.0;
		LEVEL 0 FOR 160.0;
		LEVEL 1 FOR 45.0;
		LEVEL 0 FOR 682.5;
	}
}

TRANSITION_LIST("AR[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 52.5;
		LEVEL 1 FOR 120.0;
		LEVEL 0 FOR 55.0;
		LEVEL 1 FOR 45.0;
		LEVEL 0 FOR 110.0;
		LEVEL 1 FOR 617.5;
	}
}

TRANSITION_LIST("AX[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("AX[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 92.5;
		LEVEL 1 FOR 907.5;
	}
}

TRANSITION_LIST("AX[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("AX[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 92.5;
		LEVEL 1 FOR 907.5;
	}
}

TRANSITION_LIST("AX[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 92.5;
		LEVEL 1 FOR 907.5;
	}
}

TRANSITION_LIST("AX[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 92.5;
		LEVEL 1 FOR 907.5;
	}
}

TRANSITION_LIST("AX[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("AX[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 92.5;
		LEVEL 1 FOR 907.5;
	}
}

TRANSITION_LIST("BX[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("BX[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("BX[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 152.5;
		LEVEL 1 FOR 847.5;
	}
}

TRANSITION_LIST("BX[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 152.5;
		LEVEL 1 FOR 847.5;
	}
}

TRANSITION_LIST("BX[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 152.5;
		LEVEL 1 FOR 847.5;
	}
}

TRANSITION_LIST("BX[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("BX[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 152.5;
		LEVEL 1 FOR 847.5;
	}
}

TRANSITION_LIST("BX[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("CLOCK")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 200;
			LEVEL 0 FOR 2.5;
			LEVEL 1 FOR 2.5;
		}
	}
}

TRANSITION_LIST("CX[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 297.5;
		LEVEL 1 FOR 702.5;
	}
}

TRANSITION_LIST("CX[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 297.5;
		LEVEL 1 FOR 702.5;
	}
}

TRANSITION_LIST("CX[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 297.5;
		LEVEL 1 FOR 702.5;
	}
}

TRANSITION_LIST("CX[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("CX[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("CX[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 297.5;
		LEVEL 1 FOR 702.5;
	}
}

TRANSITION_LIST("CX[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 297.5;
		LEVEL 1 FOR 702.5;
	}
}

TRANSITION_LIST("CX[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 297.5;
		LEVEL 1 FOR 702.5;
	}
}

TRANSITION_LIST("DR[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DR[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DR[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DR[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DR[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DR[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DR[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 282.5;
		LEVEL 1 FOR 110.0;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 562.5;
	}
}

TRANSITION_LIST("DR[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 122.5;
		LEVEL 1 FOR 60.0;
		LEVEL 0 FOR 55.0;
		LEVEL 1 FOR 45.0;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 65.0;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 562.5;
	}
}

TRANSITION_LIST("DX[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DX[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 482.5;
		LEVEL 1 FOR 517.5;
	}
}

TRANSITION_LIST("DX[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 482.5;
		LEVEL 1 FOR 517.5;
	}
}

TRANSITION_LIST("DX[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DX[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 482.5;
		LEVEL 1 FOR 517.5;
	}
}

TRANSITION_LIST("DX[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DX[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DX[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 482.5;
		LEVEL 1 FOR 517.5;
	}
}

TRANSITION_LIST("IP[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 32.5;
		LEVEL 1 FOR 967.5;
	}
}

TRANSITION_LIST("IP[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 427.5;
		LEVEL 1 FOR 572.5;
	}
}

TRANSITION_LIST("IP[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 32.5;
		LEVEL 1 FOR 395.0;
		LEVEL 0 FOR 215.0;
		LEVEL 1 FOR 357.5;
	}
}

TRANSITION_LIST("IP[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 227.5;
		LEVEL 1 FOR 200.0;
		LEVEL 0 FOR 135.0;
		LEVEL 1 FOR 80.0;
		LEVEL 0 FOR 80.0;
		LEVEL 1 FOR 277.5;
	}
}

TRANSITION_LIST("IP[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 112.5;
		LEVEL 1 FOR 115.0;
		LEVEL 0 FOR 90.0;
		LEVEL 1 FOR 110.0;
		LEVEL 0 FOR 95.0;
		NODE
		{
			REPEAT = 3;
			LEVEL 1 FOR 40.0;
			LEVEL 0 FOR 40.0;
		}
		LEVEL 1 FOR 237.5;
	}
}

TRANSITION_LIST("IP[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 60.0;
		LEVEL 0 FOR 60.0;
		LEVEL 1 FOR 55.0;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 45.0;
		LEVEL 0 FOR 65.0;
		LEVEL 1 FOR 45.0;
		LEVEL 0 FOR 75.0;
		NODE
		{
			REPEAT = 7;
			LEVEL 1 FOR 20.0;
			LEVEL 0 FOR 20.0;
		}
		LEVEL 1 FOR 217.5;
	}
}

TRANSITION_LIST("IP[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 10.0;
			LEVEL 0 FOR 50.0;
		}
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 45.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 10.0;
			LEVEL 0 FOR 35.0;
		}
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 55.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 65.0;
		NODE
		{
			REPEAT = 15;
			LEVEL 1 FOR 10.0;
			LEVEL 0 FOR 10.0;
		}
		LEVEL 1 FOR 207.5;
	}
}

TRANSITION_LIST("IP[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 10.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 10.0;
			LEVEL 0 FOR 5.0;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 40.0;
		}
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 35.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 10.0;
			LEVEL 0 FOR 5.0;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 25.0;
		}
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 55.0;
		LEVEL 1 FOR 10.0;
		NODE
		{
			REPEAT = 30;
			LEVEL 0 FOR 5.0;
			LEVEL 1 FOR 5.0;
		}
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 202.5;
	}
}

TRANSITION_LIST("IR[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 150.0;
		LEVEL 0 FOR 50.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 50.0;
		LEVEL 0 FOR 60.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 80.0;
		LEVEL 0 FOR 502.5;
	}
}

TRANSITION_LIST("IR[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 480.0;
		LEVEL 0 FOR 502.5;
	}
}

TRANSITION_LIST("IR[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 30.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 0 FOR 55.0;
			LEVEL 1 FOR 5.0;
		}
		LEVEL 0 FOR 50.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 40.0;
		}
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 60.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 70.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 502.5;
	}
}

TRANSITION_LIST("IR[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 20.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 55.0;
		}
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 50.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 40.0;
		}
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 60.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 70.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 502.5;
	}
}

TRANSITION_LIST("ADDR[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 32.5;
		LEVEL 1 FOR 32.5;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 130.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 140.0;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 515.0;
	}
}

TRANSITION_LIST("ADDR[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 125.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 172.5;
		LEVEL 1 FOR 572.5;
	}
}

TRANSITION_LIST("ADDR[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 32.5;
		LEVEL 1 FOR 92.5;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 272.5;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 45.0;
		LEVEL 0 FOR 157.5;
		LEVEL 1 FOR 357.5;
	}
}

TRANSITION_LIST("ADDR[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 227.5;
		LEVEL 1 FOR 12.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 0 FOR 15.0;
			LEVEL 1 FOR 30.0;
		}
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 135.0;
		LEVEL 1 FOR 80.0;
		LEVEL 0 FOR 80.0;
		LEVEL 1 FOR 277.5;
	}
}

TRANSITION_LIST("ADDR[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 112.5;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 90.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 95.0;
		NODE
		{
			REPEAT = 3;
			LEVEL 1 FOR 40.0;
			LEVEL 0 FOR 40.0;
		}
		LEVEL 1 FOR 237.5;
	}
}

TRANSITION_LIST("ADDR[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 60.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 65.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 75.0;
		NODE
		{
			REPEAT = 7;
			LEVEL 1 FOR 20.0;
			LEVEL 0 FOR 20.0;
		}
		LEVEL 1 FOR 217.5;
	}
}

TRANSITION_LIST("ADDR[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 50.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 55.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 65.0;
		NODE
		{
			REPEAT = 15;
			LEVEL 1 FOR 10.0;
			LEVEL 0 FOR 10.0;
		}
		LEVEL 1 FOR 207.5;
	}
}

TRANSITION_LIST("ADDR[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 10.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 0 FOR 5.0;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 12.5;
			LEVEL 1 FOR 37.5;
		}
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 37.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 22.5;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 27.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 47.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 22.5;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 52.5;
		NODE
		{
			REPEAT = 30;
			LEVEL 0 FOR 5.0;
			LEVEL 1 FOR 5.0;
		}
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 202.5;
	}
}

TRANSITION_LIST("CACHE-RAM_DATA_BUS[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 35.0;
		LEVEL 0 FOR 17.5;
		LEVEL Z FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 5.0;
		LEVEL Z FOR 10.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 17.5;
		LEVEL Z FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 7.5;
		LEVEL Z FOR 5.0;
		LEVEL 0 FOR 32.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 12.5;
		LEVEL Z FOR 10.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 17.5;
		LEVEL Z FOR 5.0;
		LEVEL 0 FOR 42.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("CACHE-RAM_DATA_BUS[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 17.5;
		LEVEL Z FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 22.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 5.0;
		LEVEL Z FOR 10.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 17.5;
		LEVEL Z FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 17.5;
		LEVEL Z FOR 5.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 10.0;
			LEVEL 0 FOR 22.5;
		}
		LEVEL Z FOR 10.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 7.5;
		LEVEL Z FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 22.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("CACHE-RAM_DATA_BUS[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 7.5;
		LEVEL Z FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 22.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 5.0;
		LEVEL Z FOR 10.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 7.5;
		LEVEL Z FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 7.5;
		LEVEL Z FOR 5.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 12.5;
		LEVEL Z FOR 10.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 7.5;
		LEVEL Z FOR 5.0;
		LEVEL 0 FOR 27.5;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("CACHE-RAM_DATA_BUS[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 2.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 5.0;
		}
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 22.5;
		LEVEL Z FOR 5.0;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 5.0;
		LEVEL Z FOR 10.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL Z FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL Z FOR 5.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 5.0;
		LEVEL Z FOR 10.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL Z FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 32.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("CACHE-RAM_DATA_BUS[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 2.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 5.0;
		}
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 22.5;
		LEVEL Z FOR 5.0;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 27.5;
		LEVEL Z FOR 10.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL Z FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL Z FOR 5.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 5.0;
		LEVEL Z FOR 10.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL Z FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 22.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("CACHE-RAM_DATA_BUS[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 2.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 5.0;
		}
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 22.5;
		LEVEL Z FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 22.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 27.5;
		LEVEL Z FOR 10.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL Z FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL Z FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 27.5;
		LEVEL Z FOR 10.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL Z FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("CACHE-RAM_DATA_BUS[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 7.5;
		LEVEL Z FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 22.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 5.0;
		LEVEL Z FOR 10.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 17.5;
		LEVEL Z FOR 15.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 7.5;
		LEVEL Z FOR 5.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 27.5;
		LEVEL Z FOR 10.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 7.5;
		LEVEL Z FOR 5.0;
		LEVEL 0 FOR 17.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("CACHE-RAM_DATA_BUS[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 7.5;
		LEVEL Z FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 22.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 5.0;
		LEVEL Z FOR 10.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 22.5;
		LEVEL Z FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 7.5;
		LEVEL Z FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 5.0;
		LEVEL Z FOR 10.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 17.5;
		LEVEL Z FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("DATA[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 35.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 50.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 65.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("DATA[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 55.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 17.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 17.5;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("DATA[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 47.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 35.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 5.0;
			LEVEL 1 FOR 10.0;
			LEVEL 0 FOR 7.5;
			LEVEL 1 FOR 15.0;
			LEVEL 0 FOR 2.5;
		}
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 47.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("DATA[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 2.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 5.0;
		}
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 47.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 60.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 27.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("DATA[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 2.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 5.0;
		}
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 47.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 60.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 17.5;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("DATA[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 2.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 5.0;
		}
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 10.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 0 FOR 2.5;
			LEVEL 1 FOR 5.0;
		}
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 60.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 17.5;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("DATA[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 47.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 50.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 40.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 27.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("DATA[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 10.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 0 FOR 2.5;
			LEVEL 1 FOR 5.0;
		}
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 27.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 27.5;
		LEVEL 0 FOR 17.5;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("DELAY_ITERATION")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 65.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 20.0;
			LEVEL 0 FOR 40.0;
		}
		LEVEL 1 FOR 15.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 0 FOR 40.0;
			LEVEL 1 FOR 5.0;
		}
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 35.0;
		LEVEL 0 FOR 525.0;
	}
}

TRANSITION_LIST("FLAGS[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("FLAGS[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("FLAGS[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("FLAGS[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 190.0;
		LEVEL 1 FOR 255.0;
		LEVEL 0 FOR 555.0;
	}
}

TRANSITION_LIST("IP[8]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("IP[9]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("IP[10]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("IP[11]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("ADDR[8]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("ADDR[9]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("ADDR[10]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("ADDR[11]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("ACLR_COUNTER")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 65.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 0 FOR 25.0;
			LEVEL 1 FOR 35.0;
		}
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 35.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 40.0;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 40.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 35.0;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 525.0;
	}
}

TRANSITION_LIST("ACLR_COUNTER_OUT")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 10.0;
		NODE
		{
			REPEAT = 2;
			LEVEL X FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		LEVEL X FOR 2.5;
		LEVEL 0 FOR 22.5;
		NODE
		{
			REPEAT = 2;
			LEVEL X FOR 2.5;
			LEVEL 0 FOR 57.5;
		}
		LEVEL X FOR 2.5;
		LEVEL 0 FOR 52.5;
		NODE
		{
			REPEAT = 2;
			LEVEL X FOR 2.5;
			LEVEL 0 FOR 42.5;
		}
		LEVEL X FOR 2.5;
		LEVEL 0 FOR 62.5;
		LEVEL X FOR 2.5;
		LEVEL 0 FOR 42.5;
		LEVEL X FOR 2.5;
		LEVEL 0 FOR 72.5;
		NODE
		{
			REPEAT = 60;
			LEVEL X FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		LEVEL X FOR 205.0;
	}
}

TRANSITION_LIST("ADDR_CACHE[11]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("ADDR_CACHE[10]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("ADDR_CACHE[9]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("ADDR_CACHE[8]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("ADDR_CACHE[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 185.0;
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 75.0;
		LEVEL 1 FOR 35.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 590.0;
	}
}

TRANSITION_LIST("ADDR_CACHE[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 125.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 185.0;
		LEVEL 1 FOR 45.0;
		LEVEL 0 FOR 515.0;
	}
}

TRANSITION_LIST("ADDR_CACHE[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 65.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 90.0;
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 35.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 15.0;
			LEVEL 0 FOR 30.0;
		}
		LEVEL 1 FOR 35.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 45.0;
		LEVEL 0 FOR 515.0;
	}
}

TRANSITION_LIST("ADDR_CACHE[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("ADDR_CACHE[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("ADDR_CACHE[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("ADDR_CACHE[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 65.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 190.0;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 700.0;
	}
}

TRANSITION_LIST("ADDR_CACHE[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 65.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 85.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 515.0;
	}
}

TRANSITION_LIST("ADDR_MEM_OUT[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 32.5;
		LEVEL 1 FOR 32.5;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 130.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 140.0;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 515.0;
	}
}

TRANSITION_LIST("ADDR_MEM_OUT[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 125.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 172.5;
		LEVEL 1 FOR 572.5;
	}
}

TRANSITION_LIST("ADDR_MEM_OUT[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 32.5;
		LEVEL 1 FOR 92.5;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 272.5;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 45.0;
		LEVEL 0 FOR 157.5;
		LEVEL 1 FOR 357.5;
	}
}

TRANSITION_LIST("ADDR_MEM_OUT[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 227.5;
		LEVEL 1 FOR 12.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 0 FOR 15.0;
			LEVEL 1 FOR 30.0;
		}
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 135.0;
		LEVEL 1 FOR 80.0;
		LEVEL 0 FOR 80.0;
		LEVEL 1 FOR 277.5;
	}
}

TRANSITION_LIST("ADDR_MEM_OUT[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 112.5;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 90.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 95.0;
		NODE
		{
			REPEAT = 3;
			LEVEL 1 FOR 40.0;
			LEVEL 0 FOR 40.0;
		}
		LEVEL 1 FOR 237.5;
	}
}

TRANSITION_LIST("ADDR_MEM_OUT[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 60.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 65.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 75.0;
		NODE
		{
			REPEAT = 7;
			LEVEL 1 FOR 20.0;
			LEVEL 0 FOR 20.0;
		}
		LEVEL 1 FOR 217.5;
	}
}

TRANSITION_LIST("ADDR_MEM_OUT[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 50.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 55.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 65.0;
		NODE
		{
			REPEAT = 15;
			LEVEL 1 FOR 10.0;
			LEVEL 0 FOR 10.0;
		}
		LEVEL 1 FOR 207.5;
	}
}

TRANSITION_LIST("ADDR_MEM_OUT[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 10.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 0 FOR 5.0;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 12.5;
			LEVEL 1 FOR 37.5;
		}
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 37.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 22.5;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 27.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 47.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 22.5;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 52.5;
		NODE
		{
			REPEAT = 30;
			LEVEL 0 FOR 5.0;
			LEVEL 1 FOR 5.0;
		}
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 202.5;
	}
}

TRANSITION_LIST("CACHE_DATA_OUT[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 77.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 200.0;
		LEVEL 1 FOR 45.0;
		LEVEL 0 FOR 667.5;
	}
}

TRANSITION_LIST("CACHE_DATA_OUT[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 77.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 37.5;
		LEVEL 0 FOR 65.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 50.0;
		LEVEL 0 FOR 37.5;
		LEVEL 1 FOR 55.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 50.0;
		LEVEL 1 FOR 45.0;
		LEVEL 0 FOR 17.5;
		LEVEL 1 FOR 532.5;
	}
}

TRANSITION_LIST("CACHE_DATA_OUT[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 77.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 62.5;
		LEVEL 1 FOR 37.5;
		LEVEL 0 FOR 62.5;
		LEVEL 1 FOR 82.5;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 127.5;
		LEVEL 1 FOR 520.0;
	}
}

TRANSITION_LIST("CACHE_DATA_OUT[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 90.0;
		LEVEL 1 FOR 37.5;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 37.5;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 87.5;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 22.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 92.5;
		LEVEL 0 FOR 27.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 520.0;
	}
}

TRANSITION_LIST("CACHE_DATA_OUT[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 90.0;
		LEVEL 1 FOR 37.5;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 37.5;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 52.5;
		LEVEL 1 FOR 37.5;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 22.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 92.5;
		LEVEL 0 FOR 17.5;
		LEVEL 1 FOR 532.5;
	}
}

TRANSITION_LIST("CACHE_DATA_OUT[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 77.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 37.5;
		LEVEL 0 FOR 65.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 50.0;
		LEVEL 0 FOR 37.5;
		LEVEL 1 FOR 55.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 50.0;
		LEVEL 1 FOR 45.0;
		LEVEL 0 FOR 17.5;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 520.0;
	}
}

TRANSITION_LIST("CACHE_DATA_OUT[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 77.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 62.5;
		LEVEL 1 FOR 37.5;
		LEVEL 0 FOR 62.5;
		LEVEL 1 FOR 82.5;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 115.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 522.5;
	}
}

TRANSITION_LIST("CACHE_DATA_OUT[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 77.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 37.5;
		LEVEL 0 FOR 65.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 50.0;
		LEVEL 0 FOR 37.5;
		LEVEL 1 FOR 55.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 92.5;
		LEVEL 0 FOR 17.5;
		LEVEL 1 FOR 532.5;
	}
}

TRANSITION_LIST("CACHE_MISS_OUT")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 67.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 22.5;
			LEVEL 0 FOR 37.5;
		}
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 132.5;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 85.0;
		LEVEL 1 FOR 37.5;
		LEVEL 0 FOR 520.0;
	}
}

TRANSITION_LIST("CACHE_TAG_OUT[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("CACHE_TAG_OUT[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("CACHE_TAG_OUT[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("CACHE_TAG_OUT[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("CACHE_TAG_OUT[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 200.0;
		LEVEL 1 FOR 87.5;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 147.5;
		LEVEL 0 FOR 520.0;
	}
}

TRANSITION_LIST("CACHE_TAG_OUT[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 150.0;
		LEVEL 1 FOR 37.5;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 87.5;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 122.5;
		LEVEL 1 FOR 520.0;
	}
}

TRANSITION_LIST("CACHE_TAG_OUT[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 90.0;
		LEVEL 1 FOR 37.5;
		LEVEL 0 FOR 72.5;
		LEVEL 1 FOR 800.0;
	}
}

TRANSITION_LIST("CLOCK_CACHE")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 67.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 5.0;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 10.0;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 37.5;
		}
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 42.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 37.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 42.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 7.5;
		}
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 37.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 37.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 520.0;
	}
}

TRANSITION_LIST("CLOCK_COUNT_DEC")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 12;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 22.5;
			NODE
			{
				REPEAT = 7;
				LEVEL 1 FOR 2.5;
				LEVEL 0 FOR 2.5;
			}
		}
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 17.5;
		NODE
		{
			REPEAT = 2;
			NODE
			{
				REPEAT = 7;
				LEVEL 1 FOR 2.5;
				LEVEL 0 FOR 2.5;
			}
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 7.5;
		}
		NODE
		{
			REPEAT = 7;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 27.5;
		NODE
		{
			REPEAT = 7;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 7.5;
		NODE
		{
			REPEAT = 7;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 37.5;
		NODE
		{
			REPEAT = 64;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		LEVEL 1 FOR 205.0;
	}
}

TRANSITION_LIST("CLOCK_FIX")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 67.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 57.5;
		}
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 52.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 42.5;
		}
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 62.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 42.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 555.0;
	}
}

TRANSITION_LIST("CLOCK_FLAG")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 70.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 55.0;
		}
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 50.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 60.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 27.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 520.0;
	}
}

TRANSITION_LIST("CLOCK_MEM_OUT")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 5;
			LEVEL 0 FOR 2.5;
			LEVEL 1 FOR 2.5;
		}
		LEVEL 0 FOR 12.5;
		NODE
		{
			REPEAT = 2;
			NODE
			{
				REPEAT = 2;
				LEVEL 1 FOR 2.5;
				LEVEL 0 FOR 2.5;
			}
			NODE
			{
				REPEAT = 2;
				LEVEL 1 FOR 2.5;
				LEVEL 0 FOR 7.5;
			}
			NODE
			{
				REPEAT = 4;
				LEVEL 1 FOR 2.5;
				LEVEL 0 FOR 2.5;
			}
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 7.5;
		}
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 7.5;
		}
		NODE
		{
			REPEAT = 3;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 7.5;
			NODE
			{
				REPEAT = 2;
				LEVEL 1 FOR 2.5;
				LEVEL 0 FOR 2.5;
			}
			NODE
			{
				REPEAT = 2;
				LEVEL 1 FOR 2.5;
				LEVEL 0 FOR 7.5;
			}
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 7.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 7.5;
		}
		NODE
		{
			REPEAT = 5;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 7.5;
			NODE
			{
				REPEAT = 2;
				LEVEL 1 FOR 2.5;
				LEVEL 0 FOR 2.5;
			}
			NODE
			{
				REPEAT = 2;
				LEVEL 1 FOR 2.5;
				LEVEL 0 FOR 7.5;
			}
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		NODE
		{
			REPEAT = 6;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 7.5;
		NODE
		{
			REPEAT = 61;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 205.0;
	}
}

TRANSITION_LIST("COUNTER[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("COUNTER[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("COUNTER[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("COUNTER[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("COUNTER[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 480.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 512.5;
	}
}

TRANSITION_LIST("COUNTER[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 85.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 12.5;
			LEVEL 0 FOR 47.5;
		}
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 137.5;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 92.5;
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 520.0;
	}
}

TRANSITION_LIST("COUNTER[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 75.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 10.0;
			LEVEL 0 FOR 50.0;
		}
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 45.0;
		NODE
		{
			REPEAT = 2;
			NODE
			{
				REPEAT = 2;
				LEVEL 1 FOR 7.5;
				LEVEL 0 FOR 37.5;
			}
			LEVEL 1 FOR 10.0;
			LEVEL 0 FOR 10.0;
		}
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 520.0;
	}
}

TRANSITION_LIST("COUNTER[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 70.0;
		NODE
		{
			REPEAT = 2;
			NODE
			{
				REPEAT = 2;
				LEVEL 1 FOR 5.0;
				LEVEL 0 FOR 5.0;
			}
			LEVEL 1 FOR 7.5;
			LEVEL 0 FOR 32.5;
		}
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		NODE
		{
			REPEAT = 3;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 40.0;
		}
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 5.0;
		}
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 40.0;
		}
		NODE
		{
			REPEAT = 3;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 5.0;
		}
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 520.0;
	}
}

TRANSITION_LIST("COUNTER_CLOCK")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 67.5;
		NODE
		{
			REPEAT = 2;
			NODE
			{
				REPEAT = 4;
				LEVEL 1 FOR 2.5;
				LEVEL 0 FOR 2.5;
			}
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 37.5;
		}
		NODE
		{
			REPEAT = 3;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		NODE
		{
			REPEAT = 3;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 37.5;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		NODE
		{
			REPEAT = 4;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 37.5;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		NODE
		{
			REPEAT = 6;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 520.0;
	}
}

TRANSITION_LIST("COUNTER_DECODE[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("COUNTER_DECODE[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 2.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 0 FOR 22.5;
			LEVEL 1 FOR 37.5;
		}
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 32.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 0 FOR 22.5;
			LEVEL 1 FOR 22.5;
		}
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 42.5;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 22.5;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 52.5;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("COUNTER_DECODE[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 15.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 10.0;
			LEVEL 0 FOR 30.0;
			LEVEL 1 FOR 7.5;
			LEVEL 0 FOR 12.5;
		}
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 25.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 7.5;
			LEVEL 0 FOR 12.5;
			LEVEL 1 FOR 10.0;
			LEVEL 0 FOR 15.0;
		}
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("COUNTER_DECODE[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 5.0;
		NODE
		{
			REPEAT = 4;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 5.0;
		}
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 2.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 5.0;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 25.0;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 5.0;
			NODE
			{
				REPEAT = 2;
				LEVEL 1 FOR 2.5;
				LEVEL 0 FOR 2.5;
			}
		}
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 20.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 5.0;
			NODE
			{
				REPEAT = 2;
				LEVEL 1 FOR 2.5;
				LEVEL 0 FOR 2.5;
			}
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 5.0;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 10.0;
		}
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		NODE
		{
			REPEAT = 61;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 2.5;
		}
		LEVEL 1 FOR 205.0;
	}
}

TRANSITION_LIST("DATA_REG_GLOB_OUT[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 77.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 55.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 70.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("DATA_REG_GLOB_OUT[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 77.5;
		LEVEL 1 FOR 10.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 0 FOR 2.5;
			LEVEL 1 FOR 5.0;
		}
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 60.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 17.5;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("DATA_REG_GLOB_OUT[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 50.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 47.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 35.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 7.5;
			LEVEL 1 FOR 7.5;
			LEVEL 0 FOR 7.5;
			LEVEL 1 FOR 15.0;
			LEVEL 0 FOR 2.5;
		}
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 47.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("DATA_REG_GLOB_OUT[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 90.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 60.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 27.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("DATA_REG_GLOB_OUT[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 90.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 60.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 17.5;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("DATA_REG_GLOB_OUT[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 77.5;
		LEVEL 1 FOR 10.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 0 FOR 2.5;
			LEVEL 1 FOR 5.0;
		}
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 60.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 17.5;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("DATA_REG_GLOB_OUT[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 50.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 47.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 50.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 37.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 27.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 7.5;
		NODE
		{
			REPEAT = 60;
			LEVEL 0 FOR 2.5;
			LEVEL 1 FOR 2.5;
		}
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 205.0;
	}
}

TRANSITION_LIST("DATA_REG_GLOB_OUT[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 50.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 10.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 0 FOR 2.5;
			LEVEL 1 FOR 5.0;
		}
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 17.5;
		LEVEL 0 FOR 27.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 17.5;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 17.5;
		LEVEL 1 FOR 25.0;
		NODE
		{
			REPEAT = 60;
			LEVEL 0 FOR 2.5;
			LEVEL 1 FOR 2.5;
		}
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 205.0;
	}
}

TRANSITION_LIST("EN_OUT_MEM")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 1 FOR 185.0;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 75.0;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 590.0;
	}
}

TRANSITION_LIST("EN_OUT_REG")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 185.0;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 75.0;
		LEVEL 1 FOR 35.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 590.0;
	}
}

TRANSITION_LIST("FIX_FLAG")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("IN_CACHE[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 75.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 50.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 57.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 795.0;
	}
}

TRANSITION_LIST("IN_CACHE[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 75.0;
		LEVEL 1 FOR 60.0;
		LEVEL 0 FOR 55.0;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 135.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 50.0;
		LEVEL 1 FOR 60.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 537.5;
	}
}

TRANSITION_LIST("IN_CACHE[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 75.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 50.0;
		LEVEL 1 FOR 55.0;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 90.0;
		LEVEL 0 FOR 137.5;
		LEVEL 1 FOR 527.5;
	}
}

TRANSITION_LIST("IN_CACHE[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 75.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 50.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 60.0;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 90.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 105.0;
		LEVEL 0 FOR 540.0;
	}
}

TRANSITION_LIST("IN_CACHE[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 75.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 110.0;
		LEVEL 0 FOR 50.0;
		LEVEL 1 FOR 90.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 105.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 537.5;
	}
}

TRANSITION_LIST("IN_CACHE[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 75.0;
		LEVEL 1 FOR 60.0;
		LEVEL 0 FOR 55.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 137.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 50.0;
		LEVEL 1 FOR 60.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 527.5;
	}
}

TRANSITION_LIST("IN_CACHE[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 75.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 50.0;
		LEVEL 1 FOR 55.0;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 90.0;
		LEVEL 0 FOR 127.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 527.5;
	}
}

TRANSITION_LIST("IN_CACHE[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 75.0;
		LEVEL 1 FOR 60.0;
		LEVEL 0 FOR 55.0;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 137.5;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 105.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 537.5;
	}
}

TRANSITION_LIST("IP_UP_SPEC_OUT")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 52.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 37.5;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 17.5;
		}
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 32.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 17.5;
			LEVEL 1 FOR 2.5;
			LEVEL 0 FOR 22.5;
		}
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 17.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 42.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 17.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 22.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 17.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 52.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 515.0;
	}
}

TRANSITION_LIST("MISS_FIX")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 70.0;
		LEVEL 1 FOR 175.0;
		LEVEL 0 FOR 90.0;
		LEVEL 1 FOR 65.0;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 555.0;
	}
}

TRANSITION_LIST("qq[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 95.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 52.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 47.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 7.5;
			LEVEL 0 FOR 37.5;
		}
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 57.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 37.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 67.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 507.5;
	}
}

TRANSITION_LIST("qq[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 90.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 55.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 50.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 5.0;
			LEVEL 0 FOR 40.0;
		}
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 60.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 70.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 515.0;
	}
}

TRANSITION_LIST("ROM_MEM_OUT")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 1 FOR 65.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 0 FOR 30.0;
			LEVEL 1 FOR 30.0;
		}
		LEVEL 0 FOR 25.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 30.0;
			LEVEL 0 FOR 15.0;
		}
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 515.0;
	}
}

TRANSITION_LIST("SELECT_REG_GLOB_OUT[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("SELECT_REG_GLOB_OUT[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("SELECT_REG_GLOB_OUT[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("SELECT_REG_GLOB_OUT[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 282.5;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 57.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 55.0;
		NODE
		{
			REPEAT = 60;
			LEVEL 0 FOR 2.5;
			LEVEL 1 FOR 2.5;
		}
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 205.0;
	}
}

TRANSITION_LIST("SELECT_REG_GLOB_OUT[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 122.5;
		LEVEL 1 FOR 40.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 55.0;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 45.0;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 12.5;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 55.0;
		NODE
		{
			REPEAT = 60;
			LEVEL 0 FOR 2.5;
			LEVEL 1 FOR 2.5;
		}
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 205.0;
	}
}

TRANSITION_LIST("STOP_OUT")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T0[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T0[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T0[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T0[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T0[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 200.0;
		LEVEL 1 FOR 280.0;
		LEVEL 0 FOR 520.0;
	}
}

TRANSITION_LIST("T0[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 200.0;
		LEVEL 1 FOR 157.5;
		LEVEL 0 FOR 122.5;
		LEVEL 1 FOR 520.0;
	}
}

TRANSITION_LIST("T0[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 200.0;
		LEVEL 1 FOR 800.0;
	}
}

TRANSITION_LIST("T3[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T3[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T3[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T3[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T3[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T3[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T3[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("TAG_FIX[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("TAG_FIX[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("TAG_FIX[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("TAG_FIX[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("TAG_FIX[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 245.0;
		LEVEL 1 FOR 45.0;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 665.0;
	}
}

TRANSITION_LIST("TAG_FIX[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 245.0;
		LEVEL 1 FOR 45.0;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 65.0;
		LEVEL 0 FOR 600.0;
	}
}

TRANSITION_LIST("TAG_FIX[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 245.0;
		LEVEL 1 FOR 755.0;
	}
}

TRANSITION_LIST("WRITE_CACHE")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 70.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 10.0;
			LEVEL 0 FOR 5.0;
			LEVEL 1 FOR 10.0;
			LEVEL 0 FOR 35.0;
		}
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 40.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 95.0;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 35.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 55.0;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 520.0;
	}
}

TRANSITION_LIST("WRITE_ON_GLOB_OUT")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 92.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 57.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 142.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 182.5;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 515.0;
	}
}

TRANSITION_LIST("WRITE_ON_MEM_OUT")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 185.0;
		LEVEL 1 FOR 25.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 75.0;
		LEVEL 1 FOR 35.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 15.0;
		LEVEL 0 FOR 590.0;
	}
}

TRANSITION_LIST("T1[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T1[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T1[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T1[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T1[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T1[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 150.0;
		LEVEL 1 FOR 850.0;
	}
}

TRANSITION_LIST("T1[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T2[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T2[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T2[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T2[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T2[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T2[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("T2[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 90.0;
		LEVEL 1 FOR 910.0;
	}
}

TRANSITION_LIST("WAY")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 135.0;
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 845.0;
	}
}

TRANSITION_LIST("C[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 135.0;
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 845.0;
	}
}

TRANSITION_LIST("C[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 80.0;
		LEVEL 1 FOR 55.0;
		LEVEL 0 FOR 12.5;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 315.0;
		LEVEL 1 FOR 530.0;
	}
}

TRANSITION_LIST("C[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 75.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 7.5;
		LEVEL 1 FOR 47.5;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 7.5;
		LEVEL 0 FOR 317.5;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 525.0;
	}
}

TRANSITION_LIST("C_ALCR")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("C_CLOCK")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 75.0;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 45.0;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 315.0;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 2.5;
		LEVEL 0 FOR 520.0;
	}
}

TRANSITION_LIST("C[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("DMA_ADDR[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 520.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 30.0;
		NODE
		{
			REPEAT = 1;
			LEVEL 0 FOR 30.0;
			LEVEL 1 FOR 30.0;
		}
		LEVEL 0 FOR 260.0;
	}
}

TRANSITION_LIST("DMA_ADDR[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 535.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 415.0;
	}
}

TRANSITION_LIST("DMA_ADDR[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 500.0;
		LEVEL 1 FOR 20.0;
		LEVEL 0 FOR 5.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 15.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 25.0;
		LEVEL 1 FOR 5.0;
		LEVEL 0 FOR 415.0;
	}
}

TRANSITION_LIST("DMA_CLOCK")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 502.5;
		LEVEL 1 FOR 2.5;
		NODE
		{
			REPEAT = 5;
			LEVEL 0 FOR 2.5;
			LEVEL 1 FOR 2.5;
		}
		LEVEL 0 FOR 2.5;
		LEVEL 1 FOR 2.5;
		NODE
		{
			REPEAT = 41;
			LEVEL 0 FOR 2.5;
			LEVEL 1 FOR 2.5;
		}
		LEVEL 0 FOR 260.0;
	}
}

TRANSITION_LIST("DMA_DATA_BIDIR[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL Z FOR 510.0;
		LEVEL 1 FOR 10.0;
		LEVEL Z FOR 20.0;
		LEVEL 0 FOR 10.0;
		LEVEL Z FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL Z FOR 420.0;
	}
}

TRANSITION_LIST("DMA_DATA_BIDIR[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL Z FOR 510.0;
		LEVEL 1 FOR 10.0;
		LEVEL Z FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL Z FOR 20.0;
		LEVEL 0 FOR 10.0;
		LEVEL Z FOR 420.0;
	}
}

TRANSITION_LIST("DMA_DATA_BIDIR[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL Z FOR 510.0;
		LEVEL 0 FOR 10.0;
		LEVEL Z FOR 20.0;
		LEVEL 0 FOR 10.0;
		LEVEL Z FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL Z FOR 420.0;
	}
}

TRANSITION_LIST("DMA_DATA_BIDIR[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL Z FOR 510.0;
		LEVEL 1 FOR 10.0;
		LEVEL Z FOR 20.0;
		LEVEL 0 FOR 10.0;
		LEVEL Z FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL Z FOR 420.0;
	}
}

TRANSITION_LIST("DMA_DATA_BIDIR[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL Z FOR 510.0;
		LEVEL 1 FOR 10.0;
		LEVEL Z FOR 20.0;
		LEVEL 0 FOR 10.0;
		LEVEL Z FOR 20.0;
		LEVEL 0 FOR 10.0;
		LEVEL Z FOR 420.0;
	}
}

TRANSITION_LIST("DMA_DATA_BIDIR[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL Z FOR 510.0;
		LEVEL 1 FOR 10.0;
		LEVEL Z FOR 20.0;
		LEVEL 0 FOR 10.0;
		LEVEL Z FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL Z FOR 420.0;
	}
}

TRANSITION_LIST("DMA_DATA_BIDIR[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL Z FOR 510.0;
		LEVEL 1 FOR 10.0;
		LEVEL Z FOR 20.0;
		LEVEL 0 FOR 10.0;
		LEVEL Z FOR 20.0;
		LEVEL 0 FOR 10.0;
		LEVEL Z FOR 420.0;
	}
}

TRANSITION_LIST("DMA_DATA_BIDIR[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL Z FOR 510.0;
		LEVEL 1 FOR 10.0;
		LEVEL Z FOR 20.0;
		LEVEL 0 FOR 10.0;
		LEVEL Z FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL Z FOR 420.0;
	}
}

TRANSITION_LIST("DMA_WRITE")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 510.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 20.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 420.0;
	}
}

TRANSITION_LIST("DMA_DATA_BIDIR[7]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 47.5;
		NODE
		{
			REPEAT = 2;
			LEVEL Z FOR 57.5;
			LEVEL 0 FOR 2.5;
		}
		LEVEL Z FOR 52.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL Z FOR 42.5;
		}
		LEVEL 1 FOR 2.5;
		LEVEL Z FOR 62.5;
		LEVEL 0 FOR 2.5;
		LEVEL Z FOR 42.5;
		LEVEL 0 FOR 2.5;
		LEVEL Z FOR 72.5;
		LEVEL 0 FOR 145.0;
		LEVEL X FOR 30.0;
		LEVEL 0 FOR 160.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 140.0;
	}
}

TRANSITION_LIST("DMA_DATA_BIDIR[6]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 47.5;
		LEVEL Z FOR 57.5;
		LEVEL 1 FOR 2.5;
		LEVEL Z FOR 57.5;
		LEVEL 0 FOR 2.5;
		LEVEL Z FOR 52.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL Z FOR 42.5;
		}
		LEVEL 1 FOR 2.5;
		LEVEL Z FOR 62.5;
		LEVEL 0 FOR 2.5;
		LEVEL Z FOR 42.5;
		LEVEL 0 FOR 2.5;
		LEVEL Z FOR 72.5;
		LEVEL 1 FOR 95.0;
		LEVEL 0 FOR 410.0;
	}
}

TRANSITION_LIST("DMA_DATA_BIDIR[5]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 47.5;
		LEVEL Z FOR 57.5;
		LEVEL 0 FOR 2.5;
		LEVEL Z FOR 57.5;
		LEVEL 1 FOR 2.5;
		LEVEL Z FOR 52.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL Z FOR 42.5;
		}
		LEVEL 1 FOR 2.5;
		LEVEL Z FOR 62.5;
		LEVEL 0 FOR 2.5;
		LEVEL Z FOR 42.5;
		LEVEL 0 FOR 2.5;
		LEVEL Z FOR 72.5;
		LEVEL 1 FOR 95.0;
		LEVEL 0 FOR 50.0;
		LEVEL X FOR 30.0;
		LEVEL 0 FOR 160.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 140.0;
	}
}

TRANSITION_LIST("DMA_DATA_BIDIR[4]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 47.5;
		NODE
		{
			REPEAT = 2;
			LEVEL Z FOR 57.5;
			LEVEL 1 FOR 2.5;
		}
		LEVEL Z FOR 52.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL Z FOR 42.5;
		}
		LEVEL 1 FOR 2.5;
		LEVEL Z FOR 62.5;
		LEVEL 1 FOR 2.5;
		LEVEL Z FOR 42.5;
		LEVEL 1 FOR 2.5;
		LEVEL Z FOR 72.5;
		LEVEL 0 FOR 95.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 20.0;
		LEVEL X FOR 30.0;
		LEVEL 0 FOR 10.0;
		LEVEL 1 FOR 30.0;
		LEVEL 0 FOR 60.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 60.0;
			LEVEL 0 FOR 30.0;
		}
		LEVEL 1 FOR 50.0;
	}
}

TRANSITION_LIST("DMA_DATA_BIDIR[3]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 47.5;
		NODE
		{
			REPEAT = 2;
			LEVEL Z FOR 57.5;
			LEVEL 1 FOR 2.5;
		}
		LEVEL Z FOR 52.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 0 FOR 2.5;
			LEVEL Z FOR 42.5;
		}
		LEVEL 0 FOR 2.5;
		LEVEL Z FOR 62.5;
		LEVEL 1 FOR 2.5;
		LEVEL Z FOR 42.5;
		LEVEL 1 FOR 2.5;
		LEVEL Z FOR 72.5;
		LEVEL 1 FOR 95.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 20.0;
		LEVEL X FOR 30.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 60.0;
		NODE
		{
			REPEAT = 2;
			LEVEL 0 FOR 60.0;
			LEVEL 1 FOR 30.0;
		}
		LEVEL 0 FOR 50.0;
	}
}

TRANSITION_LIST("DMA_DATA_BIDIR[2]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 47.5;
		LEVEL Z FOR 57.5;
		LEVEL 1 FOR 2.5;
		LEVEL Z FOR 57.5;
		LEVEL 0 FOR 2.5;
		LEVEL Z FOR 52.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 0 FOR 2.5;
			LEVEL Z FOR 42.5;
		}
		LEVEL 0 FOR 2.5;
		LEVEL Z FOR 62.5;
		LEVEL 0 FOR 2.5;
		LEVEL Z FOR 42.5;
		LEVEL 0 FOR 2.5;
		LEVEL Z FOR 72.5;
		LEVEL 0 FOR 95.0;
		LEVEL 1 FOR 50.0;
		LEVEL X FOR 30.0;
		LEVEL 1 FOR 10.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 60.0;
		LEVEL 0 FOR 120.0;
		LEVEL 1 FOR 110.0;
	}
}

TRANSITION_LIST("DMA_DATA_BIDIR[1]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 47.5;
		LEVEL Z FOR 57.5;
		LEVEL 0 FOR 2.5;
		LEVEL Z FOR 57.5;
		LEVEL 1 FOR 2.5;
		LEVEL Z FOR 52.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 1 FOR 2.5;
			LEVEL Z FOR 42.5;
		}
		LEVEL 1 FOR 2.5;
		LEVEL Z FOR 62.5;
		LEVEL 0 FOR 2.5;
		LEVEL Z FOR 42.5;
		LEVEL 0 FOR 2.5;
		LEVEL Z FOR 72.5;
		LEVEL 0 FOR 125.0;
		LEVEL 1 FOR 60.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 60.0;
		LEVEL 0 FOR 60.0;
		LEVEL 1 FOR 60.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 80.0;
	}
}

TRANSITION_LIST("DMA_DATA_BIDIR[0]~result")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 47.5;
		LEVEL Z FOR 57.5;
		LEVEL 1 FOR 2.5;
		LEVEL Z FOR 57.5;
		LEVEL 0 FOR 2.5;
		LEVEL Z FOR 52.5;
		NODE
		{
			REPEAT = 2;
			LEVEL 0 FOR 2.5;
			LEVEL Z FOR 42.5;
		}
		LEVEL 0 FOR 2.5;
		LEVEL Z FOR 62.5;
		LEVEL 1 FOR 2.5;
		LEVEL Z FOR 42.5;
		LEVEL 1 FOR 2.5;
		LEVEL Z FOR 72.5;
		LEVEL 1 FOR 185.0;
		LEVEL 0 FOR 30.0;
		LEVEL 1 FOR 60.0;
		NODE
		{
			REPEAT = 3;
			LEVEL 0 FOR 30.0;
			LEVEL 1 FOR 30.0;
		}
		LEVEL 0 FOR 50.0;
	}
}

DISPLAY_LINE
{
	CHANNEL = "AX";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 0;
	TREE_LEVEL = 0;
	CHILDREN = 1, 2, 3, 4, 5, 6, 7, 8;
}

DISPLAY_LINE
{
	CHANNEL = "AX[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 1;
	TREE_LEVEL = 1;
	PARENT = 0;
}

DISPLAY_LINE
{
	CHANNEL = "AX[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 2;
	TREE_LEVEL = 1;
	PARENT = 0;
}

DISPLAY_LINE
{
	CHANNEL = "AX[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 3;
	TREE_LEVEL = 1;
	PARENT = 0;
}

DISPLAY_LINE
{
	CHANNEL = "AX[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 4;
	TREE_LEVEL = 1;
	PARENT = 0;
}

DISPLAY_LINE
{
	CHANNEL = "AX[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 5;
	TREE_LEVEL = 1;
	PARENT = 0;
}

DISPLAY_LINE
{
	CHANNEL = "AX[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 6;
	TREE_LEVEL = 1;
	PARENT = 0;
}

DISPLAY_LINE
{
	CHANNEL = "AX[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 7;
	TREE_LEVEL = 1;
	PARENT = 0;
}

DISPLAY_LINE
{
	CHANNEL = "AX[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 8;
	TREE_LEVEL = 1;
	PARENT = 0;
}

DISPLAY_LINE
{
	CHANNEL = "BX";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 9;
	TREE_LEVEL = 0;
	CHILDREN = 10, 11, 12, 13, 14, 15, 16, 17;
}

DISPLAY_LINE
{
	CHANNEL = "BX[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 10;
	TREE_LEVEL = 1;
	PARENT = 9;
}

DISPLAY_LINE
{
	CHANNEL = "BX[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 11;
	TREE_LEVEL = 1;
	PARENT = 9;
}

DISPLAY_LINE
{
	CHANNEL = "BX[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 12;
	TREE_LEVEL = 1;
	PARENT = 9;
}

DISPLAY_LINE
{
	CHANNEL = "BX[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 13;
	TREE_LEVEL = 1;
	PARENT = 9;
}

DISPLAY_LINE
{
	CHANNEL = "BX[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 14;
	TREE_LEVEL = 1;
	PARENT = 9;
}

DISPLAY_LINE
{
	CHANNEL = "BX[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 15;
	TREE_LEVEL = 1;
	PARENT = 9;
}

DISPLAY_LINE
{
	CHANNEL = "BX[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 16;
	TREE_LEVEL = 1;
	PARENT = 9;
}

DISPLAY_LINE
{
	CHANNEL = "BX[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 17;
	TREE_LEVEL = 1;
	PARENT = 9;
}

DISPLAY_LINE
{
	CHANNEL = "CX";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 18;
	TREE_LEVEL = 0;
	CHILDREN = 19, 20, 21, 22, 23, 24, 25, 26;
}

DISPLAY_LINE
{
	CHANNEL = "CX[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 19;
	TREE_LEVEL = 1;
	PARENT = 18;
}

DISPLAY_LINE
{
	CHANNEL = "CX[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 20;
	TREE_LEVEL = 1;
	PARENT = 18;
}

DISPLAY_LINE
{
	CHANNEL = "CX[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 21;
	TREE_LEVEL = 1;
	PARENT = 18;
}

DISPLAY_LINE
{
	CHANNEL = "CX[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 22;
	TREE_LEVEL = 1;
	PARENT = 18;
}

DISPLAY_LINE
{
	CHANNEL = "CX[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 23;
	TREE_LEVEL = 1;
	PARENT = 18;
}

DISPLAY_LINE
{
	CHANNEL = "CX[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 24;
	TREE_LEVEL = 1;
	PARENT = 18;
}

DISPLAY_LINE
{
	CHANNEL = "CX[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 25;
	TREE_LEVEL = 1;
	PARENT = 18;
}

DISPLAY_LINE
{
	CHANNEL = "CX[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 26;
	TREE_LEVEL = 1;
	PARENT = 18;
}

DISPLAY_LINE
{
	CHANNEL = "DX";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 27;
	TREE_LEVEL = 0;
	CHILDREN = 28, 29, 30, 31, 32, 33, 34, 35;
}

DISPLAY_LINE
{
	CHANNEL = "DX[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 28;
	TREE_LEVEL = 1;
	PARENT = 27;
}

DISPLAY_LINE
{
	CHANNEL = "DX[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 29;
	TREE_LEVEL = 1;
	PARENT = 27;
}

DISPLAY_LINE
{
	CHANNEL = "DX[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 30;
	TREE_LEVEL = 1;
	PARENT = 27;
}

DISPLAY_LINE
{
	CHANNEL = "DX[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 31;
	TREE_LEVEL = 1;
	PARENT = 27;
}

DISPLAY_LINE
{
	CHANNEL = "DX[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 32;
	TREE_LEVEL = 1;
	PARENT = 27;
}

DISPLAY_LINE
{
	CHANNEL = "DX[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 33;
	TREE_LEVEL = 1;
	PARENT = 27;
}

DISPLAY_LINE
{
	CHANNEL = "DX[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 34;
	TREE_LEVEL = 1;
	PARENT = 27;
}

DISPLAY_LINE
{
	CHANNEL = "DX[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 35;
	TREE_LEVEL = 1;
	PARENT = 27;
}

DISPLAY_LINE
{
	CHANNEL = "CLOCK";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 36;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_ADDR";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 37;
	TREE_LEVEL = 0;
	CHILDREN = 38, 39, 40;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_ADDR[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 38;
	TREE_LEVEL = 1;
	PARENT = 37;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_ADDR[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 39;
	TREE_LEVEL = 1;
	PARENT = 37;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_ADDR[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 40;
	TREE_LEVEL = 1;
	PARENT = 37;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_CLOCK";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 41;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_WRITE";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 42;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_DATA_BIDIR";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 43;
	TREE_LEVEL = 0;
	CHILDREN = 44, 45, 46, 47, 48, 49, 50, 51;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_DATA_BIDIR[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 44;
	TREE_LEVEL = 1;
	PARENT = 43;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_DATA_BIDIR[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 45;
	TREE_LEVEL = 1;
	PARENT = 43;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_DATA_BIDIR[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 46;
	TREE_LEVEL = 1;
	PARENT = 43;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_DATA_BIDIR[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 47;
	TREE_LEVEL = 1;
	PARENT = 43;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_DATA_BIDIR[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 48;
	TREE_LEVEL = 1;
	PARENT = 43;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_DATA_BIDIR[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 49;
	TREE_LEVEL = 1;
	PARENT = 43;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_DATA_BIDIR[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 50;
	TREE_LEVEL = 1;
	PARENT = 43;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_DATA_BIDIR[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 51;
	TREE_LEVEL = 1;
	PARENT = 43;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_DATA_BIDIR~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 52;
	TREE_LEVEL = 0;
	CHILDREN = 53, 54, 55, 56, 57, 58, 59, 60;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_DATA_BIDIR[7]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 53;
	TREE_LEVEL = 1;
	PARENT = 52;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_DATA_BIDIR[6]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 54;
	TREE_LEVEL = 1;
	PARENT = 52;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_DATA_BIDIR[5]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 55;
	TREE_LEVEL = 1;
	PARENT = 52;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_DATA_BIDIR[4]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 56;
	TREE_LEVEL = 1;
	PARENT = 52;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_DATA_BIDIR[3]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 57;
	TREE_LEVEL = 1;
	PARENT = 52;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_DATA_BIDIR[2]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 58;
	TREE_LEVEL = 1;
	PARENT = 52;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_DATA_BIDIR[1]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 59;
	TREE_LEVEL = 1;
	PARENT = 52;
}

DISPLAY_LINE
{
	CHANNEL = "DMA_DATA_BIDIR[0]~result";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 60;
	TREE_LEVEL = 1;
	PARENT = 52;
}

DISPLAY_LINE
{
	CHANNEL = "IP";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 61;
	TREE_LEVEL = 0;
	CHILDREN = 62, 63, 64, 65, 66, 67, 68, 69, 70, 71, 72, 73;
}

DISPLAY_LINE
{
	CHANNEL = "IP[11]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 62;
	TREE_LEVEL = 1;
	PARENT = 61;
}

DISPLAY_LINE
{
	CHANNEL = "IP[10]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 63;
	TREE_LEVEL = 1;
	PARENT = 61;
}

DISPLAY_LINE
{
	CHANNEL = "IP[9]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 64;
	TREE_LEVEL = 1;
	PARENT = 61;
}

DISPLAY_LINE
{
	CHANNEL = "IP[8]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 65;
	TREE_LEVEL = 1;
	PARENT = 61;
}

DISPLAY_LINE
{
	CHANNEL = "IP[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 66;
	TREE_LEVEL = 1;
	PARENT = 61;
}

DISPLAY_LINE
{
	CHANNEL = "IP[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 67;
	TREE_LEVEL = 1;
	PARENT = 61;
}

DISPLAY_LINE
{
	CHANNEL = "IP[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 68;
	TREE_LEVEL = 1;
	PARENT = 61;
}

DISPLAY_LINE
{
	CHANNEL = "IP[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 69;
	TREE_LEVEL = 1;
	PARENT = 61;
}

DISPLAY_LINE
{
	CHANNEL = "IP[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 70;
	TREE_LEVEL = 1;
	PARENT = 61;
}

DISPLAY_LINE
{
	CHANNEL = "IP[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 71;
	TREE_LEVEL = 1;
	PARENT = 61;
}

DISPLAY_LINE
{
	CHANNEL = "IP[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 72;
	TREE_LEVEL = 1;
	PARENT = 61;
}

DISPLAY_LINE
{
	CHANNEL = "IP[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 73;
	TREE_LEVEL = 1;
	PARENT = 61;
}

DISPLAY_LINE
{
	CHANNEL = "IR";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 74;
	TREE_LEVEL = 0;
	CHILDREN = 75, 76, 77, 78;
}

DISPLAY_LINE
{
	CHANNEL = "IR[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 75;
	TREE_LEVEL = 1;
	PARENT = 74;
}

DISPLAY_LINE
{
	CHANNEL = "IR[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 76;
	TREE_LEVEL = 1;
	PARENT = 74;
}

DISPLAY_LINE
{
	CHANNEL = "IR[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 77;
	TREE_LEVEL = 1;
	PARENT = 74;
}

DISPLAY_LINE
{
	CHANNEL = "IR[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 78;
	TREE_LEVEL = 1;
	PARENT = 74;
}

DISPLAY_LINE
{
	CHANNEL = "AR";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 79;
	TREE_LEVEL = 0;
	CHILDREN = 80, 81, 82, 83, 84, 85, 86, 87;
}

DISPLAY_LINE
{
	CHANNEL = "AR[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 80;
	TREE_LEVEL = 1;
	PARENT = 79;
}

DISPLAY_LINE
{
	CHANNEL = "AR[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 81;
	TREE_LEVEL = 1;
	PARENT = 79;
}

DISPLAY_LINE
{
	CHANNEL = "AR[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 82;
	TREE_LEVEL = 1;
	PARENT = 79;
}

DISPLAY_LINE
{
	CHANNEL = "AR[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 83;
	TREE_LEVEL = 1;
	PARENT = 79;
}

DISPLAY_LINE
{
	CHANNEL = "AR[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 84;
	TREE_LEVEL = 1;
	PARENT = 79;
}

DISPLAY_LINE
{
	CHANNEL = "AR[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 85;
	TREE_LEVEL = 1;
	PARENT = 79;
}

DISPLAY_LINE
{
	CHANNEL = "AR[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 86;
	TREE_LEVEL = 1;
	PARENT = 79;
}

DISPLAY_LINE
{
	CHANNEL = "AR[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 87;
	TREE_LEVEL = 1;
	PARENT = 79;
}

DISPLAY_LINE
{
	CHANNEL = "DR";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 88;
	TREE_LEVEL = 0;
	CHILDREN = 89, 90, 91, 92, 93, 94, 95, 96;
}

DISPLAY_LINE
{
	CHANNEL = "DR[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 89;
	TREE_LEVEL = 1;
	PARENT = 88;
}

DISPLAY_LINE
{
	CHANNEL = "DR[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 90;
	TREE_LEVEL = 1;
	PARENT = 88;
}

DISPLAY_LINE
{
	CHANNEL = "DR[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 91;
	TREE_LEVEL = 1;
	PARENT = 88;
}

DISPLAY_LINE
{
	CHANNEL = "DR[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 92;
	TREE_LEVEL = 1;
	PARENT = 88;
}

DISPLAY_LINE
{
	CHANNEL = "DR[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 93;
	TREE_LEVEL = 1;
	PARENT = 88;
}

DISPLAY_LINE
{
	CHANNEL = "DR[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 94;
	TREE_LEVEL = 1;
	PARENT = 88;
}

DISPLAY_LINE
{
	CHANNEL = "DR[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 95;
	TREE_LEVEL = 1;
	PARENT = 88;
}

DISPLAY_LINE
{
	CHANNEL = "DR[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 96;
	TREE_LEVEL = 1;
	PARENT = 88;
}

DISPLAY_LINE
{
	CHANNEL = "ACLR_COUNTER";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 97;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "ACLR_COUNTER_OUT";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 98;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "WRITE_CACHE";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 99;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "CLOCK_CACHE";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 100;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_CACHE";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 101;
	TREE_LEVEL = 0;
	CHILDREN = 102, 103, 104, 105, 106, 107, 108, 109, 110, 111, 112, 113;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_CACHE[11]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 102;
	TREE_LEVEL = 1;
	PARENT = 101;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_CACHE[10]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 103;
	TREE_LEVEL = 1;
	PARENT = 101;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_CACHE[9]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 104;
	TREE_LEVEL = 1;
	PARENT = 101;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_CACHE[8]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 105;
	TREE_LEVEL = 1;
	PARENT = 101;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_CACHE[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 106;
	TREE_LEVEL = 1;
	PARENT = 101;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_CACHE[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 107;
	TREE_LEVEL = 1;
	PARENT = 101;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_CACHE[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 108;
	TREE_LEVEL = 1;
	PARENT = 101;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_CACHE[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 109;
	TREE_LEVEL = 1;
	PARENT = 101;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_CACHE[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 110;
	TREE_LEVEL = 1;
	PARENT = 101;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_CACHE[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 111;
	TREE_LEVEL = 1;
	PARENT = 101;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_CACHE[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 112;
	TREE_LEVEL = 1;
	PARENT = 101;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_CACHE[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 113;
	TREE_LEVEL = 1;
	PARENT = 101;
}

DISPLAY_LINE
{
	CHANNEL = "IN_CACHE";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 114;
	TREE_LEVEL = 0;
	CHILDREN = 115, 116, 117, 118, 119, 120, 121, 122;
}

DISPLAY_LINE
{
	CHANNEL = "IN_CACHE[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 115;
	TREE_LEVEL = 1;
	PARENT = 114;
}

DISPLAY_LINE
{
	CHANNEL = "IN_CACHE[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 116;
	TREE_LEVEL = 1;
	PARENT = 114;
}

DISPLAY_LINE
{
	CHANNEL = "IN_CACHE[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 117;
	TREE_LEVEL = 1;
	PARENT = 114;
}

DISPLAY_LINE
{
	CHANNEL = "IN_CACHE[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 118;
	TREE_LEVEL = 1;
	PARENT = 114;
}

DISPLAY_LINE
{
	CHANNEL = "IN_CACHE[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 119;
	TREE_LEVEL = 1;
	PARENT = 114;
}

DISPLAY_LINE
{
	CHANNEL = "IN_CACHE[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 120;
	TREE_LEVEL = 1;
	PARENT = 114;
}

DISPLAY_LINE
{
	CHANNEL = "IN_CACHE[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 121;
	TREE_LEVEL = 1;
	PARENT = 114;
}

DISPLAY_LINE
{
	CHANNEL = "IN_CACHE[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 122;
	TREE_LEVEL = 1;
	PARENT = 114;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE_MISS_OUT";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 123;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE_DATA_OUT";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 124;
	TREE_LEVEL = 0;
	CHILDREN = 125, 126, 127, 128, 129, 130, 131, 132;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE_DATA_OUT[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 125;
	TREE_LEVEL = 1;
	PARENT = 124;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE_DATA_OUT[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 126;
	TREE_LEVEL = 1;
	PARENT = 124;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE_DATA_OUT[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 127;
	TREE_LEVEL = 1;
	PARENT = 124;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE_DATA_OUT[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 128;
	TREE_LEVEL = 1;
	PARENT = 124;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE_DATA_OUT[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 129;
	TREE_LEVEL = 1;
	PARENT = 124;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE_DATA_OUT[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 130;
	TREE_LEVEL = 1;
	PARENT = 124;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE_DATA_OUT[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 131;
	TREE_LEVEL = 1;
	PARENT = 124;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE_DATA_OUT[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 132;
	TREE_LEVEL = 1;
	PARENT = 124;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE_TAG_OUT";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 133;
	TREE_LEVEL = 0;
	CHILDREN = 134, 135, 136, 137, 138, 139, 140;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE_TAG_OUT[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 134;
	TREE_LEVEL = 1;
	PARENT = 133;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE_TAG_OUT[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 135;
	TREE_LEVEL = 1;
	PARENT = 133;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE_TAG_OUT[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 136;
	TREE_LEVEL = 1;
	PARENT = 133;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE_TAG_OUT[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 137;
	TREE_LEVEL = 1;
	PARENT = 133;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE_TAG_OUT[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 138;
	TREE_LEVEL = 1;
	PARENT = 133;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE_TAG_OUT[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 139;
	TREE_LEVEL = 1;
	PARENT = 133;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE_TAG_OUT[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 140;
	TREE_LEVEL = 1;
	PARENT = 133;
}

DISPLAY_LINE
{
	CHANNEL = "CLOCK_COUNT_DEC";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 141;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "CLOCK_FIX";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 142;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "CLOCK_FLAG";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 143;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "CLOCK_MEM_OUT";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 144;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_MEM_OUT";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 145;
	TREE_LEVEL = 0;
	CHILDREN = 146, 147, 148, 149, 150, 151, 152, 153;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_MEM_OUT[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 146;
	TREE_LEVEL = 1;
	PARENT = 145;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_MEM_OUT[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 147;
	TREE_LEVEL = 1;
	PARENT = 145;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_MEM_OUT[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 148;
	TREE_LEVEL = 1;
	PARENT = 145;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_MEM_OUT[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 149;
	TREE_LEVEL = 1;
	PARENT = 145;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_MEM_OUT[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 150;
	TREE_LEVEL = 1;
	PARENT = 145;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_MEM_OUT[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 151;
	TREE_LEVEL = 1;
	PARENT = 145;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_MEM_OUT[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 152;
	TREE_LEVEL = 1;
	PARENT = 145;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR_MEM_OUT[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 153;
	TREE_LEVEL = 1;
	PARENT = 145;
}

DISPLAY_LINE
{
	CHANNEL = "WRITE_ON_MEM_OUT";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 154;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE-RAM_DATA_BUS";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 155;
	TREE_LEVEL = 0;
	CHILDREN = 156, 157, 158, 159, 160, 161, 162, 163;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE-RAM_DATA_BUS[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 156;
	TREE_LEVEL = 1;
	PARENT = 155;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE-RAM_DATA_BUS[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 157;
	TREE_LEVEL = 1;
	PARENT = 155;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE-RAM_DATA_BUS[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 158;
	TREE_LEVEL = 1;
	PARENT = 155;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE-RAM_DATA_BUS[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 159;
	TREE_LEVEL = 1;
	PARENT = 155;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE-RAM_DATA_BUS[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 160;
	TREE_LEVEL = 1;
	PARENT = 155;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE-RAM_DATA_BUS[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 161;
	TREE_LEVEL = 1;
	PARENT = 155;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE-RAM_DATA_BUS[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 162;
	TREE_LEVEL = 1;
	PARENT = 155;
}

DISPLAY_LINE
{
	CHANNEL = "CACHE-RAM_DATA_BUS[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 163;
	TREE_LEVEL = 1;
	PARENT = 155;
}

DISPLAY_LINE
{
	CHANNEL = "COUNTER";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 164;
	TREE_LEVEL = 0;
	CHILDREN = 165, 166, 167, 168, 169, 170, 171, 172;
}

DISPLAY_LINE
{
	CHANNEL = "COUNTER[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 165;
	TREE_LEVEL = 1;
	PARENT = 164;
}

DISPLAY_LINE
{
	CHANNEL = "COUNTER[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 166;
	TREE_LEVEL = 1;
	PARENT = 164;
}

DISPLAY_LINE
{
	CHANNEL = "COUNTER[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 167;
	TREE_LEVEL = 1;
	PARENT = 164;
}

DISPLAY_LINE
{
	CHANNEL = "COUNTER[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 168;
	TREE_LEVEL = 1;
	PARENT = 164;
}

DISPLAY_LINE
{
	CHANNEL = "COUNTER[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 169;
	TREE_LEVEL = 1;
	PARENT = 164;
}

DISPLAY_LINE
{
	CHANNEL = "COUNTER[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 170;
	TREE_LEVEL = 1;
	PARENT = 164;
}

DISPLAY_LINE
{
	CHANNEL = "COUNTER[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 171;
	TREE_LEVEL = 1;
	PARENT = 164;
}

DISPLAY_LINE
{
	CHANNEL = "COUNTER[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 172;
	TREE_LEVEL = 1;
	PARENT = 164;
}

DISPLAY_LINE
{
	CHANNEL = "COUNTER_DECODE";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 173;
	TREE_LEVEL = 0;
	CHILDREN = 174, 175, 176, 177;
}

DISPLAY_LINE
{
	CHANNEL = "COUNTER_DECODE[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 174;
	TREE_LEVEL = 1;
	PARENT = 173;
}

DISPLAY_LINE
{
	CHANNEL = "COUNTER_DECODE[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 175;
	TREE_LEVEL = 1;
	PARENT = 173;
}

DISPLAY_LINE
{
	CHANNEL = "COUNTER_DECODE[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 176;
	TREE_LEVEL = 1;
	PARENT = 173;
}

DISPLAY_LINE
{
	CHANNEL = "COUNTER_DECODE[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 177;
	TREE_LEVEL = 1;
	PARENT = 173;
}

DISPLAY_LINE
{
	CHANNEL = "COUNTER_CLOCK";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 178;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "C";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 179;
	TREE_LEVEL = 0;
	CHILDREN = 180, 181, 182, 183;
}

DISPLAY_LINE
{
	CHANNEL = "C[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 180;
	TREE_LEVEL = 1;
	PARENT = 179;
}

DISPLAY_LINE
{
	CHANNEL = "C[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 181;
	TREE_LEVEL = 1;
	PARENT = 179;
}

DISPLAY_LINE
{
	CHANNEL = "C[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 182;
	TREE_LEVEL = 1;
	PARENT = 179;
}

DISPLAY_LINE
{
	CHANNEL = "C[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 183;
	TREE_LEVEL = 1;
	PARENT = 179;
}

DISPLAY_LINE
{
	CHANNEL = "C_ALCR";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 184;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "C_CLOCK";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 185;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "WAY";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 186;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "T0";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 187;
	TREE_LEVEL = 0;
	CHILDREN = 188, 189, 190, 191, 192, 193, 194;
}

DISPLAY_LINE
{
	CHANNEL = "T0[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 188;
	TREE_LEVEL = 1;
	PARENT = 187;
}

DISPLAY_LINE
{
	CHANNEL = "T0[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 189;
	TREE_LEVEL = 1;
	PARENT = 187;
}

DISPLAY_LINE
{
	CHANNEL = "T0[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 190;
	TREE_LEVEL = 1;
	PARENT = 187;
}

DISPLAY_LINE
{
	CHANNEL = "T0[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 191;
	TREE_LEVEL = 1;
	PARENT = 187;
}

DISPLAY_LINE
{
	CHANNEL = "T0[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 192;
	TREE_LEVEL = 1;
	PARENT = 187;
}

DISPLAY_LINE
{
	CHANNEL = "T0[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 193;
	TREE_LEVEL = 1;
	PARENT = 187;
}

DISPLAY_LINE
{
	CHANNEL = "T0[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 194;
	TREE_LEVEL = 1;
	PARENT = 187;
}

DISPLAY_LINE
{
	CHANNEL = "T1";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 195;
	TREE_LEVEL = 0;
	CHILDREN = 196, 197, 198, 199, 200, 201, 202;
}

DISPLAY_LINE
{
	CHANNEL = "T1[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 196;
	TREE_LEVEL = 1;
	PARENT = 195;
}

DISPLAY_LINE
{
	CHANNEL = "T1[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 197;
	TREE_LEVEL = 1;
	PARENT = 195;
}

DISPLAY_LINE
{
	CHANNEL = "T1[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 198;
	TREE_LEVEL = 1;
	PARENT = 195;
}

DISPLAY_LINE
{
	CHANNEL = "T1[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 199;
	TREE_LEVEL = 1;
	PARENT = 195;
}

DISPLAY_LINE
{
	CHANNEL = "T1[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 200;
	TREE_LEVEL = 1;
	PARENT = 195;
}

DISPLAY_LINE
{
	CHANNEL = "T1[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 201;
	TREE_LEVEL = 1;
	PARENT = 195;
}

DISPLAY_LINE
{
	CHANNEL = "T1[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 202;
	TREE_LEVEL = 1;
	PARENT = 195;
}

DISPLAY_LINE
{
	CHANNEL = "T2";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 203;
	TREE_LEVEL = 0;
	CHILDREN = 204, 205, 206, 207, 208, 209, 210;
}

DISPLAY_LINE
{
	CHANNEL = "T2[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 204;
	TREE_LEVEL = 1;
	PARENT = 203;
}

DISPLAY_LINE
{
	CHANNEL = "T2[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 205;
	TREE_LEVEL = 1;
	PARENT = 203;
}

DISPLAY_LINE
{
	CHANNEL = "T2[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 206;
	TREE_LEVEL = 1;
	PARENT = 203;
}

DISPLAY_LINE
{
	CHANNEL = "T2[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 207;
	TREE_LEVEL = 1;
	PARENT = 203;
}

DISPLAY_LINE
{
	CHANNEL = "T2[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 208;
	TREE_LEVEL = 1;
	PARENT = 203;
}

DISPLAY_LINE
{
	CHANNEL = "T2[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 209;
	TREE_LEVEL = 1;
	PARENT = 203;
}

DISPLAY_LINE
{
	CHANNEL = "T2[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 210;
	TREE_LEVEL = 1;
	PARENT = 203;
}

DISPLAY_LINE
{
	CHANNEL = "T3";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 211;
	TREE_LEVEL = 0;
	CHILDREN = 212, 213, 214, 215, 216, 217, 218;
}

DISPLAY_LINE
{
	CHANNEL = "T3[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 212;
	TREE_LEVEL = 1;
	PARENT = 211;
}

DISPLAY_LINE
{
	CHANNEL = "T3[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 213;
	TREE_LEVEL = 1;
	PARENT = 211;
}

DISPLAY_LINE
{
	CHANNEL = "T3[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 214;
	TREE_LEVEL = 1;
	PARENT = 211;
}

DISPLAY_LINE
{
	CHANNEL = "T3[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 215;
	TREE_LEVEL = 1;
	PARENT = 211;
}

DISPLAY_LINE
{
	CHANNEL = "T3[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 216;
	TREE_LEVEL = 1;
	PARENT = 211;
}

DISPLAY_LINE
{
	CHANNEL = "T3[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 217;
	TREE_LEVEL = 1;
	PARENT = 211;
}

DISPLAY_LINE
{
	CHANNEL = "T3[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 218;
	TREE_LEVEL = 1;
	PARENT = 211;
}

DISPLAY_LINE
{
	CHANNEL = "FIX_FLAG";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 219;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "DATA_REG_GLOB_OUT";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 220;
	TREE_LEVEL = 0;
	CHILDREN = 221, 222, 223, 224, 225, 226, 227, 228;
}

DISPLAY_LINE
{
	CHANNEL = "DATA_REG_GLOB_OUT[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 221;
	TREE_LEVEL = 1;
	PARENT = 220;
}

DISPLAY_LINE
{
	CHANNEL = "DATA_REG_GLOB_OUT[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 222;
	TREE_LEVEL = 1;
	PARENT = 220;
}

DISPLAY_LINE
{
	CHANNEL = "DATA_REG_GLOB_OUT[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 223;
	TREE_LEVEL = 1;
	PARENT = 220;
}

DISPLAY_LINE
{
	CHANNEL = "DATA_REG_GLOB_OUT[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 224;
	TREE_LEVEL = 1;
	PARENT = 220;
}

DISPLAY_LINE
{
	CHANNEL = "DATA_REG_GLOB_OUT[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 225;
	TREE_LEVEL = 1;
	PARENT = 220;
}

DISPLAY_LINE
{
	CHANNEL = "DATA_REG_GLOB_OUT[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 226;
	TREE_LEVEL = 1;
	PARENT = 220;
}

DISPLAY_LINE
{
	CHANNEL = "DATA_REG_GLOB_OUT[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 227;
	TREE_LEVEL = 1;
	PARENT = 220;
}

DISPLAY_LINE
{
	CHANNEL = "DATA_REG_GLOB_OUT[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 228;
	TREE_LEVEL = 1;
	PARENT = 220;
}

DISPLAY_LINE
{
	CHANNEL = "EN_OUT_MEM";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 229;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "EN_OUT_REG";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 230;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "IP_UP_SPEC_OUT";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 231;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "MISS_FIX";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 232;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "qq";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 233;
	TREE_LEVEL = 0;
	CHILDREN = 234, 235;
}

DISPLAY_LINE
{
	CHANNEL = "qq[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 234;
	TREE_LEVEL = 1;
	PARENT = 233;
}

DISPLAY_LINE
{
	CHANNEL = "qq[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 235;
	TREE_LEVEL = 1;
	PARENT = 233;
}

DISPLAY_LINE
{
	CHANNEL = "ROM_MEM_OUT";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 236;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "SELECT_REG_GLOB_OUT";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 237;
	TREE_LEVEL = 0;
	CHILDREN = 238, 239, 240, 241, 242;
}

DISPLAY_LINE
{
	CHANNEL = "SELECT_REG_GLOB_OUT[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 238;
	TREE_LEVEL = 1;
	PARENT = 237;
}

DISPLAY_LINE
{
	CHANNEL = "SELECT_REG_GLOB_OUT[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 239;
	TREE_LEVEL = 1;
	PARENT = 237;
}

DISPLAY_LINE
{
	CHANNEL = "SELECT_REG_GLOB_OUT[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 240;
	TREE_LEVEL = 1;
	PARENT = 237;
}

DISPLAY_LINE
{
	CHANNEL = "SELECT_REG_GLOB_OUT[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 241;
	TREE_LEVEL = 1;
	PARENT = 237;
}

DISPLAY_LINE
{
	CHANNEL = "SELECT_REG_GLOB_OUT[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 242;
	TREE_LEVEL = 1;
	PARENT = 237;
}

DISPLAY_LINE
{
	CHANNEL = "STOP_OUT";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 243;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "TAG_FIX";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 244;
	TREE_LEVEL = 0;
	CHILDREN = 245, 246, 247, 248, 249, 250, 251;
}

DISPLAY_LINE
{
	CHANNEL = "TAG_FIX[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 245;
	TREE_LEVEL = 1;
	PARENT = 244;
}

DISPLAY_LINE
{
	CHANNEL = "TAG_FIX[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 246;
	TREE_LEVEL = 1;
	PARENT = 244;
}

DISPLAY_LINE
{
	CHANNEL = "TAG_FIX[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 247;
	TREE_LEVEL = 1;
	PARENT = 244;
}

DISPLAY_LINE
{
	CHANNEL = "TAG_FIX[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 248;
	TREE_LEVEL = 1;
	PARENT = 244;
}

DISPLAY_LINE
{
	CHANNEL = "TAG_FIX[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 249;
	TREE_LEVEL = 1;
	PARENT = 244;
}

DISPLAY_LINE
{
	CHANNEL = "TAG_FIX[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 250;
	TREE_LEVEL = 1;
	PARENT = 244;
}

DISPLAY_LINE
{
	CHANNEL = "TAG_FIX[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 251;
	TREE_LEVEL = 1;
	PARENT = 244;
}

DISPLAY_LINE
{
	CHANNEL = "WRITE_ON_GLOB_OUT";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 252;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 253;
	TREE_LEVEL = 0;
	CHILDREN = 254, 255, 256, 257, 258, 259, 260, 261, 262, 263, 264, 265;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[11]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 254;
	TREE_LEVEL = 1;
	PARENT = 253;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[10]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 255;
	TREE_LEVEL = 1;
	PARENT = 253;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[9]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 256;
	TREE_LEVEL = 1;
	PARENT = 253;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[8]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 257;
	TREE_LEVEL = 1;
	PARENT = 253;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 258;
	TREE_LEVEL = 1;
	PARENT = 253;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 259;
	TREE_LEVEL = 1;
	PARENT = 253;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 260;
	TREE_LEVEL = 1;
	PARENT = 253;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 261;
	TREE_LEVEL = 1;
	PARENT = 253;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 262;
	TREE_LEVEL = 1;
	PARENT = 253;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 263;
	TREE_LEVEL = 1;
	PARENT = 253;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 264;
	TREE_LEVEL = 1;
	PARENT = 253;
}

DISPLAY_LINE
{
	CHANNEL = "ADDR[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 265;
	TREE_LEVEL = 1;
	PARENT = 253;
}

DISPLAY_LINE
{
	CHANNEL = "DATA";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 266;
	TREE_LEVEL = 0;
	CHILDREN = 267, 268, 269, 270, 271, 272, 273, 274;
}

DISPLAY_LINE
{
	CHANNEL = "DATA[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 267;
	TREE_LEVEL = 1;
	PARENT = 266;
}

DISPLAY_LINE
{
	CHANNEL = "DATA[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 268;
	TREE_LEVEL = 1;
	PARENT = 266;
}

DISPLAY_LINE
{
	CHANNEL = "DATA[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 269;
	TREE_LEVEL = 1;
	PARENT = 266;
}

DISPLAY_LINE
{
	CHANNEL = "DATA[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 270;
	TREE_LEVEL = 1;
	PARENT = 266;
}

DISPLAY_LINE
{
	CHANNEL = "DATA[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 271;
	TREE_LEVEL = 1;
	PARENT = 266;
}

DISPLAY_LINE
{
	CHANNEL = "DATA[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 272;
	TREE_LEVEL = 1;
	PARENT = 266;
}

DISPLAY_LINE
{
	CHANNEL = "DATA[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 273;
	TREE_LEVEL = 1;
	PARENT = 266;
}

DISPLAY_LINE
{
	CHANNEL = "DATA[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 274;
	TREE_LEVEL = 1;
	PARENT = 266;
}

DISPLAY_LINE
{
	CHANNEL = "DELAY_ITERATION";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 275;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "FLAGS";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 276;
	TREE_LEVEL = 0;
	CHILDREN = 277, 278, 279, 280;
}

DISPLAY_LINE
{
	CHANNEL = "FLAGS[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 277;
	TREE_LEVEL = 1;
	PARENT = 276;
}

DISPLAY_LINE
{
	CHANNEL = "FLAGS[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 278;
	TREE_LEVEL = 1;
	PARENT = 276;
}

DISPLAY_LINE
{
	CHANNEL = "FLAGS[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 279;
	TREE_LEVEL = 1;
	PARENT = 276;
}

DISPLAY_LINE
{
	CHANNEL = "FLAGS[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 280;
	TREE_LEVEL = 1;
	PARENT = 276;
}

TIME_BAR
{
	TIME = 0;
	MASTER = TRUE;
}

TIME_BAR
{
	TIME = 0;
	MASTER = TRUE;
}

TIME_BAR
{
	TIME = 0;
	MASTER = TRUE;
}
;
