-- megafunction wizard: %LPM_ADD_SUB%
-- GENERATION: STANDARD
-- VERSION: WM1.0
-- MODULE: lpm_add_sub 

-- ============================================================
-- File Name: lpm_add_sub4.tdf
-- Megafunction Name(s):
-- 			lpm_add_sub
--
-- Simulation Library Files(s):
-- 			lpm
-- ============================================================
-- ************************************************************
-- THIS IS A WIZARD-GENERATED FILE. DO NOT EDIT THIS FILE!
--
-- 9.1 Build 222 10/21/2009 SJ Web Edition
-- ************************************************************


--Copyright (C) 1991-2009 Altera Corporation
--Your use of Altera Corporation's design tools, logic functions 
--and other software and tools, and its AMPP partner logic 
--functions, and any output files from any of the foregoing 
--(including device programming or simulation files), and any 
--associated documentation or information are expressly subject 
--to the terms and conditions of the Altera Program License 
--Subscription Agreement, Altera MegaCore Function License 
--Agreement, or other applicable license agreement, including, 
--without limitation, that your use is for the sole purpose of 
--programming logic devices manufactured by Altera and sold by 
--Altera or its authorized distributors.  Please refer to the 
--applicable agreement for further details.

INCLUDE "lpm_add_sub.inc";



SUBDESIGN lpm_add_sub4
(
	datab[7..0]	 : INPUT;
	result[7..0]	 : OUTPUT;
)

VARIABLE

	lpm_add_sub_component : lpm_add_sub WITH (
			LPM_DIRECTION = "SUB",
			LPM_HINT = "ONE_INPUT_IS_CONSTANT=YES,CIN_USED=NO",
			LPM_REPRESENTATION = "UNSIGNED",
			LPM_TYPE = "LPM_ADD_SUB",
			LPM_WIDTH = 8
			);

BEGIN

	result[7..0] = lpm_add_sub_component.result[7..0];
	lpm_add_sub_component.dataa[7..0] = 11;
	lpm_add_sub_component.datab[7..0] = datab[7..0];
END;



-- ============================================================
-- CNX file retrieval info
-- ============================================================
-- Retrieval info: PRIVATE: CarryIn NUMERIC "0"
-- Retrieval info: PRIVATE: CarryOut NUMERIC "0"
-- Retrieval info: PRIVATE: ConstantA NUMERIC "11"
-- Retrieval info: PRIVATE: ConstantB NUMERIC "0"
-- Retrieval info: PRIVATE: Function NUMERIC "1"
-- Retrieval info: PRIVATE: INTENDED_DEVICE_FAMILY STRING "Cyclone"
-- Retrieval info: PRIVATE: LPM_PIPELINE NUMERIC "0"
-- Retrieval info: PRIVATE: Latency NUMERIC "0"
-- Retrieval info: PRIVATE: Overflow NUMERIC "0"
-- Retrieval info: PRIVATE: RadixA NUMERIC "10"
-- Retrieval info: PRIVATE: RadixB NUMERIC "10"
-- Retrieval info: PRIVATE: Representation NUMERIC "1"
-- Retrieval info: PRIVATE: SYNTH_WRAPPER_GEN_POSTFIX STRING "0"
-- Retrieval info: PRIVATE: ValidCtA NUMERIC "1"
-- Retrieval info: PRIVATE: ValidCtB NUMERIC "0"
-- Retrieval info: PRIVATE: WhichConstant NUMERIC "1"
-- Retrieval info: PRIVATE: aclr NUMERIC "0"
-- Retrieval info: PRIVATE: clken NUMERIC "0"
-- Retrieval info: PRIVATE: nBit NUMERIC "8"
-- Retrieval info: CONSTANT: LPM_DIRECTION STRING "SUB"
-- Retrieval info: CONSTANT: LPM_HINT STRING "ONE_INPUT_IS_CONSTANT=YES,CIN_USED=NO"
-- Retrieval info: CONSTANT: LPM_REPRESENTATION STRING "UNSIGNED"
-- Retrieval info: CONSTANT: LPM_TYPE STRING "LPM_ADD_SUB"
-- Retrieval info: CONSTANT: LPM_WIDTH NUMERIC "8"
-- Retrieval info: USED_PORT: datab 0 0 8 0 INPUT NODEFVAL datab[7..0]
-- Retrieval info: USED_PORT: result 0 0 8 0 OUTPUT NODEFVAL result[7..0]
-- Retrieval info: CONNECT: result 0 0 8 0 @result 0 0 8 0
-- Retrieval info: CONNECT: @dataa 0 0 8 0 11 0 0 0 0
-- Retrieval info: CONNECT: @datab 0 0 8 0 datab 0 0 8 0
-- Retrieval info: LIBRARY: lpm lpm.lpm_components.all
-- Retrieval info: GEN_FILE: TYPE_NORMAL lpm_add_sub4.tdf TRUE
-- Retrieval info: GEN_FILE: TYPE_NORMAL lpm_add_sub4.inc FALSE
-- Retrieval info: GEN_FILE: TYPE_NORMAL lpm_add_sub4.cmp TRUE
-- Retrieval info: GEN_FILE: TYPE_NORMAL lpm_add_sub4.bsf TRUE FALSE
-- Retrieval info: GEN_FILE: TYPE_NORMAL lpm_add_sub4_inst.tdf FALSE
-- Retrieval info: GEN_FILE: TYPE_NORMAL lpm_add_sub4_waveforms.html TRUE
-- Retrieval info: GEN_FILE: TYPE_NORMAL lpm_add_sub4_wave*.jpg FALSE
-- Retrieval info: LIB_FILE: lpm
