/*
WARNING: Do NOT edit the input and output ports in this file in a text
editor if you plan to continue editing the block that represents it in
the Block Editor! File corruption is VERY likely to occur.
*/
/*
Copyright (C) 1991-2009 Altera Corporation
Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and its AMPP partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, Altera MegaCore Function License 
Agreement, or other applicable license agreement, including, 
without limitation, that your use is for the sole purpose of 
programming logic devices manufactured by Altera and sold by 
Altera or its authorized distributors.  Please refer to the 
applicable agreement for further details.
*/
(header "symbol" (version "1.1"))
(symbol
	(rect 16 16 216 144)
	(text "DMA_BLOCK" (rect 5 0 80 14)(font "Arial" (font_size 8)))
	(text "inst" (rect 8 112 25 124)(font "Arial" ))
	(port
		(pt 0 32)
		(input)
		(text "IN_BYTE[2..0]" (rect 0 0 77 14)(font "Arial" (font_size 8)))
		(text "IN_BYTE[2..0]" (rect 21 27 98 41)(font "Arial" (font_size 8)))
		(line (pt 0 32)(pt 16 32)(line_width 3))
	)
	(port
		(pt 0 48)
		(input)
		(text "IN_CLOCK" (rect 0 0 59 14)(font "Arial" (font_size 8)))
		(text "IN_CLOCK" (rect 21 43 80 57)(font "Arial" (font_size 8)))
		(line (pt 0 48)(pt 16 48)(line_width 1))
	)
	(port
		(pt 0 64)
		(input)
		(text "IN_WRITE" (rect 0 0 54 14)(font "Arial" (font_size 8)))
		(text "IN_WRITE" (rect 21 59 75 73)(font "Arial" (font_size 8)))
		(line (pt 0 64)(pt 16 64)(line_width 1))
	)
	(port
		(pt 200 32)
		(output)
		(text "ADDR[11..0]" (rect 0 0 69 14)(font "Arial" (font_size 8)))
		(text "ADDR[11..0]" (rect 110 27 179 41)(font "Arial" (font_size 8)))
		(line (pt 200 32)(pt 184 32)(line_width 3))
	)
	(port
		(pt 200 48)
		(output)
		(text "CLOCK" (rect 0 0 41 14)(font "Arial" (font_size 8)))
		(text "CLOCK" (rect 138 43 179 57)(font "Arial" (font_size 8)))
		(line (pt 200 48)(pt 184 48)(line_width 1))
	)
	(port
		(pt 200 64)
		(output)
		(text "W" (rect 0 0 11 14)(font "Arial" (font_size 8)))
		(text "W" (rect 168 59 179 73)(font "Arial" (font_size 8)))
		(line (pt 200 64)(pt 184 64)(line_width 1))
	)
	(port
		(pt 200 80)
		(bidir)
		(text "DATA[7..0]" (rect 0 0 62 14)(font "Arial" (font_size 8)))
		(text "DATA[7..0]" (rect 117 75 179 89)(font "Arial" (font_size 8)))
		(line (pt 200 80)(pt 184 80)(line_width 3))
	)
	(drawing
		(rectangle (rect 16 16 184 112)(line_width 1))
	)
)
