Analysis & Synthesis report for JMPER
Wed Nov 06 15:13:20 2013
Quartus II Version 9.1 Build 222 10/21/2009 SJ Web Edition


---------------------
; Table of Contents ;
---------------------
  1. Legal Notice
  2. Analysis & Synthesis Summary
  3. Analysis & Synthesis Settings
  4. Parallel Compilation
  5. Analysis & Synthesis Source Files Read
  6. Analysis & Synthesis Resource Usage Summary
  7. Analysis & Synthesis Resource Utilization by Entity
  8. Analysis & Synthesis RAM Summary
  9. Logic Cells Representing Combinational Loops
 10. General Register Statistics
 11. Source assignments for A1_BLOCK:inst|LPM_RAM_IO:inst1|altram:sram|altsyncram:ram_block|altsyncram_a791:auto_generated
 12. Source assignments for CONTROL_BLOCK:inst2|lpm_counter0:inst|lpm_counter:lpm_counter_component
 13. Source assignments for CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component
 14. Source assignments for CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component|cntr_6li:auto_generated
 15. Source assignments for A2_BLOCK:inst1|LPM_RAM_IO:inst17|altram:sram|altsyncram:ram_block|altsyncram_e791:auto_generated
 16. Source assignments for SELECTOR_BLOCK:inst4|lpm_counter2:inst41|lpm_counter:lpm_counter_component
 17. Source assignments for SELECTOR_BLOCK:inst4|lpm_counter2:inst42|lpm_counter:lpm_counter_component
 18. Source assignments for SELECTOR_BLOCK:inst4|lpm_counter2:inst43|lpm_counter:lpm_counter_component
 19. Source assignments for SELECTOR_BLOCK:inst4|lpm_counter2:inst45|lpm_counter:lpm_counter_component
 20. Parameter Settings for User Entity Instance: A1_BLOCK:inst|LPM_RAM_IO:inst1
 21. Parameter Settings for User Entity Instance: CONTROL_BLOCK:inst2|lpm_decode0:inst1|lpm_decode:lpm_decode_component
 22. Parameter Settings for User Entity Instance: CONTROL_BLOCK:inst2|lpm_counter0:inst|lpm_counter:lpm_counter_component
 23. Parameter Settings for User Entity Instance: CONTROL_BLOCK:inst2|lpm_shiftreg0:inst3|lpm_shiftreg:lpm_shiftreg_component
 24. Parameter Settings for User Entity Instance: CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component
 25. Parameter Settings for User Entity Instance: A2_BLOCK:inst1|LPM_RAM_IO:inst17
 26. Parameter Settings for User Entity Instance: SELECTOR_BLOCK:inst4|BUSMUX:inst38
 27. Parameter Settings for User Entity Instance: SELECTOR_BLOCK:inst4|lpm_compare0:inst39|lpm_compare:lpm_compare_component
 28. Parameter Settings for User Entity Instance: SELECTOR_BLOCK:inst4|lpm_shiftreg0:inst3|lpm_shiftreg:lpm_shiftreg_component
 29. Parameter Settings for User Entity Instance: SELECTOR_BLOCK:inst4|lpm_shiftreg0:inst4|lpm_shiftreg:lpm_shiftreg_component
 30. Parameter Settings for User Entity Instance: SELECTOR_BLOCK:inst4|lpm_counter2:inst41|lpm_counter:lpm_counter_component
 31. Parameter Settings for User Entity Instance: SELECTOR_BLOCK:inst4|lpm_counter2:inst42|lpm_counter:lpm_counter_component
 32. Parameter Settings for User Entity Instance: SELECTOR_BLOCK:inst4|lpm_counter2:inst43|lpm_counter:lpm_counter_component
 33. Parameter Settings for User Entity Instance: SELECTOR_BLOCK:inst4|lpm_counter2:inst45|lpm_counter:lpm_counter_component
 34. lpm_shiftreg Parameter Settings by Entity Instance
 35. Analysis & Synthesis Messages



----------------
; Legal Notice ;
----------------
Copyright (C) 1991-2009 Altera Corporation
Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and its AMPP partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, Altera MegaCore Function License 
Agreement, or other applicable license agreement, including, 
without limitation, that your use is for the sole purpose of 
programming logic devices manufactured by Altera and sold by 
Altera or its authorized distributors.  Please refer to the 
applicable agreement for further details.



+------------------------------------------------------------------------------+
; Analysis & Synthesis Summary                                                 ;
+------------------------------------+-----------------------------------------+
; Analysis & Synthesis Status        ; Successful - Wed Nov 06 15:13:19 2013   ;
; Quartus II Version                 ; 9.1 Build 222 10/21/2009 SJ Web Edition ;
; Revision Name                      ; JMPER                                   ;
; Top-level Entity Name              ; MAIN_MODULE                             ;
; Family                             ; Cyclone II                              ;
; Total logic elements               ; 253                                     ;
;     Total combinational functions  ; 206                                     ;
;     Dedicated logic registers      ; 108                                     ;
; Total registers                    ; 108                                     ;
; Total pins                         ; 128                                     ;
; Total virtual pins                 ; 0                                       ;
; Total memory bits                  ; 1,280                                   ;
; Embedded Multiplier 9-bit elements ; 0                                       ;
; Total PLLs                         ; 0                                       ;
+------------------------------------+-----------------------------------------+


+----------------------------------------------------------------------------------------------------------------------+
; Analysis & Synthesis Settings                                                                                        ;
+----------------------------------------------------------------------------+--------------------+--------------------+
; Option                                                                     ; Setting            ; Default Value      ;
+----------------------------------------------------------------------------+--------------------+--------------------+
; Top-level entity name                                                      ; MAIN_MODULE        ; JMPER              ;
; Family name                                                                ; Cyclone II         ; Stratix II         ;
; Use Generated Physical Constraints File                                    ; Off                ;                    ;
; Use smart compilation                                                      ; Off                ; Off                ;
; Enable parallel Assembler and TimeQuest Timing Analyzer during compilation ; On                 ; On                 ;
; Enable compact report table                                                ; Off                ; Off                ;
; Restructure Multiplexers                                                   ; Auto               ; Auto               ;
; Create Debugging Nodes for IP Cores                                        ; Off                ; Off                ;
; Preserve fewer node names                                                  ; On                 ; On                 ;
; Disable OpenCore Plus hardware evaluation                                  ; Off                ; Off                ;
; Verilog Version                                                            ; Verilog_2001       ; Verilog_2001       ;
; VHDL Version                                                               ; VHDL_1993          ; VHDL_1993          ;
; State Machine Processing                                                   ; Auto               ; Auto               ;
; Safe State Machine                                                         ; Off                ; Off                ;
; Extract Verilog State Machines                                             ; On                 ; On                 ;
; Extract VHDL State Machines                                                ; On                 ; On                 ;
; Ignore Verilog initial constructs                                          ; Off                ; Off                ;
; Iteration limit for constant Verilog loops                                 ; 5000               ; 5000               ;
; Iteration limit for non-constant Verilog loops                             ; 250                ; 250                ;
; Add Pass-Through Logic to Inferred RAMs                                    ; On                 ; On                 ;
; Parallel Synthesis                                                         ; On                 ; On                 ;
; DSP Block Balancing                                                        ; Auto               ; Auto               ;
; NOT Gate Push-Back                                                         ; On                 ; On                 ;
; Power-Up Don't Care                                                        ; On                 ; On                 ;
; Remove Redundant Logic Cells                                               ; Off                ; Off                ;
; Remove Duplicate Registers                                                 ; On                 ; On                 ;
; Ignore CARRY Buffers                                                       ; Off                ; Off                ;
; Ignore CASCADE Buffers                                                     ; Off                ; Off                ;
; Ignore GLOBAL Buffers                                                      ; Off                ; Off                ;
; Ignore ROW GLOBAL Buffers                                                  ; Off                ; Off                ;
; Ignore LCELL Buffers                                                       ; Off                ; Off                ;
; Ignore SOFT Buffers                                                        ; On                 ; On                 ;
; Limit AHDL Integers to 32 Bits                                             ; Off                ; Off                ;
; Optimization Technique                                                     ; Balanced           ; Balanced           ;
; Carry Chain Length                                                         ; 70                 ; 70                 ;
; Auto Carry Chains                                                          ; On                 ; On                 ;
; Auto Open-Drain Pins                                                       ; On                 ; On                 ;
; Perform WYSIWYG Primitive Resynthesis                                      ; Off                ; Off                ;
; Auto ROM Replacement                                                       ; On                 ; On                 ;
; Auto RAM Replacement                                                       ; On                 ; On                 ;
; Auto Shift Register Replacement                                            ; Auto               ; Auto               ;
; Auto Clock Enable Replacement                                              ; On                 ; On                 ;
; Strict RAM Replacement                                                     ; Off                ; Off                ;
; Allow Synchronous Control Signals                                          ; On                 ; On                 ;
; Force Use of Synchronous Clear Signals                                     ; Off                ; Off                ;
; Auto RAM to Logic Cell Conversion                                          ; Off                ; Off                ;
; Auto Resource Sharing                                                      ; Off                ; Off                ;
; Allow Any RAM Size For Recognition                                         ; Off                ; Off                ;
; Allow Any ROM Size For Recognition                                         ; Off                ; Off                ;
; Allow Any Shift Register Size For Recognition                              ; Off                ; Off                ;
; Use LogicLock Constraints during Resource Balancing                        ; On                 ; On                 ;
; Ignore translate_off and synthesis_off directives                          ; Off                ; Off                ;
; Timing-Driven Synthesis                                                    ; Off                ; Off                ;
; Show Parameter Settings Tables in Synthesis Report                         ; On                 ; On                 ;
; Ignore Maximum Fan-Out Assignments                                         ; Off                ; Off                ;
; Synchronization Register Chain Length                                      ; 2                  ; 2                  ;
; PowerPlay Power Optimization                                               ; Normal compilation ; Normal compilation ;
; HDL message level                                                          ; Level2             ; Level2             ;
; Suppress Register Optimization Related Messages                            ; Off                ; Off                ;
; Number of Removed Registers Reported in Synthesis Report                   ; 100                ; 100                ;
; Number of Inverted Registers Reported in Synthesis Report                  ; 100                ; 100                ;
; Clock MUX Protection                                                       ; On                 ; On                 ;
; Auto Gated Clock Conversion                                                ; Off                ; Off                ;
; Block Design Naming                                                        ; Auto               ; Auto               ;
; SDC constraint protection                                                  ; Off                ; Off                ;
; Synthesis Effort                                                           ; Auto               ; Auto               ;
; Shift Register Replacement - Allow Asynchronous Clear Signal               ; On                 ; On                 ;
; Analysis & Synthesis Message Level                                         ; Medium             ; Medium             ;
; Disable Register Merging Across Hierarchies                                ; Auto               ; Auto               ;
; Resource Aware Inference For Block RAM                                     ; On                 ; On                 ;
+----------------------------------------------------------------------------+--------------------+--------------------+


Parallel compilation was disabled, but you have multiple processors available. Enable parallel compilation to reduce compilation time.
+-------------------------------------+
; Parallel Compilation                ;
+----------------------------+--------+
; Processors                 ; Number ;
+----------------------------+--------+
; Number detected on machine ; 2      ;
; Maximum allowed            ; 1      ;
+----------------------------+--------+


+------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Analysis & Synthesis Source Files Read                                                                                                                     ;
+----------------------------------+-----------------+---------------------------------------+---------------------------------------------------------------+
; File Name with User-Entered Path ; Used in Netlist ; File Type                             ; File Name with Absolute Path                                  ;
+----------------------------------+-----------------+---------------------------------------+---------------------------------------------------------------+
; MAIN_MODULE.bdf                  ; yes             ; User Block Diagram/Schematic File     ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/MAIN_MODULE.bdf            ;
; SELECTOR_BLOCK.bdf               ; yes             ; User Block Diagram/Schematic File     ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/SELECTOR_BLOCK.bdf         ;
; CONTROL_BLOCK.bdf                ; yes             ; User Block Diagram/Schematic File     ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/CONTROL_BLOCK.bdf          ;
; A1_BLOCK.bdf                     ; yes             ; User Block Diagram/Schematic File     ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/A1_BLOCK.bdf               ;
; A2_BLOCK.bdf                     ; yes             ; User Block Diagram/Schematic File     ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/A2_BLOCK.bdf               ;
; A1.hex                           ; yes             ; User Hexadecimal (Intel-Format) File  ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/A1.hex                     ;
; A2.hex                           ; yes             ; User Hexadecimal (Intel-Format) File  ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/A2.hex                     ;
; COUNTER_BLOCK.vhd                ; yes             ; User VHDL File                        ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/COUNTER_BLOCK.vhd          ;
; DOWN_BLOCK.vhd                   ; yes             ; User VHDL File                        ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/DOWN_BLOCK.vhd             ;
; lpm_counter0.vhd                 ; yes             ; User Wizard-Generated File            ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/lpm_counter0.vhd           ;
; lpm_decode0.vhd                  ; yes             ; User Wizard-Generated File            ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/lpm_decode0.vhd            ;
; lpm_shiftreg0.vhd                ; yes             ; User Wizard-Generated File            ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/lpm_shiftreg0.vhd          ;
; lpm_compare0.vhd                 ; yes             ; User Wizard-Generated File            ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/lpm_compare0.vhd           ;
; lpm_counter2.vhd                 ; yes             ; User Wizard-Generated File            ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/lpm_counter2.vhd           ;
; lpm_counter3.vhd                 ; yes             ; User Wizard-Generated File            ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/lpm_counter3.vhd           ;
; lpm_ram_io.tdf                   ; yes             ; Megafunction                          ; c:/altera/91/quartus/libraries/megafunctions/lpm_ram_io.tdf   ;
; altram.tdf                       ; yes             ; Megafunction                          ; c:/altera/91/quartus/libraries/megafunctions/altram.tdf       ;
; altsyncram.tdf                   ; yes             ; Megafunction                          ; c:/altera/91/quartus/libraries/megafunctions/altsyncram.tdf   ;
; db/altsyncram_a791.tdf           ; yes             ; Auto-Generated Megafunction           ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/db/altsyncram_a791.tdf     ;
; lpm_decode.tdf                   ; yes             ; Megafunction                          ; c:/altera/91/quartus/libraries/megafunctions/lpm_decode.tdf   ;
; db/decode_s6f.tdf                ; yes             ; Auto-Generated Megafunction           ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/db/decode_s6f.tdf          ;
; lpm_counter.tdf                  ; yes             ; Megafunction                          ; c:/altera/91/quartus/libraries/megafunctions/lpm_counter.tdf  ;
; db/cntr_p2i.tdf                  ; yes             ; Auto-Generated Megafunction           ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/db/cntr_p2i.tdf            ;
; lpm_shiftreg.tdf                 ; yes             ; Megafunction                          ; c:/altera/91/quartus/libraries/megafunctions/lpm_shiftreg.tdf ;
; db/cntr_6li.tdf                  ; yes             ; Auto-Generated Megafunction           ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/db/cntr_6li.tdf            ;
; db/altsyncram_e791.tdf           ; yes             ; Auto-Generated Megafunction           ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/db/altsyncram_e791.tdf     ;
; busmux.tdf                       ; yes             ; Megafunction                          ; c:/altera/91/quartus/libraries/megafunctions/busmux.tdf       ;
; lpm_mux.tdf                      ; yes             ; Megafunction                          ; c:/altera/91/quartus/libraries/megafunctions/lpm_mux.tdf      ;
; db/mux_lmc.tdf                   ; yes             ; Auto-Generated Megafunction           ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/db/mux_lmc.tdf             ;
; lpm_compare.tdf                  ; yes             ; Megafunction                          ; c:/altera/91/quartus/libraries/megafunctions/lpm_compare.tdf  ;
; db/cmpr_bhg.tdf                  ; yes             ; Auto-Generated Megafunction           ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/db/cmpr_bhg.tdf            ;
; db/cntr_skh.tdf                  ; yes             ; Auto-Generated Megafunction           ; F:/UNIVER/4_1/SIFO/LAB/LAB10/LAB10/db/cntr_skh.tdf            ;
+----------------------------------+-----------------+---------------------------------------+---------------------------------------------------------------+


+--------------------------------------------------------------------------+
; Analysis & Synthesis Resource Usage Summary                              ;
+---------------------------------------------+----------------------------+
; Resource                                    ; Usage                      ;
+---------------------------------------------+----------------------------+
; Estimated Total logic elements              ; 253                        ;
;                                             ;                            ;
; Total combinational functions               ; 206                        ;
; Logic element usage by number of LUT inputs ;                            ;
;     -- 4 input functions                    ; 94                         ;
;     -- 3 input functions                    ; 49                         ;
;     -- <=2 input functions                  ; 63                         ;
;                                             ;                            ;
; Logic elements by mode                      ;                            ;
;     -- normal mode                          ; 143                        ;
;     -- arithmetic mode                      ; 63                         ;
;                                             ;                            ;
; Total registers                             ; 108                        ;
;     -- Dedicated logic registers            ; 108                        ;
;     -- I/O registers                        ; 0                          ;
;                                             ;                            ;
; I/O pins                                    ; 128                        ;
; Total memory bits                           ; 1280                       ;
; Maximum fan-out node                        ; SELECTOR_BLOCK:inst4|inst8 ;
; Maximum fan-out                             ; 43                         ;
; Total fan-out                               ; 1038                       ;
; Average fan-out                             ; 2.32                       ;
+---------------------------------------------+----------------------------+


+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Analysis & Synthesis Resource Utilization by Entity                                                                                                                                                                                                                                          ;
+-------------------------------------------------+-------------------+--------------+-------------+--------------+---------+-----------+------+--------------+-----------------------------------------------------------------------------------------------------------------+--------------+
; Compilation Hierarchy Node                      ; LC Combinationals ; LC Registers ; Memory Bits ; DSP Elements ; DSP 9x9 ; DSP 18x18 ; Pins ; Virtual Pins ; Full Hierarchy Name                                                                                             ; Library Name ;
+-------------------------------------------------+-------------------+--------------+-------------+--------------+---------+-----------+------+--------------+-----------------------------------------------------------------------------------------------------------------+--------------+
; |MAIN_MODULE                                    ; 206 (0)           ; 108 (0)      ; 1280        ; 0            ; 0       ; 0         ; 128  ; 0            ; |MAIN_MODULE                                                                                                    ; work         ;
;    |A1_BLOCK:inst|                              ; 5 (5)             ; 0 (0)        ; 256         ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|A1_BLOCK:inst                                                                                      ;              ;
;       |lpm_ram_io:inst1|                        ; 0 (0)             ; 0 (0)        ; 256         ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|A1_BLOCK:inst|lpm_ram_io:inst1                                                                     ; work         ;
;          |altram:sram|                          ; 0 (0)             ; 0 (0)        ; 256         ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|A1_BLOCK:inst|lpm_ram_io:inst1|altram:sram                                                         ; work         ;
;             |altsyncram:ram_block|              ; 0 (0)             ; 0 (0)        ; 256         ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|A1_BLOCK:inst|lpm_ram_io:inst1|altram:sram|altsyncram:ram_block                                    ; work         ;
;                |altsyncram_a791:auto_generated| ; 0 (0)             ; 0 (0)        ; 256         ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|A1_BLOCK:inst|lpm_ram_io:inst1|altram:sram|altsyncram:ram_block|altsyncram_a791:auto_generated     ; work         ;
;    |A2_BLOCK:inst1|                             ; 16 (16)           ; 0 (0)        ; 1024        ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|A2_BLOCK:inst1                                                                                     ; work         ;
;       |lpm_ram_io:inst17|                       ; 0 (0)             ; 0 (0)        ; 1024        ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|A2_BLOCK:inst1|lpm_ram_io:inst17                                                                   ; work         ;
;          |altram:sram|                          ; 0 (0)             ; 0 (0)        ; 1024        ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|A2_BLOCK:inst1|lpm_ram_io:inst17|altram:sram                                                       ; work         ;
;             |altsyncram:ram_block|              ; 0 (0)             ; 0 (0)        ; 1024        ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|A2_BLOCK:inst1|lpm_ram_io:inst17|altram:sram|altsyncram:ram_block                                  ; work         ;
;                |altsyncram_e791:auto_generated| ; 0 (0)             ; 0 (0)        ; 1024        ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|A2_BLOCK:inst1|lpm_ram_io:inst17|altram:sram|altsyncram:ram_block|altsyncram_e791:auto_generated   ; work         ;
;    |CONTROL_BLOCK:inst2|                        ; 64 (2)            ; 36 (0)       ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|CONTROL_BLOCK:inst2                                                                                ; work         ;
;       |DOWN_BLOCK:inst5|                        ; 0 (0)             ; 1 (1)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|CONTROL_BLOCK:inst2|DOWN_BLOCK:inst5                                                               ; work         ;
;       |lpm_counter0:inst|                       ; 3 (0)             ; 3 (0)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|CONTROL_BLOCK:inst2|lpm_counter0:inst                                                              ; work         ;
;          |lpm_counter:lpm_counter_component|    ; 3 (0)             ; 3 (0)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|CONTROL_BLOCK:inst2|lpm_counter0:inst|lpm_counter:lpm_counter_component                            ; work         ;
;             |cntr_p2i:auto_generated|           ; 3 (3)             ; 3 (3)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|CONTROL_BLOCK:inst2|lpm_counter0:inst|lpm_counter:lpm_counter_component|cntr_p2i:auto_generated    ; work         ;
;       |lpm_counter3:inst4|                      ; 57 (0)            ; 16 (0)       ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|CONTROL_BLOCK:inst2|lpm_counter3:inst4                                                             ; work         ;
;          |lpm_counter:lpm_counter_component|    ; 57 (0)            ; 16 (0)       ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component                           ; work         ;
;             |cntr_6li:auto_generated|           ; 57 (57)           ; 16 (16)      ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component|cntr_6li:auto_generated   ; work         ;
;       |lpm_decode0:inst1|                       ; 2 (0)             ; 0 (0)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|CONTROL_BLOCK:inst2|lpm_decode0:inst1                                                              ;              ;
;          |lpm_decode:lpm_decode_component|      ; 2 (0)             ; 0 (0)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|CONTROL_BLOCK:inst2|lpm_decode0:inst1|lpm_decode:lpm_decode_component                              ; work         ;
;             |decode_s6f:auto_generated|         ; 2 (2)             ; 0 (0)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|CONTROL_BLOCK:inst2|lpm_decode0:inst1|lpm_decode:lpm_decode_component|decode_s6f:auto_generated    ; work         ;
;       |lpm_shiftreg0:inst3|                     ; 0 (0)             ; 16 (0)       ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|CONTROL_BLOCK:inst2|lpm_shiftreg0:inst3                                                            ; work         ;
;          |lpm_shiftreg:lpm_shiftreg_component|  ; 0 (0)             ; 16 (16)      ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|CONTROL_BLOCK:inst2|lpm_shiftreg0:inst3|lpm_shiftreg:lpm_shiftreg_component                        ; work         ;
;    |SELECTOR_BLOCK:inst4|                       ; 121 (9)           ; 72 (0)       ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4                                                                               ; work         ;
;       |COUNTER_BLOCK:inst40|                    ; 76 (76)           ; 8 (8)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|COUNTER_BLOCK:inst40                                                          ; work         ;
;       |busmux:inst38|                           ; 1 (0)             ; 0 (0)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|busmux:inst38                                                                 ; work         ;
;          |lpm_mux:$00000|                       ; 1 (0)             ; 0 (0)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|busmux:inst38|lpm_mux:$00000                                                  ;              ;
;             |mux_lmc:auto_generated|            ; 1 (1)             ; 0 (0)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|busmux:inst38|lpm_mux:$00000|mux_lmc:auto_generated                           ;              ;
;       |lpm_compare0:inst39|                     ; 3 (0)             ; 0 (0)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|lpm_compare0:inst39                                                           ;              ;
;          |lpm_compare:lpm_compare_component|    ; 3 (0)             ; 0 (0)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|lpm_compare0:inst39|lpm_compare:lpm_compare_component                         ;              ;
;             |cmpr_bhg:auto_generated|           ; 3 (3)             ; 0 (0)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|lpm_compare0:inst39|lpm_compare:lpm_compare_component|cmpr_bhg:auto_generated ; work         ;
;       |lpm_counter2:inst41|                     ; 8 (0)             ; 8 (0)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|lpm_counter2:inst41                                                           ; work         ;
;          |lpm_counter:lpm_counter_component|    ; 8 (0)             ; 8 (0)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|lpm_counter2:inst41|lpm_counter:lpm_counter_component                         ; work         ;
;             |cntr_skh:auto_generated|           ; 8 (8)             ; 8 (8)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|lpm_counter2:inst41|lpm_counter:lpm_counter_component|cntr_skh:auto_generated ; work         ;
;       |lpm_counter2:inst42|                     ; 8 (0)             ; 8 (0)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|lpm_counter2:inst42                                                           ; work         ;
;          |lpm_counter:lpm_counter_component|    ; 8 (0)             ; 8 (0)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|lpm_counter2:inst42|lpm_counter:lpm_counter_component                         ; work         ;
;             |cntr_skh:auto_generated|           ; 8 (8)             ; 8 (8)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|lpm_counter2:inst42|lpm_counter:lpm_counter_component|cntr_skh:auto_generated ; work         ;
;       |lpm_counter2:inst43|                     ; 8 (0)             ; 8 (0)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|lpm_counter2:inst43                                                           ; work         ;
;          |lpm_counter:lpm_counter_component|    ; 8 (0)             ; 8 (0)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|lpm_counter2:inst43|lpm_counter:lpm_counter_component                         ; work         ;
;             |cntr_skh:auto_generated|           ; 8 (8)             ; 8 (8)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|lpm_counter2:inst43|lpm_counter:lpm_counter_component|cntr_skh:auto_generated ; work         ;
;       |lpm_counter2:inst45|                     ; 8 (0)             ; 8 (0)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|lpm_counter2:inst45                                                           ; work         ;
;          |lpm_counter:lpm_counter_component|    ; 8 (0)             ; 8 (0)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|lpm_counter2:inst45|lpm_counter:lpm_counter_component                         ; work         ;
;             |cntr_skh:auto_generated|           ; 8 (8)             ; 8 (8)        ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|lpm_counter2:inst45|lpm_counter:lpm_counter_component|cntr_skh:auto_generated ; work         ;
;       |lpm_shiftreg0:inst3|                     ; 0 (0)             ; 16 (0)       ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|lpm_shiftreg0:inst3                                                           ; work         ;
;          |lpm_shiftreg:lpm_shiftreg_component|  ; 0 (0)             ; 16 (16)      ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|lpm_shiftreg0:inst3|lpm_shiftreg:lpm_shiftreg_component                       ; work         ;
;       |lpm_shiftreg0:inst4|                     ; 0 (0)             ; 16 (0)       ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|lpm_shiftreg0:inst4                                                           ; work         ;
;          |lpm_shiftreg:lpm_shiftreg_component|  ; 0 (0)             ; 16 (16)      ; 0           ; 0            ; 0       ; 0         ; 0    ; 0            ; |MAIN_MODULE|SELECTOR_BLOCK:inst4|lpm_shiftreg0:inst4|lpm_shiftreg:lpm_shiftreg_component                       ; work         ;
+-------------------------------------------------+-------------------+--------------+-------------+--------------+---------+-----------+------+--------------+-----------------------------------------------------------------------------------------------------------------+--------------+
Note: For table entries with two numbers listed, the numbers in parentheses indicate the number of resources of the given type used by the specific entity alone. The numbers listed outside of parentheses indicate the total resources of the given type used by the specific entity and all of its sub-entities in the hierarchy.


+--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Analysis & Synthesis RAM Summary                                                                                                                                                                             ;
+-------------------------------------------------------------------------------------------------------------+------+-------------+--------------+--------------+--------------+--------------+------+--------+
; Name                                                                                                        ; Type ; Mode        ; Port A Depth ; Port A Width ; Port B Depth ; Port B Width ; Size ; MIF    ;
+-------------------------------------------------------------------------------------------------------------+------+-------------+--------------+--------------+--------------+--------------+------+--------+
; A1_BLOCK:inst|lpm_ram_io:inst1|altram:sram|altsyncram:ram_block|altsyncram_a791:auto_generated|ALTSYNCRAM   ; AUTO ; Single Port ; 256          ; 1            ; --           ; --           ; 256  ; A1.hex ;
; A2_BLOCK:inst1|lpm_ram_io:inst17|altram:sram|altsyncram:ram_block|altsyncram_e791:auto_generated|ALTSYNCRAM ; AUTO ; Single Port ; 256          ; 4            ; --           ; --           ; 1024 ; A2.hex ;
+-------------------------------------------------------------------------------------------------------------+------+-------------+--------------+--------------+--------------+--------------+------+--------+


+--------------------------------------------------------------------------------------------------------------------------+
; Logic Cells Representing Combinational Loops                                                                             ;
+---------------------------------------------------------------------------------------------------------------------+----+
; Logic Cell Name                                                                                                     ;    ;
+---------------------------------------------------------------------------------------------------------------------+----+
; CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component|cntr_6li:auto_generated|latch_signal[15]~0 ;    ;
; CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component|cntr_6li:auto_generated|latch_signal[14]~1 ;    ;
; CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component|cntr_6li:auto_generated|latch_signal[13]~2 ;    ;
; CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component|cntr_6li:auto_generated|latch_signal[12]~3 ;    ;
; CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component|cntr_6li:auto_generated|latch_signal[11]~4 ;    ;
; CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component|cntr_6li:auto_generated|latch_signal[10]~5 ;    ;
; CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component|cntr_6li:auto_generated|latch_signal[9]~6  ;    ;
; CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component|cntr_6li:auto_generated|latch_signal[8]~7  ;    ;
; CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component|cntr_6li:auto_generated|latch_signal[7]~8  ;    ;
; CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component|cntr_6li:auto_generated|latch_signal[6]~9  ;    ;
; CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component|cntr_6li:auto_generated|latch_signal[5]~10 ;    ;
; CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component|cntr_6li:auto_generated|latch_signal[4]~11 ;    ;
; CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component|cntr_6li:auto_generated|latch_signal[3]~12 ;    ;
; CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component|cntr_6li:auto_generated|latch_signal[2]~13 ;    ;
; CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component|cntr_6li:auto_generated|latch_signal[1]~14 ;    ;
; CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component|cntr_6li:auto_generated|latch_signal[0]~15 ;    ;
; Number of logic cells representing combinational loops                                                              ; 16 ;
+---------------------------------------------------------------------------------------------------------------------+----+
Note: All cells listed above may not be present at the end of synthesis due to various synthesis optimizations.


+------------------------------------------------------+
; General Register Statistics                          ;
+----------------------------------------------+-------+
; Statistic                                    ; Value ;
+----------------------------------------------+-------+
; Total registers                              ; 108   ;
; Number of registers using Synchronous Clear  ; 0     ;
; Number of registers using Synchronous Load   ; 0     ;
; Number of registers using Asynchronous Clear ; 20    ;
; Number of registers using Asynchronous Load  ; 0     ;
; Number of registers using Clock Enable       ; 0     ;
; Number of registers using Preset             ; 0     ;
+----------------------------------------------+-------+


+-----------------------------------------------------------------------------------------------------------------------+
; Source assignments for A1_BLOCK:inst|LPM_RAM_IO:inst1|altram:sram|altsyncram:ram_block|altsyncram_a791:auto_generated ;
+---------------------------------+--------------------+------+---------------------------------------------------------+
; Assignment                      ; Value              ; From ; To                                                      ;
+---------------------------------+--------------------+------+---------------------------------------------------------+
; OPTIMIZE_POWER_DURING_SYNTHESIS ; NORMAL_COMPILATION ; -    ; -                                                       ;
+---------------------------------+--------------------+------+---------------------------------------------------------+


+------------------------------------------------------------------------------------------------+
; Source assignments for CONTROL_BLOCK:inst2|lpm_counter0:inst|lpm_counter:lpm_counter_component ;
+---------------------------+-------+------+-----------------------------------------------------+
; Assignment                ; Value ; From ; To                                                  ;
+---------------------------+-------+------+-----------------------------------------------------+
; SUPPRESS_DA_RULE_INTERNAL ; a101  ; -    ; -                                                   ;
; SUPPRESS_DA_RULE_INTERNAL ; s102  ; -    ; -                                                   ;
; SUPPRESS_DA_RULE_INTERNAL ; s103  ; -    ; -                                                   ;
+---------------------------+-------+------+-----------------------------------------------------+


+-------------------------------------------------------------------------------------------------+
; Source assignments for CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component ;
+---------------------------+-------+------+------------------------------------------------------+
; Assignment                ; Value ; From ; To                                                   ;
+---------------------------+-------+------+------------------------------------------------------+
; SUPPRESS_DA_RULE_INTERNAL ; a101  ; -    ; -                                                    ;
; SUPPRESS_DA_RULE_INTERNAL ; s102  ; -    ; -                                                    ;
; SUPPRESS_DA_RULE_INTERNAL ; s103  ; -    ; -                                                    ;
+---------------------------+-------+------+------------------------------------------------------+


+-------------------------------------------------------------------------------------------------------------------------+
; Source assignments for CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component|cntr_6li:auto_generated ;
+---------------------------+-------+------+------------------------------------------------------------------------------+
; Assignment                ; Value ; From ; To                                                                           ;
+---------------------------+-------+------+------------------------------------------------------------------------------+
; SUPPRESS_DA_RULE_INTERNAL ; a101  ; -    ; -                                                                            ;
; SUPPRESS_DA_RULE_INTERNAL ; s102  ; -    ; -                                                                            ;
; SUPPRESS_DA_RULE_INTERNAL ; s103  ; -    ; -                                                                            ;
+---------------------------+-------+------+------------------------------------------------------------------------------+


+-------------------------------------------------------------------------------------------------------------------------+
; Source assignments for A2_BLOCK:inst1|LPM_RAM_IO:inst17|altram:sram|altsyncram:ram_block|altsyncram_e791:auto_generated ;
+---------------------------------+--------------------+------+-----------------------------------------------------------+
; Assignment                      ; Value              ; From ; To                                                        ;
+---------------------------------+--------------------+------+-----------------------------------------------------------+
; OPTIMIZE_POWER_DURING_SYNTHESIS ; NORMAL_COMPILATION ; -    ; -                                                         ;
+---------------------------------+--------------------+------+-----------------------------------------------------------+


+---------------------------------------------------------------------------------------------------+
; Source assignments for SELECTOR_BLOCK:inst4|lpm_counter2:inst41|lpm_counter:lpm_counter_component ;
+---------------------------+-------+------+--------------------------------------------------------+
; Assignment                ; Value ; From ; To                                                     ;
+---------------------------+-------+------+--------------------------------------------------------+
; SUPPRESS_DA_RULE_INTERNAL ; a101  ; -    ; -                                                      ;
; SUPPRESS_DA_RULE_INTERNAL ; s102  ; -    ; -                                                      ;
; SUPPRESS_DA_RULE_INTERNAL ; s103  ; -    ; -                                                      ;
+---------------------------+-------+------+--------------------------------------------------------+


+---------------------------------------------------------------------------------------------------+
; Source assignments for SELECTOR_BLOCK:inst4|lpm_counter2:inst42|lpm_counter:lpm_counter_component ;
+---------------------------+-------+------+--------------------------------------------------------+
; Assignment                ; Value ; From ; To                                                     ;
+---------------------------+-------+------+--------------------------------------------------------+
; SUPPRESS_DA_RULE_INTERNAL ; a101  ; -    ; -                                                      ;
; SUPPRESS_DA_RULE_INTERNAL ; s102  ; -    ; -                                                      ;
; SUPPRESS_DA_RULE_INTERNAL ; s103  ; -    ; -                                                      ;
+---------------------------+-------+------+--------------------------------------------------------+


+---------------------------------------------------------------------------------------------------+
; Source assignments for SELECTOR_BLOCK:inst4|lpm_counter2:inst43|lpm_counter:lpm_counter_component ;
+---------------------------+-------+------+--------------------------------------------------------+
; Assignment                ; Value ; From ; To                                                     ;
+---------------------------+-------+------+--------------------------------------------------------+
; SUPPRESS_DA_RULE_INTERNAL ; a101  ; -    ; -                                                      ;
; SUPPRESS_DA_RULE_INTERNAL ; s102  ; -    ; -                                                      ;
; SUPPRESS_DA_RULE_INTERNAL ; s103  ; -    ; -                                                      ;
+---------------------------+-------+------+--------------------------------------------------------+


+---------------------------------------------------------------------------------------------------+
; Source assignments for SELECTOR_BLOCK:inst4|lpm_counter2:inst45|lpm_counter:lpm_counter_component ;
+---------------------------+-------+------+--------------------------------------------------------+
; Assignment                ; Value ; From ; To                                                     ;
+---------------------------+-------+------+--------------------------------------------------------+
; SUPPRESS_DA_RULE_INTERNAL ; a101  ; -    ; -                                                      ;
; SUPPRESS_DA_RULE_INTERNAL ; s102  ; -    ; -                                                      ;
; SUPPRESS_DA_RULE_INTERNAL ; s103  ; -    ; -                                                      ;
+---------------------------+-------+------+--------------------------------------------------------+


+-----------------------------------------------------------------------------+
; Parameter Settings for User Entity Instance: A1_BLOCK:inst|LPM_RAM_IO:inst1 ;
+------------------------+--------------+-------------------------------------+
; Parameter Name         ; Value        ; Type                                ;
+------------------------+--------------+-------------------------------------+
; LPM_WIDTH              ; 1            ; Untyped                             ;
; LPM_WIDTHAD            ; 8            ; Untyped                             ;
; LPM_NUMWORDS           ; 256          ; Untyped                             ;
; LPM_INDATA             ; REGISTERED   ; Untyped                             ;
; LPM_ADDRESS_CONTROL    ; REGISTERED   ; Untyped                             ;
; LPM_OUTDATA            ; UNREGISTERED ; Untyped                             ;
; LPM_FILE               ; A1.hex       ; Untyped                             ;
; USE_EAB                ; ON           ; Untyped                             ;
; DEVICE_FAMILY          ; Cyclone II   ; Untyped                             ;
; AUTO_CARRY_CHAINS      ; ON           ; AUTO_CARRY                          ;
; IGNORE_CARRY_BUFFERS   ; OFF          ; IGNORE_CARRY                        ;
; AUTO_CASCADE_CHAINS    ; ON           ; AUTO_CASCADE                        ;
; IGNORE_CASCADE_BUFFERS ; OFF          ; IGNORE_CASCADE                      ;
+------------------------+--------------+-------------------------------------+
Note: In order to hide this table in the UI and the text report file, please set the "Show Parameter Settings Tables in Synthesis Report" option in "Analysis and Synthesis Settings -> More Settings" to "Off".


+--------------------------------------------------------------------------------------------------------------------+
; Parameter Settings for User Entity Instance: CONTROL_BLOCK:inst2|lpm_decode0:inst1|lpm_decode:lpm_decode_component ;
+------------------------+------------+------------------------------------------------------------------------------+
; Parameter Name         ; Value      ; Type                                                                         ;
+------------------------+------------+------------------------------------------------------------------------------+
; LPM_WIDTH              ; 3          ; Signed Integer                                                               ;
; LPM_DECODES            ; 8          ; Signed Integer                                                               ;
; LPM_PIPELINE           ; 0          ; Untyped                                                                      ;
; CASCADE_CHAIN          ; MANUAL     ; Untyped                                                                      ;
; DEVICE_FAMILY          ; Cyclone II ; Untyped                                                                      ;
; CBXI_PARAMETER         ; decode_s6f ; Untyped                                                                      ;
; AUTO_CARRY_CHAINS      ; ON         ; AUTO_CARRY                                                                   ;
; IGNORE_CARRY_BUFFERS   ; OFF        ; IGNORE_CARRY                                                                 ;
; AUTO_CASCADE_CHAINS    ; ON         ; AUTO_CASCADE                                                                 ;
; IGNORE_CASCADE_BUFFERS ; OFF        ; IGNORE_CASCADE                                                               ;
+------------------------+------------+------------------------------------------------------------------------------+
Note: In order to hide this table in the UI and the text report file, please set the "Show Parameter Settings Tables in Synthesis Report" option in "Analysis and Synthesis Settings -> More Settings" to "Off".


+----------------------------------------------------------------------------------------------------------------------+
; Parameter Settings for User Entity Instance: CONTROL_BLOCK:inst2|lpm_counter0:inst|lpm_counter:lpm_counter_component ;
+------------------------+-------------+-------------------------------------------------------------------------------+
; Parameter Name         ; Value       ; Type                                                                          ;
+------------------------+-------------+-------------------------------------------------------------------------------+
; AUTO_CARRY_CHAINS      ; ON          ; AUTO_CARRY                                                                    ;
; IGNORE_CARRY_BUFFERS   ; OFF         ; IGNORE_CARRY                                                                  ;
; AUTO_CASCADE_CHAINS    ; ON          ; AUTO_CASCADE                                                                  ;
; IGNORE_CASCADE_BUFFERS ; OFF         ; IGNORE_CASCADE                                                                ;
; LPM_WIDTH              ; 3           ; Signed Integer                                                                ;
; LPM_DIRECTION          ; UP          ; Untyped                                                                       ;
; LPM_MODULUS            ; 0           ; Untyped                                                                       ;
; LPM_AVALUE             ; UNUSED      ; Untyped                                                                       ;
; LPM_SVALUE             ; UNUSED      ; Untyped                                                                       ;
; LPM_PORT_UPDOWN        ; PORT_UNUSED ; Untyped                                                                       ;
; DEVICE_FAMILY          ; Cyclone II  ; Untyped                                                                       ;
; CARRY_CHAIN            ; MANUAL      ; Untyped                                                                       ;
; CARRY_CHAIN_LENGTH     ; 48          ; CARRY_CHAIN_LENGTH                                                            ;
; NOT_GATE_PUSH_BACK     ; ON          ; NOT_GATE_PUSH_BACK                                                            ;
; CARRY_CNT_EN           ; SMART       ; Untyped                                                                       ;
; LABWIDE_SCLR           ; ON          ; Untyped                                                                       ;
; USE_NEW_VERSION        ; TRUE        ; Untyped                                                                       ;
; CBXI_PARAMETER         ; cntr_p2i    ; Untyped                                                                       ;
+------------------------+-------------+-------------------------------------------------------------------------------+
Note: In order to hide this table in the UI and the text report file, please set the "Show Parameter Settings Tables in Synthesis Report" option in "Analysis and Synthesis Settings -> More Settings" to "Off".


+--------------------------------------------------------------------------------------------------------------------------+
; Parameter Settings for User Entity Instance: CONTROL_BLOCK:inst2|lpm_shiftreg0:inst3|lpm_shiftreg:lpm_shiftreg_component ;
+------------------------+------------+------------------------------------------------------------------------------------+
; Parameter Name         ; Value      ; Type                                                                               ;
+------------------------+------------+------------------------------------------------------------------------------------+
; LPM_WIDTH              ; 16         ; Signed Integer                                                                     ;
; LPM_DIRECTION          ; LEFT       ; Untyped                                                                            ;
; LPM_AVALUE             ; UNUSED     ; Untyped                                                                            ;
; LPM_SVALUE             ; UNUSED     ; Untyped                                                                            ;
; DEVICE_FAMILY          ; Cyclone II ; Untyped                                                                            ;
; AUTO_CARRY_CHAINS      ; ON         ; AUTO_CARRY                                                                         ;
; IGNORE_CARRY_BUFFERS   ; OFF        ; IGNORE_CARRY                                                                       ;
; AUTO_CASCADE_CHAINS    ; ON         ; AUTO_CASCADE                                                                       ;
; IGNORE_CASCADE_BUFFERS ; OFF        ; IGNORE_CASCADE                                                                     ;
+------------------------+------------+------------------------------------------------------------------------------------+
Note: In order to hide this table in the UI and the text report file, please set the "Show Parameter Settings Tables in Synthesis Report" option in "Analysis and Synthesis Settings -> More Settings" to "Off".


+-----------------------------------------------------------------------------------------------------------------------+
; Parameter Settings for User Entity Instance: CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component ;
+------------------------+-------------+--------------------------------------------------------------------------------+
; Parameter Name         ; Value       ; Type                                                                           ;
+------------------------+-------------+--------------------------------------------------------------------------------+
; AUTO_CARRY_CHAINS      ; ON          ; AUTO_CARRY                                                                     ;
; IGNORE_CARRY_BUFFERS   ; OFF         ; IGNORE_CARRY                                                                   ;
; AUTO_CASCADE_CHAINS    ; ON          ; AUTO_CASCADE                                                                   ;
; IGNORE_CASCADE_BUFFERS ; OFF         ; IGNORE_CASCADE                                                                 ;
; LPM_WIDTH              ; 16          ; Signed Integer                                                                 ;
; LPM_DIRECTION          ; UP          ; Untyped                                                                        ;
; LPM_MODULUS            ; 0           ; Untyped                                                                        ;
; LPM_AVALUE             ; UNUSED      ; Untyped                                                                        ;
; LPM_SVALUE             ; UNUSED      ; Untyped                                                                        ;
; LPM_PORT_UPDOWN        ; PORT_UNUSED ; Untyped                                                                        ;
; DEVICE_FAMILY          ; Cyclone II  ; Untyped                                                                        ;
; CARRY_CHAIN            ; MANUAL      ; Untyped                                                                        ;
; CARRY_CHAIN_LENGTH     ; 48          ; CARRY_CHAIN_LENGTH                                                             ;
; NOT_GATE_PUSH_BACK     ; ON          ; NOT_GATE_PUSH_BACK                                                             ;
; CARRY_CNT_EN           ; SMART       ; Untyped                                                                        ;
; LABWIDE_SCLR           ; ON          ; Untyped                                                                        ;
; USE_NEW_VERSION        ; TRUE        ; Untyped                                                                        ;
; CBXI_PARAMETER         ; cntr_6li    ; Untyped                                                                        ;
+------------------------+-------------+--------------------------------------------------------------------------------+
Note: In order to hide this table in the UI and the text report file, please set the "Show Parameter Settings Tables in Synthesis Report" option in "Analysis and Synthesis Settings -> More Settings" to "Off".


+-------------------------------------------------------------------------------+
; Parameter Settings for User Entity Instance: A2_BLOCK:inst1|LPM_RAM_IO:inst17 ;
+------------------------+--------------+---------------------------------------+
; Parameter Name         ; Value        ; Type                                  ;
+------------------------+--------------+---------------------------------------+
; LPM_WIDTH              ; 4            ; Untyped                               ;
; LPM_WIDTHAD            ; 8            ; Untyped                               ;
; LPM_NUMWORDS           ; 256          ; Untyped                               ;
; LPM_INDATA             ; REGISTERED   ; Untyped                               ;
; LPM_ADDRESS_CONTROL    ; REGISTERED   ; Untyped                               ;
; LPM_OUTDATA            ; UNREGISTERED ; Untyped                               ;
; LPM_FILE               ; A2.hex       ; Untyped                               ;
; USE_EAB                ; ON           ; Untyped                               ;
; DEVICE_FAMILY          ; Cyclone II   ; Untyped                               ;
; AUTO_CARRY_CHAINS      ; ON           ; AUTO_CARRY                            ;
; IGNORE_CARRY_BUFFERS   ; OFF          ; IGNORE_CARRY                          ;
; AUTO_CASCADE_CHAINS    ; ON           ; AUTO_CASCADE                          ;
; IGNORE_CASCADE_BUFFERS ; OFF          ; IGNORE_CASCADE                        ;
+------------------------+--------------+---------------------------------------+
Note: In order to hide this table in the UI and the text report file, please set the "Show Parameter Settings Tables in Synthesis Report" option in "Analysis and Synthesis Settings -> More Settings" to "Off".


+---------------------------------------------------------------------------------+
; Parameter Settings for User Entity Instance: SELECTOR_BLOCK:inst4|BUSMUX:inst38 ;
+----------------+-------+--------------------------------------------------------+
; Parameter Name ; Value ; Type                                                   ;
+----------------+-------+--------------------------------------------------------+
; WIDTH          ; 1     ; Untyped                                                ;
+----------------+-------+--------------------------------------------------------+
Note: In order to hide this table in the UI and the text report file, please set the "Show Parameter Settings Tables in Synthesis Report" option in "Analysis and Synthesis Settings -> More Settings" to "Off".


+-------------------------------------------------------------------------------------------------------------------------+
; Parameter Settings for User Entity Instance: SELECTOR_BLOCK:inst4|lpm_compare0:inst39|lpm_compare:lpm_compare_component ;
+------------------------+------------+-----------------------------------------------------------------------------------+
; Parameter Name         ; Value      ; Type                                                                              ;
+------------------------+------------+-----------------------------------------------------------------------------------+
; lpm_width              ; 4          ; Signed Integer                                                                    ;
; LPM_REPRESENTATION     ; UNSIGNED   ; Untyped                                                                           ;
; LPM_PIPELINE           ; 0          ; Untyped                                                                           ;
; CHAIN_SIZE             ; 8          ; Untyped                                                                           ;
; ONE_INPUT_IS_CONSTANT  ; NO         ; Untyped                                                                           ;
; CARRY_CHAIN            ; MANUAL     ; Untyped                                                                           ;
; CASCADE_CHAIN          ; MANUAL     ; Untyped                                                                           ;
; CARRY_CHAIN_LENGTH     ; 48         ; CARRY_CHAIN_LENGTH                                                                ;
; CASCADE_CHAIN_LENGTH   ; 2          ; CASCADE_CHAIN_LENGTH                                                              ;
; DEVICE_FAMILY          ; Cyclone II ; Untyped                                                                           ;
; CBXI_PARAMETER         ; cmpr_bhg   ; Untyped                                                                           ;
; AUTO_CARRY_CHAINS      ; ON         ; AUTO_CARRY                                                                        ;
; IGNORE_CARRY_BUFFERS   ; OFF        ; IGNORE_CARRY                                                                      ;
; AUTO_CASCADE_CHAINS    ; ON         ; AUTO_CASCADE                                                                      ;
; IGNORE_CASCADE_BUFFERS ; OFF        ; IGNORE_CASCADE                                                                    ;
+------------------------+------------+-----------------------------------------------------------------------------------+
Note: In order to hide this table in the UI and the text report file, please set the "Show Parameter Settings Tables in Synthesis Report" option in "Analysis and Synthesis Settings -> More Settings" to "Off".


+---------------------------------------------------------------------------------------------------------------------------+
; Parameter Settings for User Entity Instance: SELECTOR_BLOCK:inst4|lpm_shiftreg0:inst3|lpm_shiftreg:lpm_shiftreg_component ;
+------------------------+------------+-------------------------------------------------------------------------------------+
; Parameter Name         ; Value      ; Type                                                                                ;
+------------------------+------------+-------------------------------------------------------------------------------------+
; LPM_WIDTH              ; 16         ; Signed Integer                                                                      ;
; LPM_DIRECTION          ; LEFT       ; Untyped                                                                             ;
; LPM_AVALUE             ; UNUSED     ; Untyped                                                                             ;
; LPM_SVALUE             ; UNUSED     ; Untyped                                                                             ;
; DEVICE_FAMILY          ; Cyclone II ; Untyped                                                                             ;
; AUTO_CARRY_CHAINS      ; ON         ; AUTO_CARRY                                                                          ;
; IGNORE_CARRY_BUFFERS   ; OFF        ; IGNORE_CARRY                                                                        ;
; AUTO_CASCADE_CHAINS    ; ON         ; AUTO_CASCADE                                                                        ;
; IGNORE_CASCADE_BUFFERS ; OFF        ; IGNORE_CASCADE                                                                      ;
+------------------------+------------+-------------------------------------------------------------------------------------+
Note: In order to hide this table in the UI and the text report file, please set the "Show Parameter Settings Tables in Synthesis Report" option in "Analysis and Synthesis Settings -> More Settings" to "Off".


+---------------------------------------------------------------------------------------------------------------------------+
; Parameter Settings for User Entity Instance: SELECTOR_BLOCK:inst4|lpm_shiftreg0:inst4|lpm_shiftreg:lpm_shiftreg_component ;
+------------------------+------------+-------------------------------------------------------------------------------------+
; Parameter Name         ; Value      ; Type                                                                                ;
+------------------------+------------+-------------------------------------------------------------------------------------+
; LPM_WIDTH              ; 16         ; Signed Integer                                                                      ;
; LPM_DIRECTION          ; LEFT       ; Untyped                                                                             ;
; LPM_AVALUE             ; UNUSED     ; Untyped                                                                             ;
; LPM_SVALUE             ; UNUSED     ; Untyped                                                                             ;
; DEVICE_FAMILY          ; Cyclone II ; Untyped                                                                             ;
; AUTO_CARRY_CHAINS      ; ON         ; AUTO_CARRY                                                                          ;
; IGNORE_CARRY_BUFFERS   ; OFF        ; IGNORE_CARRY                                                                        ;
; AUTO_CASCADE_CHAINS    ; ON         ; AUTO_CASCADE                                                                        ;
; IGNORE_CASCADE_BUFFERS ; OFF        ; IGNORE_CASCADE                                                                      ;
+------------------------+------------+-------------------------------------------------------------------------------------+
Note: In order to hide this table in the UI and the text report file, please set the "Show Parameter Settings Tables in Synthesis Report" option in "Analysis and Synthesis Settings -> More Settings" to "Off".


+-------------------------------------------------------------------------------------------------------------------------+
; Parameter Settings for User Entity Instance: SELECTOR_BLOCK:inst4|lpm_counter2:inst41|lpm_counter:lpm_counter_component ;
+------------------------+-------------+----------------------------------------------------------------------------------+
; Parameter Name         ; Value       ; Type                                                                             ;
+------------------------+-------------+----------------------------------------------------------------------------------+
; AUTO_CARRY_CHAINS      ; ON          ; AUTO_CARRY                                                                       ;
; IGNORE_CARRY_BUFFERS   ; OFF         ; IGNORE_CARRY                                                                     ;
; AUTO_CASCADE_CHAINS    ; ON          ; AUTO_CASCADE                                                                     ;
; IGNORE_CASCADE_BUFFERS ; OFF         ; IGNORE_CASCADE                                                                   ;
; LPM_WIDTH              ; 8           ; Signed Integer                                                                   ;
; LPM_DIRECTION          ; UP          ; Untyped                                                                          ;
; LPM_MODULUS            ; 0           ; Untyped                                                                          ;
; LPM_AVALUE             ; UNUSED      ; Untyped                                                                          ;
; LPM_SVALUE             ; UNUSED      ; Untyped                                                                          ;
; LPM_PORT_UPDOWN        ; PORT_UNUSED ; Untyped                                                                          ;
; DEVICE_FAMILY          ; Cyclone II  ; Untyped                                                                          ;
; CARRY_CHAIN            ; MANUAL      ; Untyped                                                                          ;
; CARRY_CHAIN_LENGTH     ; 48          ; CARRY_CHAIN_LENGTH                                                               ;
; NOT_GATE_PUSH_BACK     ; ON          ; NOT_GATE_PUSH_BACK                                                               ;
; CARRY_CNT_EN           ; SMART       ; Untyped                                                                          ;
; LABWIDE_SCLR           ; ON          ; Untyped                                                                          ;
; USE_NEW_VERSION        ; TRUE        ; Untyped                                                                          ;
; CBXI_PARAMETER         ; cntr_skh    ; Untyped                                                                          ;
+------------------------+-------------+----------------------------------------------------------------------------------+
Note: In order to hide this table in the UI and the text report file, please set the "Show Parameter Settings Tables in Synthesis Report" option in "Analysis and Synthesis Settings -> More Settings" to "Off".


+-------------------------------------------------------------------------------------------------------------------------+
; Parameter Settings for User Entity Instance: SELECTOR_BLOCK:inst4|lpm_counter2:inst42|lpm_counter:lpm_counter_component ;
+------------------------+-------------+----------------------------------------------------------------------------------+
; Parameter Name         ; Value       ; Type                                                                             ;
+------------------------+-------------+----------------------------------------------------------------------------------+
; AUTO_CARRY_CHAINS      ; ON          ; AUTO_CARRY                                                                       ;
; IGNORE_CARRY_BUFFERS   ; OFF         ; IGNORE_CARRY                                                                     ;
; AUTO_CASCADE_CHAINS    ; ON          ; AUTO_CASCADE                                                                     ;
; IGNORE_CASCADE_BUFFERS ; OFF         ; IGNORE_CASCADE                                                                   ;
; LPM_WIDTH              ; 8           ; Signed Integer                                                                   ;
; LPM_DIRECTION          ; UP          ; Untyped                                                                          ;
; LPM_MODULUS            ; 0           ; Untyped                                                                          ;
; LPM_AVALUE             ; UNUSED      ; Untyped                                                                          ;
; LPM_SVALUE             ; UNUSED      ; Untyped                                                                          ;
; LPM_PORT_UPDOWN        ; PORT_UNUSED ; Untyped                                                                          ;
; DEVICE_FAMILY          ; Cyclone II  ; Untyped                                                                          ;
; CARRY_CHAIN            ; MANUAL      ; Untyped                                                                          ;
; CARRY_CHAIN_LENGTH     ; 48          ; CARRY_CHAIN_LENGTH                                                               ;
; NOT_GATE_PUSH_BACK     ; ON          ; NOT_GATE_PUSH_BACK                                                               ;
; CARRY_CNT_EN           ; SMART       ; Untyped                                                                          ;
; LABWIDE_SCLR           ; ON          ; Untyped                                                                          ;
; USE_NEW_VERSION        ; TRUE        ; Untyped                                                                          ;
; CBXI_PARAMETER         ; cntr_skh    ; Untyped                                                                          ;
+------------------------+-------------+----------------------------------------------------------------------------------+
Note: In order to hide this table in the UI and the text report file, please set the "Show Parameter Settings Tables in Synthesis Report" option in "Analysis and Synthesis Settings -> More Settings" to "Off".


+-------------------------------------------------------------------------------------------------------------------------+
; Parameter Settings for User Entity Instance: SELECTOR_BLOCK:inst4|lpm_counter2:inst43|lpm_counter:lpm_counter_component ;
+------------------------+-------------+----------------------------------------------------------------------------------+
; Parameter Name         ; Value       ; Type                                                                             ;
+------------------------+-------------+----------------------------------------------------------------------------------+
; AUTO_CARRY_CHAINS      ; ON          ; AUTO_CARRY                                                                       ;
; IGNORE_CARRY_BUFFERS   ; OFF         ; IGNORE_CARRY                                                                     ;
; AUTO_CASCADE_CHAINS    ; ON          ; AUTO_CASCADE                                                                     ;
; IGNORE_CASCADE_BUFFERS ; OFF         ; IGNORE_CASCADE                                                                   ;
; LPM_WIDTH              ; 8           ; Signed Integer                                                                   ;
; LPM_DIRECTION          ; UP          ; Untyped                                                                          ;
; LPM_MODULUS            ; 0           ; Untyped                                                                          ;
; LPM_AVALUE             ; UNUSED      ; Untyped                                                                          ;
; LPM_SVALUE             ; UNUSED      ; Untyped                                                                          ;
; LPM_PORT_UPDOWN        ; PORT_UNUSED ; Untyped                                                                          ;
; DEVICE_FAMILY          ; Cyclone II  ; Untyped                                                                          ;
; CARRY_CHAIN            ; MANUAL      ; Untyped                                                                          ;
; CARRY_CHAIN_LENGTH     ; 48          ; CARRY_CHAIN_LENGTH                                                               ;
; NOT_GATE_PUSH_BACK     ; ON          ; NOT_GATE_PUSH_BACK                                                               ;
; CARRY_CNT_EN           ; SMART       ; Untyped                                                                          ;
; LABWIDE_SCLR           ; ON          ; Untyped                                                                          ;
; USE_NEW_VERSION        ; TRUE        ; Untyped                                                                          ;
; CBXI_PARAMETER         ; cntr_skh    ; Untyped                                                                          ;
+------------------------+-------------+----------------------------------------------------------------------------------+
Note: In order to hide this table in the UI and the text report file, please set the "Show Parameter Settings Tables in Synthesis Report" option in "Analysis and Synthesis Settings -> More Settings" to "Off".


+-------------------------------------------------------------------------------------------------------------------------+
; Parameter Settings for User Entity Instance: SELECTOR_BLOCK:inst4|lpm_counter2:inst45|lpm_counter:lpm_counter_component ;
+------------------------+-------------+----------------------------------------------------------------------------------+
; Parameter Name         ; Value       ; Type                                                                             ;
+------------------------+-------------+----------------------------------------------------------------------------------+
; AUTO_CARRY_CHAINS      ; ON          ; AUTO_CARRY                                                                       ;
; IGNORE_CARRY_BUFFERS   ; OFF         ; IGNORE_CARRY                                                                     ;
; AUTO_CASCADE_CHAINS    ; ON          ; AUTO_CASCADE                                                                     ;
; IGNORE_CASCADE_BUFFERS ; OFF         ; IGNORE_CASCADE                                                                   ;
; LPM_WIDTH              ; 8           ; Signed Integer                                                                   ;
; LPM_DIRECTION          ; UP          ; Untyped                                                                          ;
; LPM_MODULUS            ; 0           ; Untyped                                                                          ;
; LPM_AVALUE             ; UNUSED      ; Untyped                                                                          ;
; LPM_SVALUE             ; UNUSED      ; Untyped                                                                          ;
; LPM_PORT_UPDOWN        ; PORT_UNUSED ; Untyped                                                                          ;
; DEVICE_FAMILY          ; Cyclone II  ; Untyped                                                                          ;
; CARRY_CHAIN            ; MANUAL      ; Untyped                                                                          ;
; CARRY_CHAIN_LENGTH     ; 48          ; CARRY_CHAIN_LENGTH                                                               ;
; NOT_GATE_PUSH_BACK     ; ON          ; NOT_GATE_PUSH_BACK                                                               ;
; CARRY_CNT_EN           ; SMART       ; Untyped                                                                          ;
; LABWIDE_SCLR           ; ON          ; Untyped                                                                          ;
; USE_NEW_VERSION        ; TRUE        ; Untyped                                                                          ;
; CBXI_PARAMETER         ; cntr_skh    ; Untyped                                                                          ;
+------------------------+-------------+----------------------------------------------------------------------------------+
Note: In order to hide this table in the UI and the text report file, please set the "Show Parameter Settings Tables in Synthesis Report" option in "Analysis and Synthesis Settings -> More Settings" to "Off".


+-----------------------------------------------------------------------------------------------------------+
; lpm_shiftreg Parameter Settings by Entity Instance                                                        ;
+----------------------------+------------------------------------------------------------------------------+
; Name                       ; Value                                                                        ;
+----------------------------+------------------------------------------------------------------------------+
; Number of entity instances ; 3                                                                            ;
; Entity Instance            ; CONTROL_BLOCK:inst2|lpm_shiftreg0:inst3|lpm_shiftreg:lpm_shiftreg_component  ;
;     -- LPM_WIDTH           ; 16                                                                           ;
;     -- LPM_DIRECTION       ; LEFT                                                                         ;
; Entity Instance            ; SELECTOR_BLOCK:inst4|lpm_shiftreg0:inst3|lpm_shiftreg:lpm_shiftreg_component ;
;     -- LPM_WIDTH           ; 16                                                                           ;
;     -- LPM_DIRECTION       ; LEFT                                                                         ;
; Entity Instance            ; SELECTOR_BLOCK:inst4|lpm_shiftreg0:inst4|lpm_shiftreg:lpm_shiftreg_component ;
;     -- LPM_WIDTH           ; 16                                                                           ;
;     -- LPM_DIRECTION       ; LEFT                                                                         ;
+----------------------------+------------------------------------------------------------------------------+


+-------------------------------+
; Analysis & Synthesis Messages ;
+-------------------------------+
Info: *******************************************************************
Info: Running Quartus II Analysis & Synthesis
    Info: Version 9.1 Build 222 10/21/2009 SJ Web Edition
    Info: Processing started: Wed Nov 06 15:13:12 2013
Info: Command: quartus_map --read_settings_files=on --write_settings_files=off JMPER -c JMPER
Info: Found 1 design units, including 1 entities, in source file main_module.bdf
    Info: Found entity 1: MAIN_MODULE
Info: Found 1 design units, including 1 entities, in source file selector_block.bdf
    Info: Found entity 1: SELECTOR_BLOCK
Info: Found 1 design units, including 1 entities, in source file control_block.bdf
    Info: Found entity 1: CONTROL_BLOCK
Info: Found 1 design units, including 1 entities, in source file a1_block.bdf
    Info: Found entity 1: A1_BLOCK
Info: Found 1 design units, including 1 entities, in source file a2_block.bdf
    Info: Found entity 1: A2_BLOCK
Info: Found 2 design units, including 1 entities, in source file counter_block.vhd
    Info: Found design unit 1: COUNTER_BLOCK-COUNTER_MAIN
    Info: Found entity 1: COUNTER_BLOCK
Info: Found 2 design units, including 1 entities, in source file up_block.vhd
    Info: Found design unit 1: UP_BLOCK-UP_MAIN
    Info: Found entity 1: UP_BLOCK
Info: Found 2 design units, including 1 entities, in source file down_block.vhd
    Info: Found design unit 1: DOWN_BLOCK-DOWN_MAIN
    Info: Found entity 1: DOWN_BLOCK
Info: Found 2 design units, including 1 entities, in source file lpm_counter0.vhd
    Info: Found design unit 1: lpm_counter0-SYN
    Info: Found entity 1: lpm_counter0
Info: Found 2 design units, including 1 entities, in source file lpm_decode0.vhd
    Info: Found design unit 1: lpm_decode0-SYN
    Info: Found entity 1: lpm_decode0
Info: Found 2 design units, including 1 entities, in source file lpm_shiftreg0.vhd
    Info: Found design unit 1: lpm_shiftreg0-SYN
    Info: Found entity 1: lpm_shiftreg0
Info: Found 2 design units, including 1 entities, in source file lpm_counter1.vhd
    Info: Found design unit 1: lpm_counter1-SYN
    Info: Found entity 1: lpm_counter1
Info: Found 2 design units, including 1 entities, in source file lpm_compare0.vhd
    Info: Found design unit 1: lpm_compare0-SYN
    Info: Found entity 1: lpm_compare0
Info: Found 2 design units, including 1 entities, in source file lpm_ram_dq0.vhd
    Info: Found design unit 1: lpm_ram_dq0-SYN
    Info: Found entity 1: lpm_ram_dq0
Info: Found 2 design units, including 1 entities, in source file lpm_ram_dq1.vhd
    Info: Found design unit 1: lpm_ram_dq1-SYN
    Info: Found entity 1: lpm_ram_dq1
Info: Found 2 design units, including 1 entities, in source file lpm_counter2.vhd
    Info: Found design unit 1: lpm_counter2-SYN
    Info: Found entity 1: lpm_counter2
Info: Found 2 design units, including 1 entities, in source file lpm_dff0.vhd
    Info: Found design unit 1: lpm_dff0-SYN
    Info: Found entity 1: lpm_dff0
Info: Found 2 design units, including 1 entities, in source file lpm_counter3.vhd
    Info: Found design unit 1: lpm_counter3-SYN
    Info: Found entity 1: lpm_counter3
Info: Elaborating entity "MAIN_MODULE" for the top level hierarchy
Info: Elaborating entity "A1_BLOCK" for hierarchy "A1_BLOCK:inst"
Warning: Can't find a definition for parameter LPM_FILE -- assuming A1.hex was intended to be a quoted string
Warning: Undeclared parameter REGISTERED
Warning: Can't find a definition for parameter LPM_ADDRESS_CONTROL -- assuming REGISTERED was intended to be a quoted string
Warning: Undeclared parameter REGISTERED
Warning: Can't find a definition for parameter LPM_INDATA -- assuming REGISTERED was intended to be a quoted string
Warning: Undeclared parameter UNREGISTERED
Warning: Can't find a definition for parameter LPM_OUTDATA -- assuming UNREGISTERED was intended to be a quoted string
Info: Elaborating entity "LPM_RAM_IO" for hierarchy "A1_BLOCK:inst|LPM_RAM_IO:inst1"
Info: Elaborated megafunction instantiation "A1_BLOCK:inst|LPM_RAM_IO:inst1"
Info: Instantiated megafunction "A1_BLOCK:inst|LPM_RAM_IO:inst1" with the following parameter:
    Info: Parameter "LPM_ADDRESS_CONTROL" = "REGISTERED"
    Info: Parameter "LPM_FILE" = "A1.hex"
    Info: Parameter "LPM_INDATA" = "REGISTERED"
    Info: Parameter "LPM_NUMWORDS" = "256"
    Info: Parameter "LPM_OUTDATA" = "UNREGISTERED"
    Info: Parameter "LPM_WIDTH" = "1"
    Info: Parameter "LPM_WIDTHAD" = "8"
Info: Elaborating entity "altram" for hierarchy "A1_BLOCK:inst|LPM_RAM_IO:inst1|altram:sram"
Warning: Assertion warning: altram does not support Cyclone II device family -- attempting best-case memory conversions, but power-up states and read during write behavior will be different for Cyclone II devices
Info: Elaborated megafunction instantiation "A1_BLOCK:inst|LPM_RAM_IO:inst1|altram:sram", which is child of megafunction instantiation "A1_BLOCK:inst|LPM_RAM_IO:inst1"
Info: Elaborating entity "altsyncram" for hierarchy "A1_BLOCK:inst|LPM_RAM_IO:inst1|altram:sram|altsyncram:ram_block"
Info: Elaborated megafunction instantiation "A1_BLOCK:inst|LPM_RAM_IO:inst1|altram:sram|altsyncram:ram_block", which is child of megafunction instantiation "A1_BLOCK:inst|LPM_RAM_IO:inst1"
Info: Found 1 design units, including 1 entities, in source file db/altsyncram_a791.tdf
    Info: Found entity 1: altsyncram_a791
Info: Elaborating entity "altsyncram_a791" for hierarchy "A1_BLOCK:inst|LPM_RAM_IO:inst1|altram:sram|altsyncram:ram_block|altsyncram_a791:auto_generated"
Info: Elaborating entity "CONTROL_BLOCK" for hierarchy "CONTROL_BLOCK:inst2"
Info: Elaborating entity "lpm_decode0" for hierarchy "CONTROL_BLOCK:inst2|lpm_decode0:inst1"
Info: Elaborating entity "lpm_decode" for hierarchy "CONTROL_BLOCK:inst2|lpm_decode0:inst1|lpm_decode:lpm_decode_component"
Info: Elaborated megafunction instantiation "CONTROL_BLOCK:inst2|lpm_decode0:inst1|lpm_decode:lpm_decode_component"
Info: Instantiated megafunction "CONTROL_BLOCK:inst2|lpm_decode0:inst1|lpm_decode:lpm_decode_component" with the following parameter:
    Info: Parameter "lpm_decodes" = "8"
    Info: Parameter "lpm_type" = "LPM_DECODE"
    Info: Parameter "lpm_width" = "3"
Info: Found 1 design units, including 1 entities, in source file db/decode_s6f.tdf
    Info: Found entity 1: decode_s6f
Info: Elaborating entity "decode_s6f" for hierarchy "CONTROL_BLOCK:inst2|lpm_decode0:inst1|lpm_decode:lpm_decode_component|decode_s6f:auto_generated"
Info: Elaborating entity "lpm_counter0" for hierarchy "CONTROL_BLOCK:inst2|lpm_counter0:inst"
Info: Elaborating entity "lpm_counter" for hierarchy "CONTROL_BLOCK:inst2|lpm_counter0:inst|lpm_counter:lpm_counter_component"
Info: Elaborated megafunction instantiation "CONTROL_BLOCK:inst2|lpm_counter0:inst|lpm_counter:lpm_counter_component"
Info: Instantiated megafunction "CONTROL_BLOCK:inst2|lpm_counter0:inst|lpm_counter:lpm_counter_component" with the following parameter:
    Info: Parameter "lpm_direction" = "UP"
    Info: Parameter "lpm_port_updown" = "PORT_UNUSED"
    Info: Parameter "lpm_type" = "LPM_COUNTER"
    Info: Parameter "lpm_width" = "3"
Info: Found 1 design units, including 1 entities, in source file db/cntr_p2i.tdf
    Info: Found entity 1: cntr_p2i
Info: Elaborating entity "cntr_p2i" for hierarchy "CONTROL_BLOCK:inst2|lpm_counter0:inst|lpm_counter:lpm_counter_component|cntr_p2i:auto_generated"
Info: Elaborating entity "DOWN_BLOCK" for hierarchy "CONTROL_BLOCK:inst2|DOWN_BLOCK:inst5"
Info: Elaborating entity "lpm_shiftreg0" for hierarchy "CONTROL_BLOCK:inst2|lpm_shiftreg0:inst3"
Info: Elaborating entity "lpm_shiftreg" for hierarchy "CONTROL_BLOCK:inst2|lpm_shiftreg0:inst3|lpm_shiftreg:lpm_shiftreg_component"
Info: Elaborated megafunction instantiation "CONTROL_BLOCK:inst2|lpm_shiftreg0:inst3|lpm_shiftreg:lpm_shiftreg_component"
Info: Instantiated megafunction "CONTROL_BLOCK:inst2|lpm_shiftreg0:inst3|lpm_shiftreg:lpm_shiftreg_component" with the following parameter:
    Info: Parameter "lpm_direction" = "LEFT"
    Info: Parameter "lpm_type" = "LPM_SHIFTREG"
    Info: Parameter "lpm_width" = "16"
Info: Elaborating entity "lpm_counter3" for hierarchy "CONTROL_BLOCK:inst2|lpm_counter3:inst4"
Info: Elaborating entity "lpm_counter" for hierarchy "CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component"
Info: Elaborated megafunction instantiation "CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component"
Info: Instantiated megafunction "CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component" with the following parameter:
    Info: Parameter "lpm_direction" = "UP"
    Info: Parameter "lpm_port_updown" = "PORT_UNUSED"
    Info: Parameter "lpm_type" = "LPM_COUNTER"
    Info: Parameter "lpm_width" = "16"
Warning: Assertion warning: Counter will power up to an undefined state.  An asynchronous signal should be asserted before the counter reaches a known state.
Info: Found 1 design units, including 1 entities, in source file db/cntr_6li.tdf
    Info: Found entity 1: cntr_6li
Info: Elaborating entity "cntr_6li" for hierarchy "CONTROL_BLOCK:inst2|lpm_counter3:inst4|lpm_counter:lpm_counter_component|cntr_6li:auto_generated"
Info: Elaborating entity "A2_BLOCK" for hierarchy "A2_BLOCK:inst1"
Warning: Can't find a definition for parameter LPM_FILE -- assuming A2.hex was intended to be a quoted string
Warning: Undeclared parameter REGISTERED
Warning: Can't find a definition for parameter LPM_ADDRESS_CONTROL -- assuming REGISTERED was intended to be a quoted string
Warning: Undeclared parameter REGISTERED
Warning: Can't find a definition for parameter LPM_INDATA -- assuming REGISTERED was intended to be a quoted string
Warning: Undeclared parameter UNREGISTERED
Warning: Can't find a definition for parameter LPM_OUTDATA -- assuming UNREGISTERED was intended to be a quoted string
Info: Elaborating entity "LPM_RAM_IO" for hierarchy "A2_BLOCK:inst1|LPM_RAM_IO:inst17"
Info: Elaborated megafunction instantiation "A2_BLOCK:inst1|LPM_RAM_IO:inst17"
Info: Instantiated megafunction "A2_BLOCK:inst1|LPM_RAM_IO:inst17" with the following parameter:
    Info: Parameter "LPM_ADDRESS_CONTROL" = "REGISTERED"
    Info: Parameter "LPM_FILE" = "A2.hex"
    Info: Parameter "LPM_INDATA" = "REGISTERED"
    Info: Parameter "LPM_NUMWORDS" = "256"
    Info: Parameter "LPM_OUTDATA" = "UNREGISTERED"
    Info: Parameter "LPM_WIDTH" = "4"
    Info: Parameter "LPM_WIDTHAD" = "8"
Info: Elaborating entity "altram" for hierarchy "A2_BLOCK:inst1|LPM_RAM_IO:inst17|altram:sram"
Warning: Assertion warning: altram does not support Cyclone II device family -- attempting best-case memory conversions, but power-up states and read during write behavior will be different for Cyclone II devices
Info: Elaborated megafunction instantiation "A2_BLOCK:inst1|LPM_RAM_IO:inst17|altram:sram", which is child of megafunction instantiation "A2_BLOCK:inst1|LPM_RAM_IO:inst17"
Info: Elaborating entity "altsyncram" for hierarchy "A2_BLOCK:inst1|LPM_RAM_IO:inst17|altram:sram|altsyncram:ram_block"
Info: Elaborated megafunction instantiation "A2_BLOCK:inst1|LPM_RAM_IO:inst17|altram:sram|altsyncram:ram_block", which is child of megafunction instantiation "A2_BLOCK:inst1|LPM_RAM_IO:inst17"
Info: Found 1 design units, including 1 entities, in source file db/altsyncram_e791.tdf
    Info: Found entity 1: altsyncram_e791
Info: Elaborating entity "altsyncram_e791" for hierarchy "A2_BLOCK:inst1|LPM_RAM_IO:inst17|altram:sram|altsyncram:ram_block|altsyncram_e791:auto_generated"
Info: Elaborating entity "SELECTOR_BLOCK" for hierarchy "SELECTOR_BLOCK:inst4"
Info: Elaborating entity "BUSMUX" for hierarchy "SELECTOR_BLOCK:inst4|BUSMUX:inst38"
Info: Elaborated megafunction instantiation "SELECTOR_BLOCK:inst4|BUSMUX:inst38"
Info: Instantiated megafunction "SELECTOR_BLOCK:inst4|BUSMUX:inst38" with the following parameter:
    Info: Parameter "WIDTH" = "1"
Info: Elaborating entity "lpm_mux" for hierarchy "SELECTOR_BLOCK:inst4|BUSMUX:inst38|lpm_mux:$00000"
Info: Elaborated megafunction instantiation "SELECTOR_BLOCK:inst4|BUSMUX:inst38|lpm_mux:$00000", which is child of megafunction instantiation "SELECTOR_BLOCK:inst4|BUSMUX:inst38"
Info: Found 1 design units, including 1 entities, in source file db/mux_lmc.tdf
    Info: Found entity 1: mux_lmc
Info: Elaborating entity "mux_lmc" for hierarchy "SELECTOR_BLOCK:inst4|BUSMUX:inst38|lpm_mux:$00000|mux_lmc:auto_generated"
Info: Elaborating entity "lpm_compare0" for hierarchy "SELECTOR_BLOCK:inst4|lpm_compare0:inst39"
Info: Elaborating entity "lpm_compare" for hierarchy "SELECTOR_BLOCK:inst4|lpm_compare0:inst39|lpm_compare:lpm_compare_component"
Info: Elaborated megafunction instantiation "SELECTOR_BLOCK:inst4|lpm_compare0:inst39|lpm_compare:lpm_compare_component"
Info: Instantiated megafunction "SELECTOR_BLOCK:inst4|lpm_compare0:inst39|lpm_compare:lpm_compare_component" with the following parameter:
    Info: Parameter "lpm_representation" = "UNSIGNED"
    Info: Parameter "lpm_type" = "LPM_COMPARE"
    Info: Parameter "lpm_width" = "4"
Info: Found 1 design units, including 1 entities, in source file db/cmpr_bhg.tdf
    Info: Found entity 1: cmpr_bhg
Info: Elaborating entity "cmpr_bhg" for hierarchy "SELECTOR_BLOCK:inst4|lpm_compare0:inst39|lpm_compare:lpm_compare_component|cmpr_bhg:auto_generated"
Info: Elaborating entity "COUNTER_BLOCK" for hierarchy "SELECTOR_BLOCK:inst4|COUNTER_BLOCK:inst40"
Info: Elaborating entity "lpm_counter2" for hierarchy "SELECTOR_BLOCK:inst4|lpm_counter2:inst41"
Info: Elaborating entity "lpm_counter" for hierarchy "SELECTOR_BLOCK:inst4|lpm_counter2:inst41|lpm_counter:lpm_counter_component"
Info: Elaborated megafunction instantiation "SELECTOR_BLOCK:inst4|lpm_counter2:inst41|lpm_counter:lpm_counter_component"
Info: Instantiated megafunction "SELECTOR_BLOCK:inst4|lpm_counter2:inst41|lpm_counter:lpm_counter_component" with the following parameter:
    Info: Parameter "lpm_direction" = "UP"
    Info: Parameter "lpm_port_updown" = "PORT_UNUSED"
    Info: Parameter "lpm_type" = "LPM_COUNTER"
    Info: Parameter "lpm_width" = "8"
Info: Found 1 design units, including 1 entities, in source file db/cntr_skh.tdf
    Info: Found entity 1: cntr_skh
Info: Elaborating entity "cntr_skh" for hierarchy "SELECTOR_BLOCK:inst4|lpm_counter2:inst41|lpm_counter:lpm_counter_component|cntr_skh:auto_generated"
Warning: Tri-state node(s) do not directly drive top-level pin(s)
    Warning: Converted the fan-out from the tri-state buffer "A1_BLOCK:inst|inst44" to the node "SELECTOR_BLOCK:inst4|inst47" into an OR gate
    Warning: Converted the fan-out from the tri-state buffer "A2_BLOCK:inst1|inst44" to the node "SELECTOR_BLOCK:inst4|inst49" into an OR gate
Warning: Tri-state node(s) do not directly drive top-level pin(s)
    Warning: Converted the fan-out from the tri-state buffer "A2_BLOCK:inst1|inst18[3]" to the node "A2_BLOCK:inst1|inst2" into an OR gate
    Warning: Converted the fan-out from the tri-state buffer "A2_BLOCK:inst1|inst18[2]" to the node "A2_BLOCK:inst1|inst2" into an OR gate
    Warning: Converted the fan-out from the tri-state buffer "A2_BLOCK:inst1|inst18[1]" to the node "A2_BLOCK:inst1|inst2" into an OR gate
    Warning: Converted the fan-out from the tri-state buffer "A2_BLOCK:inst1|inst18[0]" to the node "A2_BLOCK:inst1|inst2" into an OR gate
    Warning: Converted the fan-out from the tri-state buffer "A1_BLOCK:inst|inst6" to the node "A1_BLOCK:inst|lpm_ram_io:inst1|altram:sram|altsyncram:ram_block|altsyncram_a791:auto_generated|q_a[0]" into an OR gate
Info: Implemented 388 device resources after synthesis - the final resource count might be different
    Info: Implemented 18 input pins
    Info: Implemented 110 output pins
    Info: Implemented 255 logic cells
    Info: Implemented 5 RAM segments
Info: Quartus II Analysis & Synthesis was successful. 0 errors, 26 warnings
    Info: Peak virtual memory: 246 megabytes
    Info: Processing ended: Wed Nov 06 15:13:20 2013
    Info: Elapsed time: 00:00:08
    Info: Total CPU time (on all processors): 00:00:07


